<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="50" unitdist="mil" unit="mm" style="lines" multiple="1" display="no" altdistance="5" altunitdist="mil" altunit="mm"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="24" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="yes" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="7" fill="1" visible="no" active="no"/>
<layer number="59" name="tCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="no" active="no"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="no" active="no"/>
<layer number="90" name="Modules" color="5" fill="1" visible="no" active="no"/>
<layer number="91" name="Nets" color="2" fill="1" visible="no" active="no"/>
<layer number="92" name="Busses" color="1" fill="1" visible="no" active="no"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="no"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="no" active="no"/>
<layer number="95" name="Names" color="7" fill="1" visible="no" active="no"/>
<layer number="96" name="Values" color="7" fill="1" visible="no" active="no"/>
<layer number="97" name="Info" color="7" fill="1" visible="no" active="no"/>
<layer number="98" name="Guide" color="6" fill="1" visible="no" active="no"/>
<layer number="99" name="SpiceOrder" color="5" fill="1" visible="no" active="no"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="yes" active="yes"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="yes" active="yes"/>
<layer number="103" name="tMap" color="7" fill="1" visible="yes" active="yes"/>
<layer number="104" name="Name" color="16" fill="1" visible="yes" active="yes"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="107" name="Crop" color="7" fill="1" visible="yes" active="yes"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="yes" active="yes"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="yes" active="yes"/>
<layer number="110" name="fp0" color="7" fill="1" visible="yes" active="yes"/>
<layer number="111" name="LPC17xx" color="7" fill="1" visible="yes" active="yes"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="113" name="IDFDebug" color="4" fill="1" visible="yes" active="yes"/>
<layer number="114" name="Badge_Outline" color="7" fill="1" visible="yes" active="yes"/>
<layer number="115" name="ReferenceISLANDS" color="7" fill="1" visible="yes" active="yes"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="129" name="Mask" color="7" fill="1" visible="yes" active="yes"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="yes" active="yes"/>
<layer number="150" name="Notes" color="7" fill="1" visible="yes" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="yes" active="yes"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="yes" active="yes"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="199" name="Contour" color="7" fill="1" visible="yes" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="yes" active="yes"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="yes" active="yes"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="yes" active="yes"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="yes" active="yes"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="yes" active="yes"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="yes" active="yes"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="yes" active="yes"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="yes" active="yes"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="yes" active="yes"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="248" name="Housing" color="7" fill="1" visible="yes" active="yes"/>
<layer number="249" name="Edge" color="7" fill="1" visible="yes" active="yes"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="yes" active="yes"/>
<layer number="255" name="routoute" color="7" fill="1" visible="yes" active="yes"/>
</layers>
<board>
<plain>
<wire x1="0" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="62" y2="43" width="0" layer="20"/>
<wire x1="62" y1="43" x2="0" y2="43" width="0" layer="20"/>
<wire x1="0" y1="43" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="40.64" drill="3"/>
<hole x="2.54" y="2.54" drill="3"/>
<hole x="59.69" y="2.54" drill="3"/>
<hole x="59.69" y="40.64" drill="3"/>
</plain>
<libraries>
<library name="Capacitor" urn="urn:adsk.eagle:library:16290819">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC3216X135" urn="urn:adsk.eagle:footprint:16290836/2" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="1.2217" x2="-1.7" y2="1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-1.2217" x2="-1.7" y2="-1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<smd name="2" x="1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<text x="0" y="1.8567" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.8567" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP7343X310N" urn="urn:adsk.eagle:footprint:16290846/1" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<wire x1="3.8" y1="2.3" x2="-4.6192" y2="2.3" width="0.12" layer="21"/>
<wire x1="-4.6192" y1="2.3" x2="-4.6192" y2="-2.3" width="0.12" layer="21"/>
<wire x1="-4.6192" y1="-2.3" x2="3.8" y2="-2.3" width="0.12" layer="21"/>
<wire x1="3.8" y1="-2.3" x2="-3.8" y2="-2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="-2.3" x2="-3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="3.8" y1="2.3" x2="3.8" y2="-2.3" width="0.12" layer="51"/>
<smd name="1" x="-3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<smd name="2" x="3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<text x="0" y="2.935" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.935" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="CAPC3216X135" urn="urn:adsk.eagle:package:16290893/2" type="model" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC3216X135"/>
</packageinstances>
</package3d>
<package3d name="CAPMP7343X310N" urn="urn:adsk.eagle:package:16290885/1" type="model" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP7343X310N"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="Diodes" urn="urn:adsk.eagle:library:11396254">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Diodes&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="DO201AD" urn="urn:adsk.eagle:footprint:10898376/1" library_version="1">
<wire x1="-4.2" y1="2.525" x2="-4.2" y2="0" width="0.127" layer="51"/>
<wire x1="-4.2" y1="0" x2="-4.2" y2="-2.525" width="0.127" layer="51"/>
<wire x1="-4.2" y1="-2.525" x2="4.2" y2="-2.525" width="0.127" layer="51"/>
<wire x1="4.2" y1="-2.525" x2="4.2" y2="0" width="0.127" layer="51"/>
<wire x1="4.2" y1="0" x2="4.2" y2="2.525" width="0.127" layer="51"/>
<wire x1="4.2" y1="2.525" x2="-4.2" y2="2.525" width="0.127" layer="51"/>
<wire x1="-4.2" y1="2.525" x2="-4.2" y2="-2.525" width="0.127" layer="21"/>
<wire x1="-4.2" y1="-2.525" x2="4.2" y2="-2.525" width="0.127" layer="21"/>
<wire x1="4.2" y1="-2.525" x2="4.2" y2="2.525" width="0.127" layer="21"/>
<wire x1="4.2" y1="2.525" x2="-4.2" y2="2.525" width="0.127" layer="21"/>
<wire x1="-6.2" y1="0" x2="-4.2" y2="0" width="0.127" layer="51"/>
<wire x1="4.2" y1="0" x2="6.2" y2="0" width="0.127" layer="51"/>
<wire x1="-5" y1="0" x2="-4.25" y2="0" width="0.127" layer="21"/>
<wire x1="4.25" y1="0" x2="5" y2="0" width="0.127" layer="21"/>
<wire x1="-7.45" y1="2.775" x2="-7.45" y2="-2.775" width="0.05" layer="39"/>
<wire x1="-7.45" y1="-2.775" x2="7.4" y2="-2.775" width="0.05" layer="39"/>
<wire x1="7.4" y1="-2.775" x2="7.4" y2="2.775" width="0.05" layer="39"/>
<wire x1="7.4" y1="2.775" x2="-7.45" y2="2.775" width="0.05" layer="39"/>
<pad name="C" x="-6.2" y="0" drill="1.25" shape="square"/>
<pad name="A" x="6.2" y="0" drill="1.25"/>
<rectangle x1="-3.5" y1="-2.525" x2="-2.25" y2="2.525" layer="21"/>
<text x="-7.75" y="3" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-7.5" y="-4.25" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DO201AD" urn="urn:adsk.eagle:package:10898389/2" type="model" library_version="1">
<packageinstances>
<packageinstance name="DO201AD"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="inductors" urn="urn:adsk.eagle:library:243">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR127" urn="urn:adsk.eagle:footprint:15034/1" library_version="4">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
<wire x1="-6.5" y1="6.5" x2="6.525" y2="6.5" width="0.2032" layer="21"/>
<wire x1="6.525" y1="6.5" x2="6.525" y2="-6.5" width="0.2032" layer="21"/>
<wire x1="6.525" y1="-6.5" x2="-6.5" y2="-6.5" width="0.2032" layer="21"/>
<wire x1="-6.5" y1="-6.5" x2="-6.5" y2="6.5" width="0.2032" layer="21"/>
<wire x1="-4.5254" y1="3.783" x2="-3.8006" y2="4.5431" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="-3.783" y1="-4.5254" x2="-4.5431" y2="-3.8006" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="4.5254" y1="-3.783" x2="3.8006" y2="-4.5431" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="3.783" y1="4.5254" x2="4.5431" y2="3.8006" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="0" y1="5.9" x2="4.9" y2="3.275" width="0.2032" layer="21" curve="-56.209779"/>
<wire x1="0" y1="5.9" x2="-4.95" y2="3.225" width="0.2032" layer="21" curve="56.95663"/>
<wire x1="0" y1="-5.9" x2="-4.9" y2="-3.275" width="0.2032" layer="21" curve="-56.209779"/>
<wire x1="0" y1="-5.9" x2="4.95" y2="-3.225" width="0.2032" layer="21" curve="56.95663"/>
<circle x="0" y="0" radius="5.9" width="0.2032" layer="51"/>
<smd name="1" x="-4.975" y="0" dx="3.85" dy="5.5" layer="1"/>
<smd name="2" x="4.975" y="0" dx="3.85" dy="5.5" layer="1"/>
<text x="-2.5" y="3" size="1.27" layer="25">&gt;NAME</text>
<text x="-3" y="-4.5" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DR127" urn="urn:adsk.eagle:package:15117/1" type="box" library_version="4">
<description>High Power Density, High Efficiency, Shielded Inductors
Source: coiltronics_dr_series.pdf</description>
<packageinstances>
<packageinstance name="DR127"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="eagle-ltspice" urn="urn:adsk.eagle:library:217">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R1206" urn="urn:adsk.eagle:footprint:13238/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="0.9525" y1="-0.8128" x2="-0.9652" y2="-0.8128" width="0.1524" layer="51"/>
<wire x1="0.9525" y1="0.8128" x2="-0.9652" y2="0.8128" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="0.983" x2="2.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="0.983" x2="2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-0.983" x2="-2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-0.983" x2="-2.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="-1.6891" y1="-0.8763" x2="-0.9525" y2="0.8763" layer="51"/>
<rectangle x1="0.9525" y1="-0.8763" x2="1.6891" y2="0.8763" layer="51"/>
<rectangle x1="-0.3" y1="-0.7" x2="0.3" y2="0.7" layer="35"/>
<smd name="1" x="-1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<smd name="2" x="1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<text x="-1.27" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.27" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1210" urn="urn:adsk.eagle:footprint:13239/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="1.219" x2="0.939" y2="1.219" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-1.219" x2="0.939" y2="-1.219" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="1.483" x2="2.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="1.483" x2="2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-1.483" x2="-2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-1.483" x2="-2.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-1.3081" x2="-0.9009" y2="1.2918" layer="51"/>
<rectangle x1="0.9144" y1="-1.3081" x2="1.6645" y2="1.2918" layer="51"/>
<rectangle x1="-0.3" y1="-0.8999" x2="0.3" y2="0.8999" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="R1206" urn="urn:adsk.eagle:package:13301/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1206"/>
</packageinstances>
</package3d>
<package3d name="R1210" urn="urn:adsk.eagle:package:13299/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1210"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="SparkFun-Connectors" urn="urn:adsk.eagle:library:513">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:footprint:37674/1" library_version="1">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="P2" x="0" y="0" drill="1.016" shape="square"/>
<pad name="P1" x="2.54" y="0" drill="1.016" shape="square"/>
<wire x1="-1.5" y1="3.25" x2="4" y2="3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="3.25" x2="4" y2="2.5" width="0.2032" layer="21"/>
<wire x1="4" y1="2.5" x2="4" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="-3.25" x2="-1.5" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="-3.25" x2="-1.5" y2="2.5" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="-1.5" y2="3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="4" y2="2.5" width="0.2032" layer="21"/>
<text x="-1.27" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-4.064" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X08_LONGPADS" urn="urn:adsk.eagle:footprint:37763/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="19.05" y1="0.635" x2="19.05" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="7" x="15.24" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="8" x="17.78" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="14.986" y1="-0.254" x2="15.494" y2="0.254" layer="51"/>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<rectangle x1="17.526" y1="-0.254" x2="18.034" y2="0.254" layer="51"/>
<text x="-1.143" y="2.159" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.016" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02" urn="urn:adsk.eagle:footprint:37654/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04" urn="urn:adsk.eagle:footprint:37702/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:package:38059/1" type="box" library_version="1">
<description>2 Pin Screw Terminal - 2.54mm
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_2.54_SCREWTERM"/>
</packageinstances>
</package3d>
<package3d name="1X08_LONGPADS" urn="urn:adsk.eagle:package:38142/1" type="box" library_version="1">
<description>Plated Through Hole -8 Pin Long Pads
Specifications:
Pin count:8
Pin pitch:0.1"

Example device(s):
CONN_08
</description>
<packageinstances>
<packageinstance name="1X08_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X02" urn="urn:adsk.eagle:package:38039/1" type="box" library_version="1">
<description>Plated Through Hole
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02"/>
</packageinstances>
</package3d>
<package3d name="1X04" urn="urn:adsk.eagle:package:38085/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="Transistor" urn="urn:adsk.eagle:library:16378713">
<description>&lt;B&gt;BJT, JFET, MOSFET, UJT, Darlington</description>
<packages>
<package name="SOT23" urn="urn:adsk.eagle:footprint:28669/1" library_version="4">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
<wire x1="1.4224" y1="0.6604" x2="1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="1.4224" y1="-0.6604" x2="-1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="-0.6604" x2="-1.4224" y2="0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="0.6604" x2="1.4224" y2="0.6604" width="0.1524" layer="51"/>
<smd name="3" x="0" y="1.1" dx="1" dy="1.4" layer="1"/>
<smd name="2" x="0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<smd name="1" x="-0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<text x="-1.905" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.2286" y1="0.7112" x2="0.2286" y2="1.2954" layer="51"/>
<rectangle x1="0.7112" y1="-1.2954" x2="1.1684" y2="-0.7112" layer="51"/>
<rectangle x1="-1.1684" y1="-1.2954" x2="-0.7112" y2="-0.7112" layer="51"/>
</package>
</packages>
<packages3d>
<package3d name="SOT23" urn="urn:adsk.eagle:package:28738/2" type="model" library_version="4">
<description>SOT-23</description>
<packageinstances>
<packageinstance name="SOT23"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="eScooter">
<packages>
<package name="DIOM5027X220N" urn="urn:adsk.eagle:footprint:21928331/1">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<wire x1="2.5" y1="1.35" x2="-3.3699" y2="1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="1.35" x2="-3.3699" y2="-1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="-1.35" x2="2.5" y2="-1.35" width="0.12" layer="21"/>
<wire x1="2.5" y1="-1.35" x2="-2.5" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="-1.35" x2="-2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="1.35" x2="2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="2.5" y1="1.35" x2="2.5" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<smd name="2" x="2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<text x="0" y="1.985" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.985" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPAE1230X1250N" urn="urn:adsk.eagle:footprint:21812987/1">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<wire x1="-6.25" y1="1.3186" x2="-6.25" y2="3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="3.6573" x2="-3.6573" y2="6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="1.3186" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-1.3186" x2="-6.25" y2="-3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-3.6573" x2="-3.6573" y2="-6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="-6.25" x2="6.25" y2="-6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="6.25" y2="-1.3186" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="-6.25" y2="-6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="-6.25" x2="-6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="-6.25" width="0.12" layer="51"/>
<smd name="1" x="-4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<smd name="2" x="4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<text x="0" y="6.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIP826W56P254L937H458Q8B" urn="urn:adsk.eagle:footprint:22059849/1">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span, 9.38 X 6.99 X 4.58 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span with body size 9.38 X 6.99 X 4.58 mm&lt;/p&gt;</description>
<circle x="-5.3669" y="3.81" radius="0.25" width="0" layer="21"/>
<wire x1="-3.935" y1="4.7969" x2="-3.935" y2="4.955" width="0.12" layer="21"/>
<wire x1="-3.935" y1="4.955" x2="3.935" y2="4.955" width="0.12" layer="21"/>
<wire x1="3.935" y1="4.955" x2="3.935" y2="4.7969" width="0.12" layer="21"/>
<wire x1="-3.935" y1="-4.7969" x2="-3.935" y2="-4.955" width="0.12" layer="21"/>
<wire x1="-3.935" y1="-4.955" x2="3.935" y2="-4.955" width="0.12" layer="21"/>
<wire x1="3.935" y1="-4.955" x2="3.935" y2="-4.7969" width="0.12" layer="21"/>
<wire x1="3.935" y1="-4.955" x2="-3.935" y2="-4.955" width="0.12" layer="51"/>
<wire x1="-3.935" y1="-4.955" x2="-3.935" y2="4.955" width="0.12" layer="51"/>
<wire x1="-3.935" y1="4.955" x2="3.935" y2="4.955" width="0.12" layer="51"/>
<wire x1="3.935" y1="4.955" x2="3.935" y2="-4.955" width="0.12" layer="51"/>
<pad name="1" x="-4.13" y="3.81" drill="0.8657" diameter="1.4657"/>
<pad name="2" x="-4.13" y="1.27" drill="0.8657" diameter="1.4657"/>
<pad name="3" x="-4.13" y="-1.27" drill="0.8657" diameter="1.4657"/>
<pad name="4" x="-4.13" y="-3.81" drill="0.8657" diameter="1.4657"/>
<pad name="5" x="4.13" y="-3.81" drill="0.8657" diameter="1.4657"/>
<pad name="6" x="4.13" y="-1.27" drill="0.8657" diameter="1.4657"/>
<pad name="7" x="4.13" y="1.27" drill="0.8657" diameter="1.4657"/>
<pad name="8" x="4.13" y="3.81" drill="0.8657" diameter="1.4657"/>
<text x="0" y="5.59" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.59" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="XT60">
<pad name="GND" x="-3.6" y="0" drill="2.6" diameter="4" shape="square"/>
<pad name="VCC" x="3.6" y="0" drill="2.6" diameter="4"/>
<text x="-2.9" y="3.5" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.1" y="-4.1" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DIOM5027X220N" urn="urn:adsk.eagle:package:21928182/1" type="model">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM5027X220N"/>
</packageinstances>
</package3d>
<package3d name="CAPAE1230X1250N" urn="urn:adsk.eagle:package:21812541/1" type="model">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE1230X1250N"/>
</packageinstances>
</package3d>
<package3d name="DIP826W56P254L937H458Q8B" urn="urn:adsk.eagle:package:22059831/1" type="model">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span, 9.38 X 6.99 X 4.58 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span with body size 9.38 X 6.99 X 4.58 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIP826W56P254L937H458Q8B"/>
</packageinstances>
</package3d>
</packages3d>
</library>
<library name="Transistor" urn="urn:adsk.eagle:library:14522416">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Transistors &lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="DPAK3" urn="urn:adsk.eagle:footprint:10893247/4" library_version="1">
<description>DPAK, 2.29 mm pitch; 3 pin, 6.095 mm L X 6.54 mm W X 2.39 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;</description>
<smd name="1" x="-2.29" y="-4.12" dx="3.08" dy="1.31" layer="1" roundness="37" rot="R270"/>
<smd name="2" x="2.29" y="-4.12" dx="3.08" dy="1.31" layer="1" roundness="37" rot="R270"/>
<smd name="3" x="0" y="2.51" dx="6.09" dy="5.63" layer="1" roundness="51"/>
<wire x1="-2.765" y1="-3.3625" x2="-1.815" y2="-3.3625" width="0.025" layer="51"/>
<wire x1="-1.815" y1="-3.3625" x2="-1.815" y2="-4.9525" width="0.025" layer="51"/>
<wire x1="-1.815" y1="-4.9525" x2="-2.765" y2="-4.9525" width="0.025" layer="51"/>
<wire x1="-2.765" y1="-4.9525" x2="-2.765" y2="-3.3625" width="0.025" layer="51"/>
<wire x1="1.815" y1="-3.3625" x2="2.765" y2="-3.3625" width="0.025" layer="51"/>
<wire x1="2.765" y1="-3.3625" x2="2.765" y2="-4.9525" width="0.025" layer="51"/>
<wire x1="2.765" y1="-4.9525" x2="1.815" y2="-4.9525" width="0.025" layer="51"/>
<wire x1="1.815" y1="-4.9525" x2="1.815" y2="-3.3625" width="0.025" layer="51"/>
<wire x1="0" y1="-0.35" x2="0" y2="0.35" width="0.05" layer="39"/>
<wire x1="-0.35" y1="0" x2="0.35" y2="0" width="0.05" layer="39"/>
<wire x1="-3.37" y1="4.093" x2="-3.37" y2="-2.128" width="0.127" layer="51"/>
<wire x1="-3.37" y1="-2.128" x2="3.37" y2="-2.128" width="0.127" layer="51"/>
<wire x1="3.37" y1="-2.128" x2="3.37" y2="4.093" width="0.127" layer="51"/>
<wire x1="3.37" y1="4.093" x2="-3.37" y2="4.093" width="0.127" layer="51"/>
<wire x1="-3.37" y1="4.093" x2="-3.37" y2="-2.128" width="0.127" layer="21"/>
<wire x1="-3.37" y1="-2.128" x2="3.37" y2="-2.128" width="0.127" layer="21"/>
<wire x1="3.37" y1="-2.128" x2="3.37" y2="4.093" width="0.127" layer="21"/>
<wire x1="-3.015" y1="4.3" x2="-3.57" y2="4.3" width="0.05" layer="39"/>
<wire x1="-3.57" y1="4.3" x2="-3.57" y2="-2.33" width="0.05" layer="39"/>
<wire x1="-3.57" y1="-2.33" x2="-3.145" y2="-2.33" width="0.05" layer="39"/>
<wire x1="-3.145" y1="-2.33" x2="-3.145" y2="-5.86" width="0.05" layer="39"/>
<wire x1="-3.145" y1="-5.86" x2="3.145" y2="-5.86" width="0.05" layer="39"/>
<wire x1="3.145" y1="-5.86" x2="3.145" y2="-2.33" width="0.05" layer="39"/>
<wire x1="3.145" y1="-2.33" x2="3.57" y2="-2.33" width="0.05" layer="39"/>
<wire x1="3.57" y1="-2.33" x2="3.57" y2="4.3" width="0.05" layer="39"/>
<wire x1="3.57" y1="4.3" x2="3.015" y2="4.3" width="0.05" layer="39"/>
<wire x1="3.015" y1="4.3" x2="3.015" y2="5.755" width="0.05" layer="39"/>
<wire x1="3.015" y1="5.755" x2="-3.015" y2="5.755" width="0.05" layer="39"/>
<wire x1="-3.015" y1="5.755" x2="-3.015" y2="4.3" width="0.05" layer="39"/>
<circle x="0" y="0" radius="0.25" width="0.05" layer="39"/>
<circle x="-2.54" y="-6.35" radius="0.1" width="0.2" layer="21"/>
<text x="-3.81" y="7.3375" size="1.2" layer="25" ratio="10">&gt;NAME</text>
<text x="-3.81" y="-8.89" size="1.2" layer="27" ratio="10">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DPAK4" urn="urn:adsk.eagle:package:10893256/5" type="model" library_version="1">
<description>DPAK, 2.29 mm pitch; 3 pin, 6.095 mm L X 6.54 mm W X 2.39 mm H body&lt;p&gt;&lt;i&gt;PCB Libraries Packages&lt;/i&gt;</description>
<packageinstances>
<packageinstance name="DPAK3"/>
</packageinstances>
</package3d>
</packages3d>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
</class>
</classes>
<designrules name="default *">
<description language="de">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
Die Standard-Design-Rules sind so gewählt, dass sie für 
die meisten Anwendungen passen. Sollte ihre Platine 
besondere Anforderungen haben, treffen Sie die erforderlichen
Einstellungen hier und speichern die Design Rules unter 
einem neuen Namen ab.</description>
<description language="en">&lt;b&gt;EAGLE Design Rules&lt;/b&gt;
&lt;p&gt;
The default Design Rules have been set to cover
a wide range of applications. Your particular design
may have different requirements, so please make the
necessary adjustments and save your customized
design rules under a new name.</description>
<param name="layerSetup" value="(1*16)"/>
<param name="mtCopper" value="0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm 0.035mm"/>
<param name="mtIsolate" value="1.5mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm 0.15mm 0.2mm"/>
<param name="mdWireWire" value="24mil"/>
<param name="mdWirePad" value="18mil"/>
<param name="mdWireVia" value="18mil"/>
<param name="mdPadPad" value="18mil"/>
<param name="mdPadVia" value="18mil"/>
<param name="mdViaVia" value="18mil"/>
<param name="mdSmdPad" value="18mil"/>
<param name="mdSmdVia" value="18mil"/>
<param name="mdSmdSmd" value="18mil"/>
<param name="mdViaViaSameLayer" value="6mil"/>
<param name="mnLayersViaInSmd" value="2"/>
<param name="mdCopperDimension" value="40mil"/>
<param name="mdDrill" value="6mil"/>
<param name="mdSmdStop" value="0mil"/>
<param name="msWidth" value="6mil"/>
<param name="msDrill" value="0.35mm"/>
<param name="msMicroVia" value="9.99mm"/>
<param name="msBlindViaRatio" value="0.5"/>
<param name="rvPadTop" value="0.25"/>
<param name="rvPadInner" value="0.25"/>
<param name="rvPadBottom" value="0.25"/>
<param name="rvViaOuter" value="0.25"/>
<param name="rvViaInner" value="0.25"/>
<param name="rvMicroViaOuter" value="0.25"/>
<param name="rvMicroViaInner" value="0.25"/>
<param name="rlMinPadTop" value="10mil"/>
<param name="rlMaxPadTop" value="20mil"/>
<param name="rlMinPadInner" value="10mil"/>
<param name="rlMaxPadInner" value="20mil"/>
<param name="rlMinPadBottom" value="10mil"/>
<param name="rlMaxPadBottom" value="20mil"/>
<param name="rlMinViaOuter" value="8mil"/>
<param name="rlMaxViaOuter" value="20mil"/>
<param name="rlMinViaInner" value="8mil"/>
<param name="rlMaxViaInner" value="20mil"/>
<param name="rlMinMicroViaOuter" value="4mil"/>
<param name="rlMaxMicroViaOuter" value="20mil"/>
<param name="rlMinMicroViaInner" value="4mil"/>
<param name="rlMaxMicroViaInner" value="20mil"/>
<param name="psTop" value="-1"/>
<param name="psBottom" value="-1"/>
<param name="psFirst" value="-1"/>
<param name="psElongationLong" value="100"/>
<param name="psElongationOffset" value="100"/>
<param name="mvStopFrame" value="1"/>
<param name="mvCreamFrame" value="0"/>
<param name="mlMinStopFrame" value="4mil"/>
<param name="mlMaxStopFrame" value="4mil"/>
<param name="mlMinCreamFrame" value="0mil"/>
<param name="mlMaxCreamFrame" value="0mil"/>
<param name="mlViaStopLimit" value="0mil"/>
<param name="srRoundness" value="0"/>
<param name="srMinRoundness" value="0mil"/>
<param name="srMaxRoundness" value="0mil"/>
<param name="slThermalIsolate" value="10mil"/>
<param name="slThermalsForVias" value="0"/>
<param name="dpMaxLengthDifference" value="10mm"/>
<param name="dpGapFactor" value="2.5"/>
<param name="checkAngle" value="0"/>
<param name="checkFont" value="1"/>
<param name="checkRestrict" value="1"/>
<param name="checkStop" value="0"/>
<param name="checkValues" value="0"/>
<param name="checkNames" value="1"/>
<param name="checkWireStubs" value="1"/>
<param name="checkPolygonWidth" value="0"/>
<param name="useDiameter" value="13"/>
<param name="maxErrors" value="50"/>
</designrules>
<autorouter>
<pass name="Default">
<param name="RoutingGrid" value="50mil"/>
<param name="AutoGrid" value="1"/>
<param name="Efforts" value="0"/>
<param name="TopRouterVariant" value="1"/>
<param name="tpViaShape" value="round"/>
<param name="PrefDir.1" value="a"/>
<param name="PrefDir.2" value="0"/>
<param name="PrefDir.3" value="0"/>
<param name="PrefDir.4" value="0"/>
<param name="PrefDir.5" value="0"/>
<param name="PrefDir.6" value="0"/>
<param name="PrefDir.7" value="0"/>
<param name="PrefDir.8" value="0"/>
<param name="PrefDir.9" value="0"/>
<param name="PrefDir.10" value="0"/>
<param name="PrefDir.11" value="0"/>
<param name="PrefDir.12" value="0"/>
<param name="PrefDir.13" value="0"/>
<param name="PrefDir.14" value="0"/>
<param name="PrefDir.15" value="0"/>
<param name="PrefDir.16" value="a"/>
<param name="cfVia" value="8"/>
<param name="cfNonPref" value="5"/>
<param name="cfChangeDir" value="2"/>
<param name="cfOrthStep" value="2"/>
<param name="cfDiagStep" value="3"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="1"/>
<param name="cfMalusStep" value="1"/>
<param name="cfPadImpact" value="4"/>
<param name="cfSmdImpact" value="4"/>
<param name="cfBusImpact" value="0"/>
<param name="cfHugging" value="3"/>
<param name="cfAvoid" value="4"/>
<param name="cfPolygon" value="10"/>
<param name="cfBase.1" value="0"/>
<param name="cfBase.2" value="1"/>
<param name="cfBase.3" value="1"/>
<param name="cfBase.4" value="1"/>
<param name="cfBase.5" value="1"/>
<param name="cfBase.6" value="1"/>
<param name="cfBase.7" value="1"/>
<param name="cfBase.8" value="1"/>
<param name="cfBase.9" value="1"/>
<param name="cfBase.10" value="1"/>
<param name="cfBase.11" value="1"/>
<param name="cfBase.12" value="1"/>
<param name="cfBase.13" value="1"/>
<param name="cfBase.14" value="1"/>
<param name="cfBase.15" value="1"/>
<param name="cfBase.16" value="0"/>
<param name="mnVias" value="20"/>
<param name="mnSegments" value="9999"/>
<param name="mnExtdSteps" value="9999"/>
<param name="mnRipupLevel" value="10"/>
<param name="mnRipupSteps" value="100"/>
<param name="mnRipupTotal" value="100"/>
</pass>
<pass name="Follow-me" refer="Default" active="yes">
</pass>
<pass name="Busses" refer="Default" active="yes">
<param name="cfNonPref" value="4"/>
<param name="cfBusImpact" value="4"/>
<param name="cfHugging" value="0"/>
<param name="mnVias" value="0"/>
</pass>
<pass name="Route" refer="Default" active="yes">
</pass>
<pass name="Optimize1" refer="Default" active="yes">
<param name="cfVia" value="99"/>
<param name="cfExtdStep" value="10"/>
<param name="cfHugging" value="1"/>
<param name="mnExtdSteps" value="1"/>
<param name="mnRipupLevel" value="0"/>
</pass>
<pass name="Optimize2" refer="Optimize1" active="yes">
<param name="cfNonPref" value="0"/>
<param name="cfChangeDir" value="6"/>
<param name="cfExtdStep" value="0"/>
<param name="cfBonusStep" value="2"/>
<param name="cfMalusStep" value="2"/>
<param name="cfPadImpact" value="2"/>
<param name="cfSmdImpact" value="2"/>
<param name="cfHugging" value="0"/>
</pass>
<pass name="Optimize3" refer="Optimize2" active="yes">
<param name="cfChangeDir" value="8"/>
<param name="cfPadImpact" value="0"/>
<param name="cfSmdImpact" value="0"/>
</pass>
<pass name="Optimize4" refer="Optimize3" active="yes">
<param name="cfChangeDir" value="25"/>
</pass>
</autorouter>
<elements>
<element name="C1" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" package="CAPC3216X135" package3d_urn="urn:adsk.eagle:package:16290893/2" value="0.1uF" x="29.21" y="13.97" smashed="yes" rot="R270">
<attribute name="CATEGORY" value="Capacitor" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MPN" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="NAME" x="29.21" y="10.7467" size="1.27" layer="25" align="bottom-center"/>
<attribute name="OPERATING_TEMP" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="PART_STATUS" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SERIES" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SUB-CATEGORY" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="THERMALLOSS" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="TYPE" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="VALUE" x="29.21" y="14.6533" size="1.27" layer="27" align="top-center"/>
<attribute name="VOLTAGE_RATING" value="" x="-15.24" y="-6.35" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="C2" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" package="CAPC3216X135" package3d_urn="urn:adsk.eagle:package:16290893/2" value="0.1uF" x="34.29" y="20.32" smashed="yes" rot="R180">
<attribute name="CATEGORY" value="Capacitor" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MANUFACTURER" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="MPN" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="NAME" x="38.1" y="21.0033" size="1.27" layer="25" rot="R180" align="bottom-center"/>
<attribute name="OPERATING_TEMP" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="PART_STATUS" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SERIES" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SUB-CATEGORY" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="THERMALLOSS" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="TYPE" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="34.29" y="22.1767" size="1.27" layer="27" rot="R180" align="top-center"/>
<attribute name="VOLTAGE_RATING" value="" x="8.89" y="64.77" size="1.778" layer="27" rot="R180" display="off"/>
</element>
<element name="C3" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" package="CAPMP7343X310N" package3d_urn="urn:adsk.eagle:package:16290885/1" value="15uF" x="49.53" y="6.35" smashed="yes" rot="R270">
<attribute name="CATEGORY" value="Capacitor" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MPN" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="NAME" x="45.72" y="1.665" size="1.27" layer="25" align="bottom-center"/>
<attribute name="OPERATING_TEMP" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="PART_STATUS" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SERIES" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SUB-CATEGORY" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="THERMALLOSS" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="TYPE" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="VALUE" x="49.53" y="7.225" size="1.27" layer="27" align="top-center"/>
<attribute name="VOLTAGE_RATING" value="" x="13.97" y="-26.67" size="1.778" layer="27" rot="R270" display="off"/>
</element>
<element name="D1" library="Diodes" library_urn="urn:adsk.eagle:library:11396254" package="DO201AD" package3d_urn="urn:adsk.eagle:package:10898389/2" value="SB5100" x="24.13" y="8.89" smashed="yes" rot="R270">
<attribute name="CREATED_BY" value="PCBLayout.com" x="-13.97" y="-11.43" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MBR360GOS-ND" x="-13.97" y="-11.43" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MANUFACTURER" value="ON Semiconductor" x="-13.97" y="-11.43" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="MPN" value="MBR360G" x="-13.97" y="-11.43" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="NAME" x="27.81" y="3" size="1.27" layer="25" ratio="10"/>
<attribute name="PACKAGE" value="DO-201AD" x="-13.97" y="-11.43" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="VALUE" x="19.88" y="16.39" size="1.27" layer="27" ratio="10" rot="R270"/>
</element>
<element name="L1" library="inductors" library_urn="urn:adsk.eagle:library:243" package="DR127" package3d_urn="urn:adsk.eagle:package:15117/1" value="DR127" x="39.37" y="11.43" smashed="yes">
<attribute name="NAME" x="39.33" y="4.62" size="1.27" layer="25" rot="R180"/>
<attribute name="POPULARITY" value="2" x="74.93" y="-13.97" size="1.778" layer="27" display="off"/>
<attribute name="SPICEPREFIX" value="L" x="74.93" y="-13.97" size="1.778" layer="27" display="off"/>
<attribute name="VALUE" x="36.37" y="6.93" size="1.27" layer="27"/>
</element>
<element name="R1" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="1M" x="17.78" y="24.13" smashed="yes">
<attribute name="NAME" x="15.24" y="24.13" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="33.02" y="-22.86" size="1.778" layer="27" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="33.02" y="-22.86" size="1.778" layer="27" display="off"/>
<attribute name="VALUE" x="16.51" y="24.13" size="1.27" layer="27"/>
</element>
<element name="R2" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="100K" x="17.78" y="26.67" smashed="yes" rot="R180">
<attribute name="NAME" x="15.24" y="26.67" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="-24.13" y="62.23" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="-24.13" y="62.23" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="16.51" y="26.67" size="1.27" layer="27"/>
</element>
<element name="R3" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="39K" x="17.78" y="29.21" smashed="yes" rot="R180">
<attribute name="NAME" x="15.24" y="29.21" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="-12.7" y="73.66" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="-12.7" y="73.66" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="16.51" y="29.21" size="1.27" layer="27"/>
</element>
<element name="J3" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" package="1X02_2.54_SCREWTERM" package3d_urn="urn:adsk.eagle:package:38059/1" value="ON/OFF" x="29.21" y="30.48" smashed="yes" rot="R180">
<attribute name="NAME" x="30.48" y="27.051" size="0.6096" layer="25" font="vector" ratio="20" rot="R180"/>
<attribute name="VALUE" x="30.48" y="34.544" size="0.6096" layer="27" font="vector" ratio="20" rot="R180"/>
</element>
<element name="Q1" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" package="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFETSOT23" x="49.53" y="34.29" smashed="yes">
<attribute name="CATEGORY" value="Transistor" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="DESCRIPTION" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="DRAIN_CURRENT" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="MPN" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="NAME" x="47.625" y="36.195" size="1.27" layer="25"/>
<attribute name="OPERATING_TEMP" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="PART_STATUS" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="SERIES" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="SUB-CATEGORY" value="MOSFET" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="THERMALLOSS" value="" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="TYPE" value="N-Channel" x="49.53" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="VALUE" x="47.625" y="31.115" size="1.27" layer="27"/>
</element>
<element name="J1" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" package="1X08_LONGPADS" package3d_urn="urn:adsk.eagle:package:38142/1" value="COMM" x="58.42" y="6.35" smashed="yes" rot="R90">
<attribute name="NAME" x="56.261" y="7.747" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="VALUE" x="61.214" y="5.334" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="J2" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" package="1X02" package3d_urn="urn:adsk.eagle:package:38039/1" value="STOP_LIGHT" x="52.07" y="39.37" smashed="yes" rot="R180">
<attribute name="NAME" x="54.61" y="39.243" size="0.6096" layer="25" font="vector" ratio="20" rot="R180"/>
<attribute name="VALUE" x="53.34" y="41.402" size="0.6096" layer="27" font="vector" ratio="20" rot="R180"/>
</element>
<element name="J5" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" package="1X04" package3d_urn="urn:adsk.eagle:package:38085/1" value="DRIVER" x="58.42" y="29.21" smashed="yes" rot="R90">
<attribute name="NAME" x="60.833" y="27.94" size="0.6096" layer="25" font="vector" ratio="20" rot="R90"/>
<attribute name="PROD_ID" value="CONN-09696" x="58.42" y="29.21" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="VALUE" x="60.452" y="27.94" size="0.6096" layer="27" font="vector" ratio="20" rot="R90"/>
</element>
<element name="R4" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1210" package3d_urn="urn:adsk.eagle:package:13299/1" value="1M" x="30.48" y="38.1" smashed="yes" rot="MR0">
<attribute name="NAME" x="27.94" y="37.465" size="1.27" layer="26" rot="MR0"/>
<attribute name="SPICEMODEL" value="NONE" x="30.48" y="38.1" size="1.778" layer="28" rot="MR0" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="30.48" y="38.1" size="1.778" layer="28" rot="MR0" display="off"/>
<attribute name="VALUE" x="31.75" y="37.465" size="1.27" layer="28" rot="MR0"/>
</element>
<element name="R5" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1210" package3d_urn="urn:adsk.eagle:package:13299/1" value="133K" x="30.48" y="34.29" smashed="yes" rot="MR180">
<attribute name="NAME" x="27.94" y="33.655" size="1.27" layer="26" rot="MR0"/>
<attribute name="SPICEMODEL" value="NONE" x="30.48" y="34.29" size="1.778" layer="28" rot="MR180" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="30.48" y="34.29" size="1.778" layer="28" rot="MR180" display="off"/>
<attribute name="VALUE" x="33.02" y="33.655" size="1.27" layer="28" rot="MR0"/>
</element>
<element name="Q2" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" package="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFETSOT23" x="22.86" y="39.37" smashed="yes" rot="MR270">
<attribute name="CATEGORY" value="Transistor" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="DESCRIPTION" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="DRAIN_CURRENT" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="MANUFACTURER" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="MPN" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="NAME" x="23.495" y="36.195" size="1.27" layer="26" rot="MR0"/>
<attribute name="OPERATING_TEMP" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="PART_STATUS" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="SERIES" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="SUB-CATEGORY" value="MOSFET" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="THERMALLOSS" value="" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="TYPE" value="N-Channel" x="22.86" y="39.37" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="VALUE" x="26.035" y="41.275" size="1.27" layer="28" rot="MR270"/>
</element>
<element name="Q3" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" package="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFETSOT23" x="53.34" y="34.29" smashed="yes">
<attribute name="CATEGORY" value="Transistor" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="DESCRIPTION" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="DRAIN_CURRENT" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="MANUFACTURER" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="MPN" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="NAME" x="51.435" y="36.195" size="1.27" layer="25"/>
<attribute name="OPERATING_TEMP" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="PART_STATUS" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="ROHS_COMPLIANT" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="SERIES" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="SUB-CATEGORY" value="MOSFET" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="THERMALLOSS" value="" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="TYPE" value="N-Channel" x="53.34" y="34.29" size="1.778" layer="27" display="off"/>
<attribute name="VALUE" x="51.435" y="31.115" size="1.27" layer="27"/>
</element>
<element name="R6" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K" x="48.26" y="24.13" smashed="yes" rot="R180">
<attribute name="NAME" x="45.72" y="25.4" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="48.26" y="24.13" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="48.26" y="24.13" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="49.53" y="24.13" size="1.27" layer="27" rot="R180"/>
</element>
<element name="R7" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K" x="52.07" y="20.32" smashed="yes">
<attribute name="NAME" x="49.53" y="21.59" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="52.07" y="20.32" size="1.778" layer="27" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="52.07" y="20.32" size="1.778" layer="27" display="off"/>
<attribute name="VALUE" x="50.8" y="17.78" size="1.27" layer="27"/>
</element>
<element name="D2" library="eScooter" package="DIOM5027X220N" package3d_urn="urn:adsk.eagle:package:21928182/1" value="P4SMAJ12CA" x="53.34" y="6.35" smashed="yes" rot="R270">
<attribute name="NAME" x="53.34" y="3.095" size="1.27" layer="25" rot="R180" align="bottom-center"/>
<attribute name="VALUE" x="51.355" y="6.35" size="1.27" layer="27" rot="R270" align="top-center"/>
</element>
<element name="R8" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K" x="52.07" y="17.78" smashed="yes" rot="R180">
<attribute name="NAME" x="49.53" y="19.05" size="1.27" layer="25" rot="R180"/>
<attribute name="SPICEMODEL" value="NONE" x="52.07" y="17.78" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="52.07" y="17.78" size="1.778" layer="27" rot="R180" display="off"/>
<attribute name="VALUE" x="53.34" y="21.59" size="1.27" layer="27" rot="R180"/>
</element>
<element name="C4" library="eScooter" package="CAPAE1230X1250N" package3d_urn="urn:adsk.eagle:package:21812541/1" value="68uF" x="13.97" y="11.43" smashed="yes" rot="R270">
<attribute name="NAME" x="13.97" y="4.545" size="1.27" layer="25" rot="R180" align="bottom-center"/>
<attribute name="VALUE" x="13.97" y="10.695" size="1.27" layer="27" rot="R180" align="top-center"/>
</element>
<element name="U$1" library="eScooter" package="DIP826W56P254L937H458Q8B" package3d_urn="urn:adsk.eagle:package:22059831/1" value="MAX5035PDIP8" x="26.67" y="21.59" smashed="yes" rot="R180">
<attribute name="NAME" x="26.67" y="28.7" size="1.27" layer="25" rot="R180" align="bottom-center"/>
<attribute name="VALUE" x="26.67" y="20.83" size="1.27" layer="27" rot="R180" align="top-center"/>
</element>
<element name="J4" library="eScooter" package="XT60" value="BATTERY" x="3.81" y="11.43" smashed="yes" rot="R90">
<attribute name="NAME" x="7.31" y="11.79" size="1.27" layer="25" rot="R270"/>
<attribute name="VALUE" x="1.56" y="8.33" size="1.27" layer="27" rot="R90"/>
</element>
<element name="J6" library="eScooter" package="XT60" value="DRIVER POWER" x="3.81" y="31.75" smashed="yes" rot="R270">
<attribute name="NAME" x="7.31" y="32.11" size="1.27" layer="25" rot="R270"/>
<attribute name="VALUE" x="1.56" y="24.84" size="1.27" layer="27" rot="R90"/>
</element>
<element name="Q4" library="Transistor" library_urn="urn:adsk.eagle:library:14522416" package="DPAK3" package3d_urn="urn:adsk.eagle:package:10893256/5" value="IRFR3607PBF" x="12.7" y="38.1" smashed="yes" rot="MR270">
<attribute name="CREATED_BY" value="PCBLayout.com" x="12.7" y="38.1" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="DIGIKEY_PART_NUMBER" value="FQD13N06LTMCT-ND" x="12.7" y="38.1" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="MANUFACTURER" value="ON Semiconductor" x="12.7" y="38.1" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="MPN" value="FQD13N06LTM" x="12.7" y="38.1" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="NAME" x="5.3625" y="41.91" size="1.2" layer="26" ratio="10" rot="MR270"/>
<attribute name="PACKAGE" value="DPAK-4" x="12.7" y="38.1" size="1.778" layer="28" rot="MR270" display="off"/>
<attribute name="VALUE" x="21.59" y="41.91" size="1.2" layer="28" ratio="10" rot="MR270"/>
</element>
<element name="R9" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="47K" x="38.1" y="26.67" smashed="yes" rot="R90">
<attribute name="NAME" x="38.1" y="29.21" size="1.27" layer="25" rot="R90"/>
<attribute name="SPICEMODEL" value="NONE" x="38.1" y="26.67" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="38.1" y="26.67" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="VALUE" x="39.37" y="25.4" size="1.27" layer="27" rot="R90"/>
</element>
<element name="R10" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="47K" x="35.56" y="26.67" smashed="yes" rot="R270">
<attribute name="NAME" x="35.56" y="29.21" size="1.27" layer="25" rot="R90"/>
<attribute name="SPICEMODEL" value="NONE" x="35.56" y="26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="35.56" y="26.67" size="1.778" layer="27" rot="R270" display="off"/>
<attribute name="VALUE" x="34.29" y="27.94" size="1.27" layer="27" rot="R270"/>
</element>
<element name="R11" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" package="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K" x="33.02" y="26.67" smashed="yes" rot="R90">
<attribute name="NAME" x="33.02" y="29.21" size="1.27" layer="25" rot="R90"/>
<attribute name="SPICEMODEL" value="NONE" x="33.02" y="26.67" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="SPICEPREFIX" value="R" x="33.02" y="26.67" size="1.778" layer="27" rot="R90" display="off"/>
<attribute name="VALUE" x="33.02" y="25.4" size="1.27" layer="27" rot="R90"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="J3" pad="P2"/>
<polygon width="1.27" layer="1">
<vertex x="0" y="43"/>
<vertex x="62" y="43"/>
<vertex x="62.23" y="0"/>
<vertex x="0" y="0"/>
</polygon>
<polygon width="1.27" layer="16">
<vertex x="0" y="43"/>
<vertex x="62" y="43"/>
<vertex x="62.23" y="0"/>
<vertex x="0" y="0"/>
</polygon>
<contactref element="J1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<via x="54.61" y="10.16" extent="1-16" drill="0.35"/>
<via x="53.34" y="11.43" extent="1-16" drill="0.35"/>
<via x="52.07" y="12.7" extent="1-16" drill="0.35"/>
<via x="50.8" y="13.97" extent="1-16" drill="0.35"/>
<via x="49.53" y="15.24" extent="1-16" drill="0.35"/>
<via x="48.26" y="16.51" extent="1-16" drill="0.35"/>
<via x="46.99" y="17.78" extent="1-16" drill="0.35"/>
<via x="45.72" y="19.05" extent="1-16" drill="0.35"/>
<via x="44.45" y="20.32" extent="1-16" drill="0.35"/>
<via x="44.45" y="25.4" extent="1-16" drill="0.35"/>
<via x="43.18" y="26.67" extent="1-16" drill="0.35"/>
<via x="44.45" y="22.86" extent="1-16" drill="0.35"/>
<via x="41.91" y="27.94" extent="1-16" drill="0.35"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="3"/>
<contactref element="J4" pad="GND"/>
<contactref element="Q4" pad="2"/>
<via x="40.64" y="29.21" extent="1-16" drill="0.35"/>
<via x="22.86" y="30.48" extent="1-16" drill="0.35"/>
<via x="26.67" y="16.51" extent="1-16" drill="0.35"/>
<via x="31.75" y="30.48" extent="1-16" drill="0.35"/>
<via x="34.29" y="30.48" extent="1-16" drill="0.35"/>
<via x="36.83" y="30.48" extent="1-16" drill="0.35"/>
<via x="39.37" y="30.48" extent="1-16" drill="0.35"/>
<via x="38.1" y="12.7" extent="1-16" drill="0.35"/>
<via x="41.91" y="3.81" extent="1-16" drill="0.35"/>
<via x="29.21" y="6.35" extent="1-16" drill="0.35"/>
<via x="19.05" y="12.7" extent="1-16" drill="0.35"/>
<via x="19.05" y="3.81" extent="1-16" drill="0.35"/>
<via x="10.16" y="8.89" extent="1-16" drill="0.35"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="R1" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="J4" pad="VCC"/>
<contactref element="J6" pad="VCC"/>
<wire x1="3.81" y1="28.15" x2="4.02" y2="27.94" width="2.54" layer="1"/>
<wire x1="4.02" y1="27.94" x2="6.35" y2="27.94" width="2.54" layer="1"/>
<wire x1="6.35" y1="27.94" x2="7.62" y2="26.67" width="2.54" layer="1"/>
<wire x1="3.81" y1="15.03" x2="4.02" y2="15.24" width="2.54" layer="1"/>
<wire x1="6.35" y1="15.24" x2="7.62" y2="16.51" width="2.54" layer="1"/>
<wire x1="7.62" y1="16.51" x2="7.62" y2="19.05" width="2.54" layer="1"/>
<wire x1="7.62" y1="19.05" x2="7.62" y2="26.67" width="2.54" layer="1"/>
<wire x1="4.02" y1="15.24" x2="6.35" y2="15.24" width="2.54" layer="1"/>
<wire x1="7.62" y1="16.51" x2="8.89" y2="17.78" width="2.54" layer="1"/>
<wire x1="12.7" y1="17.78" x2="8.89" y2="17.78" width="2.54" layer="1"/>
<wire x1="12.7" y1="17.78" x2="13.97" y2="17.78" width="2.54" layer="1"/>
<wire x1="13.97" y1="16.355" x2="17.935" y2="20.32" width="2.54" layer="1"/>
<wire x1="22.54" y1="20.32" x2="17.935" y2="20.32" width="2.54" layer="1"/>
<wire x1="13.97" y1="16.355" x2="12.7" y2="17.625" width="2.54" layer="1"/>
<wire x1="12.7" y1="17.625" x2="12.7" y2="17.78" width="2.54" layer="1"/>
<wire x1="8.89" y1="17.78" x2="7.62" y2="19.05" width="2.54" layer="1"/>
<wire x1="17.935" y1="20.32" x2="16.358" y2="21.897" width="1.27" layer="1"/>
<wire x1="16.358" y1="21.897" x2="16.358" y2="24.13" width="1.27" layer="1"/>
<via x="17.78" y="31.75" extent="1-16" drill="0.35"/>
<wire x1="7.62" y1="26.67" x2="8.255" y2="27.305" width="1.27" layer="1"/>
<wire x1="20.32" y1="34.29" x2="17.78" y2="31.75" width="0.8128" layer="16"/>
<wire x1="20.32" y1="34.29" x2="20.32" y2="38.1" width="0.8128" layer="16"/>
<wire x1="20.32" y1="38.1" x2="21.59" y2="39.37" width="0.8128" layer="16"/>
<wire x1="21.59" y1="39.37" x2="21.76" y2="39.37" width="0.8128" layer="16"/>
<wire x1="8.255" y1="27.305" x2="12.7" y2="31.75" width="0.8128" layer="1"/>
<wire x1="12.7" y1="31.75" x2="17.78" y2="31.75" width="0.8128" layer="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="1"/>
<wire x1="30.8" y1="17.78" x2="30.48" y2="17.78" width="1.27" layer="1"/>
<wire x1="30.48" y1="17.78" x2="29.21" y2="16.51" width="1.27" layer="1"/>
<wire x1="29.21" y1="16.51" x2="29.21" y2="15.4454" width="1.27" layer="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="L1" pad="1"/>
<contactref element="U$1" pad="8"/>
<wire x1="24.13" y1="15.09" x2="22.54" y2="16.68" width="1.27" layer="1"/>
<wire x1="22.54" y1="16.68" x2="22.54" y2="17.78" width="1.27" layer="1"/>
<wire x1="27.79" y1="11.43" x2="24.13" y2="15.09" width="1.27" layer="1"/>
<wire x1="34.395" y1="11.43" x2="28.1454" y2="11.43" width="1.27" layer="1"/>
<wire x1="29.21" y1="12.4946" x2="28.1454" y2="11.43" width="1.27" layer="1"/>
<wire x1="28.1454" y1="11.43" x2="27.79" y2="11.43" width="1.27" layer="1"/>
</signal>
<signal name="12V">
<contactref element="L1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D2" pad="1"/>
<wire x1="43.18" y1="11.43" x2="44.345" y2="11.43" width="1.27" layer="1"/>
<wire x1="53.0912" y1="8.45" x2="52.07" y2="9.4712" width="1.27" layer="1"/>
<wire x1="49.53" y1="9.4712" x2="52.07" y2="9.4712" width="1.27" layer="1"/>
<wire x1="53.0912" y1="8.45" x2="53.34" y2="8.45" width="1.27" layer="1"/>
<wire x1="53.34" y1="8.45" x2="55.44" y2="6.35" width="1.27" layer="1"/>
<wire x1="55.44" y1="6.35" x2="58.42" y2="6.35" width="1.27" layer="1"/>
<wire x1="59.69" y1="6.35" x2="58.42" y2="6.35" width="1.27" layer="1"/>
<wire x1="46.3038" y1="9.4712" x2="44.345" y2="11.43" width="1.27" layer="1"/>
<wire x1="46.3038" y1="9.4712" x2="49.53" y2="9.4712" width="1.27" layer="1"/>
<contactref element="R9" pad="1"/>
<wire x1="38.1" y1="25.248" x2="38.1" y2="23.978" width="0.8128" layer="1"/>
<wire x1="44.345" y1="17.733" x2="38.1" y2="23.978" width="0.8128" layer="1"/>
<wire x1="44.345" y1="17.733" x2="44.345" y2="11.43" width="0.8128" layer="1"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="2"/>
<wire x1="30.8" y1="20.32" x2="32.8146" y2="20.32" width="1.27" layer="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="P1"/>
<contactref element="U$1" pad="5"/>
<wire x1="19.202" y1="24.13" x2="19.202" y2="25.4" width="1.27" layer="1"/>
<wire x1="19.202" y1="25.4" x2="19.202" y2="26.67" width="1.27" layer="1"/>
<wire x1="19.202" y1="25.4" x2="22.54" y2="25.4" width="1.27" layer="1"/>
<wire x1="22.54" y1="25.4" x2="24.13" y2="25.4" width="1.27" layer="1"/>
<wire x1="24.13" y1="25.4" x2="26.67" y2="27.94" width="1.27" layer="1"/>
<wire x1="26.67" y1="27.94" x2="26.67" y2="30.48" width="1.27" layer="1"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<wire x1="16.358" y1="26.67" x2="16.358" y2="29.21" width="1.27" layer="1"/>
</signal>
<signal name="SPIN">
<contactref element="J5" pad="1"/>
<contactref element="J1" pad="8"/>
<wire x1="58.42" y1="29.21" x2="57.15" y2="29.21" width="0.8128" layer="16"/>
<wire x1="57.15" y1="29.21" x2="55.88" y2="27.94" width="0.8128" layer="16"/>
<wire x1="55.88" y1="27.94" x2="55.88" y2="25.4" width="0.8128" layer="16"/>
<wire x1="57.15" y1="24.13" x2="55.88" y2="25.4" width="0.8128" layer="16"/>
<wire x1="57.15" y1="24.13" x2="58.42" y2="24.13" width="0.8128" layer="16"/>
</signal>
<signal name="SPOUT">
<contactref element="J5" pad="2"/>
<contactref element="J1" pad="7"/>
<wire x1="58.42" y1="31.75" x2="57.15" y2="31.75" width="0.8128" layer="16"/>
<wire x1="57.15" y1="31.75" x2="54.4576" y2="29.0576" width="0.8128" layer="16"/>
<wire x1="54.4576" y1="29.0576" x2="54.4576" y2="24.2824" width="0.8128" layer="16"/>
<wire x1="57.15" y1="21.59" x2="58.42" y2="21.59" width="0.8128" layer="16"/>
<wire x1="54.4576" y1="24.2824" x2="57.15" y2="21.59" width="0.8128" layer="16"/>
</signal>
<signal name="ST">
<contactref element="J5" pad="3"/>
<contactref element="Q3" pad="2"/>
<wire x1="54.29" y1="33.19" x2="56.05" y2="33.19" width="0.8128" layer="1"/>
<wire x1="56.05" y1="33.19" x2="57.15" y2="34.29" width="0.8128" layer="1"/>
<wire x1="57.15" y1="34.29" x2="58.42" y2="34.29" width="0.8128" layer="1"/>
</signal>
<signal name="5V">
<contactref element="J5" pad="4"/>
<contactref element="J2" pad="1"/>
<wire x1="52.07" y1="39.37" x2="52.07" y2="38.1" width="0.8128" layer="16"/>
<wire x1="53.34" y1="36.83" x2="52.07" y2="38.1" width="0.8128" layer="16"/>
<wire x1="53.34" y1="36.83" x2="58.42" y2="36.83" width="0.8128" layer="16"/>
<contactref element="Q3" pad="3"/>
<wire x1="53.34" y1="35.39" x2="53.34" y2="36.83" width="0.8128" layer="1"/>
<wire x1="53.34" y1="36.83" x2="52.07" y2="38.1" width="0.8128" layer="1"/>
<wire x1="52.07" y1="38.1" x2="52.07" y2="39.37" width="0.8128" layer="1"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="J2" pad="2"/>
<wire x1="49.53" y1="39.37" x2="49.53" y2="35.39" width="0.8128" layer="1"/>
</signal>
<signal name="STLEDCTL">
<contactref element="Q1" pad="1"/>
<contactref element="J1" pad="5"/>
<wire x1="58.42" y1="16.51" x2="57.15" y2="16.51" width="0.8128" layer="16"/>
<wire x1="57.15" y1="16.51" x2="50.48" y2="23.18" width="0.8128" layer="16"/>
<wire x1="50.48" y1="23.18" x2="50.48" y2="26.99" width="0.8128" layer="16"/>
<via x="50.48" y="26.99" extent="1-16" drill="0.35"/>
<wire x1="48.58" y1="33.19" x2="48.58" y2="28.89" width="0.8128" layer="1"/>
<wire x1="50.48" y1="26.99" x2="48.58" y2="28.89" width="0.8128" layer="1"/>
<contactref element="R6" pad="1"/>
<wire x1="50.48" y1="26.99" x2="50.48" y2="24.928" width="0.8128" layer="1"/>
<wire x1="50.48" y1="24.928" x2="49.682" y2="24.13" width="0.8128" layer="1"/>
</signal>
<signal name="PWM">
<contactref element="Q2" pad="1"/>
<wire x1="48.26" y1="30.48" x2="48.26" y2="22.86" width="0.8128" layer="16"/>
<contactref element="J1" pad="4"/>
<wire x1="48.26" y1="22.86" x2="57.15" y2="13.97" width="0.8128" layer="16"/>
<wire x1="57.15" y1="13.97" x2="58.42" y2="13.97" width="0.8128" layer="16"/>
<contactref element="R8" pad="1"/>
<wire x1="58.42" y1="13.97" x2="57.15" y2="13.97" width="0.8128" layer="1"/>
<wire x1="57.15" y1="13.97" x2="53.492" y2="17.628" width="0.8128" layer="1"/>
<wire x1="53.492" y1="17.628" x2="53.492" y2="17.78" width="0.8128" layer="1"/>
<contactref element="Q4" pad="1"/>
<wire x1="23.96" y1="40.32" x2="22.7024" y2="41.5776" width="0.8128" layer="16"/>
<wire x1="16.82" y1="40.39" x2="18.0076" y2="41.5776" width="0.8128" layer="16"/>
<wire x1="22.7024" y1="41.5776" x2="18.0076" y2="41.5776" width="0.8128" layer="16"/>
<wire x1="38.42" y1="40.32" x2="48.26" y2="30.48" width="0.8128" layer="16"/>
<wire x1="23.96" y1="40.32" x2="38.42" y2="40.32" width="0.8128" layer="16"/>
</signal>
<signal name="BAT">
<contactref element="J1" pad="3"/>
<wire x1="58.42" y1="11.43" x2="57.15" y2="11.43" width="0.8128" layer="16"/>
<wire x1="57.15" y1="11.43" x2="46.8376" y2="21.7424" width="0.8128" layer="16"/>
<wire x1="46.8376" y1="29.21" x2="46.8376" y2="21.7424" width="0.8128" layer="16"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<wire x1="39.2176" y1="36.83" x2="46.8376" y2="29.21" width="0.8128" layer="16"/>
<wire x1="31.88" y1="38.1" x2="33.02" y2="38.1" width="0.8128" layer="16"/>
<wire x1="33.02" y1="38.1" x2="34.29" y2="36.83" width="0.8128" layer="16"/>
<wire x1="34.29" y1="35.56" x2="34.29" y2="36.83" width="0.8128" layer="16"/>
<wire x1="34.29" y1="35.56" x2="33.02" y2="34.29" width="0.8128" layer="16"/>
<wire x1="33.02" y1="34.29" x2="31.88" y2="34.29" width="0.8128" layer="16"/>
<wire x1="34.29" y1="36.83" x2="39.2176" y2="36.83" width="0.8128" layer="16"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="2"/>
<wire x1="23.96" y1="38.42" x2="24.28" y2="38.1" width="0.8128" layer="16"/>
<wire x1="24.28" y1="38.1" x2="29.08" y2="38.1" width="0.8128" layer="16"/>
</signal>
<signal name="STOUT">
<contactref element="J1" pad="6"/>
<contactref element="Q3" pad="1"/>
<wire x1="54.93" y1="29.38" x2="52.39" y2="31.92" width="0.8128" layer="1"/>
<wire x1="52.39" y1="31.92" x2="52.39" y2="33.19" width="0.8128" layer="1"/>
<wire x1="54.93" y1="29.38" x2="54.93" y2="21.758" width="0.8128" layer="1"/>
<wire x1="57.15" y1="19.05" x2="58.42" y2="19.05" width="0.8128" layer="1"/>
<contactref element="R7" pad="2"/>
<wire x1="53.492" y1="20.32" x2="54.93" y2="21.758" width="0.8128" layer="1"/>
<wire x1="54.93" y1="21.758" x2="54.93" y2="21.27" width="0.8128" layer="1"/>
<wire x1="54.93" y1="21.27" x2="57.15" y2="19.05" width="0.8128" layer="1"/>
</signal>
<signal name="P$1">
<contactref element="J6" pad="GND"/>
<contactref element="Q4" pad="3"/>
<wire x1="3.81" y1="35.35" x2="6.56" y2="38.1" width="2.54" layer="16"/>
<wire x1="6.56" y1="38.1" x2="8.89" y2="38.1" width="2.54" layer="16"/>
<wire x1="10.19" y1="38.1" x2="11.43" y2="38.1" width="2.54" layer="16"/>
<wire x1="10.19" y1="38.1" x2="8.89" y2="38.1" width="2.54" layer="16"/>
</signal>
<signal name="N$6">
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<wire x1="35.56" y1="28.092" x2="38.1" y2="28.092" width="0.8128" layer="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="4"/>
<contactref element="R11" pad="1"/>
<contactref element="R10" pad="2"/>
<wire x1="30.8" y1="25.4" x2="32.868" y2="25.4" width="0.8128" layer="1"/>
<wire x1="32.868" y1="25.4" x2="33.02" y2="25.248" width="0.8128" layer="1"/>
<wire x1="33.02" y1="25.248" x2="35.56" y2="25.248" width="0.8128" layer="1"/>
</signal>
</signals>
<mfgpreviewcolors>
<mfgpreviewcolor name="soldermaskcolor" color="0xC8008000"/>
<mfgpreviewcolor name="silkscreencolor" color="0xFFFEFEFE"/>
<mfgpreviewcolor name="backgroundcolor" color="0xFF282828"/>
<mfgpreviewcolor name="coppercolor" color="0xFFFFBF00"/>
<mfgpreviewcolor name="substratecolor" color="0xFF786E46"/>
</mfgpreviewcolors>
</board>
</drawing>
<compatibility>
<note version="8.2" severity="warning">
Since Version 8.2, EAGLE supports online libraries. The ids
of those online libraries will not be understood (or retained)
with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
</compatibility>
</eagle>
