<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="no" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="no" active="no"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="no" active="no"/>
<layer number="17" name="Pads" color="2" fill="1" visible="no" active="no"/>
<layer number="18" name="Vias" color="2" fill="1" visible="no" active="no"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="no" active="no"/>
<layer number="20" name="Dimension" color="24" fill="1" visible="no" active="no"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="no" active="no"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="no" active="no"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="25" name="tNames" color="7" fill="1" visible="no" active="no"/>
<layer number="26" name="bNames" color="7" fill="1" visible="no" active="no"/>
<layer number="27" name="tValues" color="7" fill="1" visible="no" active="no"/>
<layer number="28" name="bValues" color="7" fill="1" visible="no" active="no"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="no"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="no"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="no"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="no"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="no"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="no"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="no"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="no"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="no"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="no"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="no" active="no"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="no" active="no"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="no" active="no"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="no" active="no"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="no" active="no"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="no"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="no"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="no"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="no"/>
<layer number="48" name="Document" color="7" fill="1" visible="no" active="no"/>
<layer number="49" name="Reference" color="7" fill="1" visible="no" active="no"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="7" fill="1" visible="no" active="no"/>
<layer number="59" name="tCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="yes" active="yes"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="yes" active="yes"/>
<layer number="90" name="Modules" color="5" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="99" name="SpiceOrder" color="7" fill="1" visible="yes" active="yes"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="yes" active="yes"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="yes" active="yes"/>
<layer number="103" name="tMap" color="7" fill="1" visible="yes" active="yes"/>
<layer number="104" name="Name" color="16" fill="1" visible="yes" active="yes"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="107" name="Crop" color="7" fill="1" visible="yes" active="yes"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="yes" active="yes"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="yes" active="yes"/>
<layer number="110" name="fp0" color="7" fill="1" visible="yes" active="yes"/>
<layer number="111" name="LPC17xx" color="7" fill="1" visible="yes" active="yes"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="113" name="IDFDebug" color="4" fill="1" visible="yes" active="yes"/>
<layer number="114" name="Badge_Outline" color="7" fill="1" visible="yes" active="yes"/>
<layer number="115" name="ReferenceISLANDS" color="7" fill="1" visible="yes" active="yes"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="129" name="Mask" color="7" fill="1" visible="yes" active="yes"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="yes" active="yes"/>
<layer number="150" name="Notes" color="7" fill="1" visible="yes" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="yes" active="yes"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="yes" active="yes"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="199" name="Contour" color="7" fill="1" visible="yes" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="yes" active="yes"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="yes" active="yes"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="yes" active="yes"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="yes" active="yes"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="yes" active="yes"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="yes" active="yes"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="yes" active="yes"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="yes" active="yes"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="yes" active="yes"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="248" name="Housing" color="7" fill="1" visible="yes" active="yes"/>
<layer number="249" name="Edge" color="7" fill="1" visible="yes" active="yes"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="yes" active="yes"/>
<layer number="255" name="routoute" color="7" fill="1" visible="yes" active="yes"/>
</layers>
<schematic xreflabel="%F%N/%S.%C%R" xrefpart="/%S.%C%R">
<libraries>
<library name="SparkFun-Connectors" urn="urn:adsk.eagle:library:513">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02" urn="urn:adsk.eagle:footprint:37654/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2" urn="urn:adsk.eagle:footprint:37655/1" library_version="1">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2" urn="urn:adsk.eagle:footprint:37656/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="3.15" x2="5.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD" urn="urn:adsk.eagle:footprint:37657/1" library_version="1">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4" y1="-1" x2="-4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-4" y1="-4.5" x2="-3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-4.5" x2="-3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-2" x2="-2" y2="-2" width="0.2032" layer="21"/>
<wire x1="2" y1="-2" x2="3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-2" x2="3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-4.5" x2="4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="4" y1="-4.5" x2="4" y2="-1" width="0.2032" layer="21"/>
<wire x1="2" y1="3" x2="-2" y2="3" width="0.2032" layer="21"/>
<smd name="1" x="-1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="2" x="1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="NC1" x="-3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<smd name="NC2" x="3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<text x="-1.397" y="1.778" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="0.635" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_BIG" urn="urn:adsk.eagle:footprint:37658/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="-1.27" width="0.127" layer="21"/>
<wire x1="-1.27" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="1.27" x2="-1.27" y2="1.27" width="0.127" layer="21"/>
<pad name="P$1" x="0" y="0" drill="1.0668"/>
<pad name="P$2" x="3.81" y="0" drill="1.0668"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD-VERT" urn="urn:adsk.eagle:footprint:37659/1" library_version="1">
<description>&lt;h3&gt;JST-Vertical Male Header SMT &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.1" y1="2.97" x2="4.2" y2="2.97" width="0.2032" layer="51"/>
<wire x1="4.2" y1="2.97" x2="4.2" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="4.2" y1="-2.13" x2="-4.1" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="-2.13" x2="-4.1" y2="2.97" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="3" x2="4.2" y2="3" width="0.2032" layer="21"/>
<wire x1="4.2" y1="3" x2="4.2" y2="2.3" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="3" x2="-4.1" y2="2.3" width="0.2032" layer="21"/>
<wire x1="2" y1="-2.1" x2="4.2" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="4.2" y1="-2.1" x2="4.2" y2="-1.7" width="0.2032" layer="21"/>
<wire x1="-2" y1="-2.1" x2="-4.1" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="-2.1" x2="-4.1" y2="-1.8" width="0.2032" layer="21"/>
<smd name="P$1" x="-3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="P$2" x="3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="VCC" x="-1" y="-2" dx="1" dy="5.5" layer="1"/>
<smd name="GND" x="1" y="-2" dx="1" dy="5.5" layer="1"/>
<text x="-3.81" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-3.81" y="2.21" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
</package>
<package name="SCREWTERMINAL-5MM-2" urn="urn:adsk.eagle:footprint:37660/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.1" y1="4.2" x2="8.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="4.2" x2="8.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="8.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-3.3" x2="-3.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-3.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-2.3" x2="-3.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-1.35" x2="-3.7" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-1.35" x2="-3.7" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-2.35" x2="-3.1" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.1" y1="4" x2="8.7" y2="4" width="0.2032" layer="51"/>
<wire x1="8.7" y1="4" x2="8.7" y2="3" width="0.2032" layer="51"/>
<wire x1="8.7" y1="3" x2="8.1" y2="3" width="0.2032" layer="51"/>
<circle x="2.5" y="3.7" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.3" diameter="2.032" shape="square"/>
<pad name="2" x="5" y="0" drill="1.3" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LOCK" urn="urn:adsk.eagle:footprint:37661/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="-0.1778" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.7178" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2_LOCK" urn="urn:adsk.eagle:footprint:37662/1" library_version="1">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset from center by 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.667" y="0" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="1X02_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37663/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.651" y1="0" x2="0.889" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.016" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.9906" x2="-0.9906" y2="1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.9906" x2="-0.9906" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.556" y2="0" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.9906" x2="3.5306" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.9906" x2="3.5306" y2="1.27" width="0.2032" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.667" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK" urn="urn:adsk.eagle:footprint:37664/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<circle x="0" y="0" radius="0.4318" width="0.0254" layer="51"/>
<circle x="3.5" y="0" radius="0.4318" width="0.0254" layer="51"/>
<pad name="1" x="-0.1778" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.6778" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LONGPADS" urn="urn:adsk.eagle:footprint:37665/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.397" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_NO_SILK" urn="urn:adsk.eagle:footprint:37666/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH" urn="urn:adsk.eagle:footprint:37667/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="2.73" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<wire x1="-2.95" y1="-1.6" x2="-2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="6" x2="2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="6" x2="2.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="-1.6" x2="-2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="-1.6" x2="2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-1.6" x2="-2.3" y2="0" width="0.2032" layer="21"/>
<wire x1="2.3" y1="-1.6" x2="2.3" y2="0" width="0.2032" layer="21"/>
</package>
<package name="1X02_XTRA_BIG" urn="urn:adsk.eagle:footprint:37668/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-5.08" y1="2.54" x2="-5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="2.54" x2="-5.08" y2="2.54" width="0.127" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="2.0574" diameter="3.556"/>
<pad name="2" x="2.54" y="0" drill="2.0574" diameter="3.556"/>
<text x="-5.08" y="2.667" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-5.08" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_PP_HOLES_ONLY" urn="urn:adsk.eagle:footprint:37669/1" library_version="1">
<description>&lt;h3&gt;Pogo Pins Connector - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<text x="-1.27" y="1.143" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-1.778" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS" urn="urn:adsk.eagle:footprint:37670/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH-NS" urn="urn:adsk.eagle:footprint:37671/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole- No Silk&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; No silk outline of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
</package>
<package name="JST-2-PTH-KIT" urn="urn:adsk.eagle:footprint:37672/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole - KIT&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
&lt;br&gt; This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<polygon width="0.127" layer="30">
<vertex x="-0.9975" y="-0.6604" curve="-90.025935"/>
<vertex x="-1.6604" y="0" curve="-90.017354"/>
<vertex x="-1" y="0.6604" curve="-90"/>
<vertex x="-0.3396" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-1" y="-0.2865" curve="-90.08005"/>
<vertex x="-1.2865" y="0" curve="-90.040011"/>
<vertex x="-1" y="0.2865" curve="-90"/>
<vertex x="-0.7135" y="0" curve="-90"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="1.0025" y="-0.6604" curve="-90.025935"/>
<vertex x="0.3396" y="0" curve="-90.017354"/>
<vertex x="1" y="0.6604" curve="-90"/>
<vertex x="1.6604" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="1" y="-0.2865" curve="-90.08005"/>
<vertex x="0.7135" y="0" curve="-90.040011"/>
<vertex x="1" y="0.2865" curve="-90"/>
<vertex x="1.2865" y="0" curve="-90"/>
</polygon>
</package>
<package name="SPRINGTERMINAL-2.54MM-2" urn="urn:adsk.eagle:footprint:37673/1" library_version="1">
<description>&lt;h3&gt;Spring Terminal- PCB Mount 2 Pin PTH&lt;/h3&gt;
tDocu marks the spring arms
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/SpringTerminal.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.2" y1="7.88" x2="-4.2" y2="-2.8" width="0.254" layer="21"/>
<wire x1="-4.2" y1="-2.8" x2="-4.2" y2="-4.72" width="0.254" layer="51"/>
<wire x1="-4.2" y1="-4.72" x2="3.44" y2="-4.72" width="0.254" layer="51"/>
<wire x1="3.44" y1="-4.72" x2="3.44" y2="-2.8" width="0.254" layer="51"/>
<wire x1="3.44" y1="7.88" x2="-4.2" y2="7.88" width="0.254" layer="21"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="1"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="1"/>
<wire x1="-4.2" y1="-2.8" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<wire x1="3.44" y1="4" x2="3.44" y2="1" width="0.254" layer="21"/>
<wire x1="3.44" y1="7.88" x2="3.44" y2="6" width="0.254" layer="21"/>
<wire x1="3.44" y1="-0.9" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1" diameter="1.9"/>
<pad name="P$2" x="0" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="P$3" x="2.54" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="2" x="2.54" y="0" drill="1.1" diameter="1.9"/>
</package>
<package name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:footprint:37674/1" library_version="1">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="P2" x="0" y="0" drill="1.016" shape="square"/>
<pad name="P1" x="2.54" y="0" drill="1.016" shape="square"/>
<wire x1="-1.5" y1="3.25" x2="4" y2="3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="3.25" x2="4" y2="2.5" width="0.2032" layer="21"/>
<wire x1="4" y1="2.5" x2="4" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="-3.25" x2="-1.5" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="-3.25" x2="-1.5" y2="2.5" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="-1.5" y2="3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="4" y2="2.5" width="0.2032" layer="21"/>
<text x="-1.27" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-4.064" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_POKEHOME" urn="urn:adsk.eagle:footprint:37675/1" library_version="1">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
<wire x1="-7" y1="-4" x2="-7" y2="2" width="0.2032" layer="21"/>
<wire x1="-7" y1="2" x2="-7" y2="4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="4" x2="4.7" y2="-4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="-4" x2="-7" y2="-4" width="0.2032" layer="21"/>
<wire x1="-7" y1="4" x2="4.7" y2="4" width="0.2032" layer="21"/>
<smd name="P2" x="5.25" y="-2" dx="3.5" dy="2" layer="1"/>
<smd name="P1" x="5.25" y="2" dx="3.5" dy="2" layer="1"/>
<smd name="P4" x="-4" y="-2" dx="6" dy="2" layer="1"/>
<smd name="P3" x="-4" y="2" dx="6" dy="2" layer="1"/>
<text x="0.635" y="-3.175" size="0.4064" layer="25">&gt;NAME</text>
<text x="0.635" y="-1.905" size="0.4064" layer="27">&gt;VALUE</text>
</package>
<package name="1X02_RA_PTH_FEMALE" urn="urn:adsk.eagle:footprint:37676/1" library_version="1">
<wire x1="-2.79" y1="4.25" x2="-2.79" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="2.79" y1="4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="4.25" x2="2.79" y2="4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="-4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<text x="-1.397" y="0.762" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.524" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<pad name="2" x="-1.27" y="-5.85" drill="0.8"/>
<pad name="1" x="1.27" y="-5.85" drill="0.8"/>
</package>
<package name="1X06" urn="urn:adsk.eagle:footprint:37589/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="11.43" y1="0.635" x2="12.065" y2="1.27" width="0.2032" layer="21"/>
<wire x1="12.065" y1="1.27" x2="13.335" y2="1.27" width="0.2032" layer="21"/>
<wire x1="13.335" y1="1.27" x2="13.97" y2="0.635" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.635" x2="13.335" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.335" y1="-1.27" x2="12.065" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="12.065" y1="-1.27" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="9.525" y2="1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.27" x2="10.795" y2="1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.27" x2="11.43" y2="0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.635" x2="10.795" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.27" x2="9.525" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.27" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6" urn="urn:adsk.eagle:footprint:37738/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="13.97" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="13.97" y1="-2.54" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="12.7" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="12.7" y2="-1.27" width="0.127" layer="21"/>
<wire x1="12.7" y1="-1.27" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="-0.635" y2="1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796"/>
<text x="4.699" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6-RA" urn="urn:adsk.eagle:footprint:37739/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle&lt;/h3&gt;
tPlace shows angle of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="-1.27" y2="0.635" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.175" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="12.7" y1="3.175" x2="0" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="0" y2="7.62" width="0.127" layer="21"/>
<wire x1="0" y1="7.62" x2="12.7" y2="7.62" width="0.127" layer="21"/>
<wire x1="12.7" y1="7.62" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796"/>
<text x="4.953" y="5.334" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="4.445" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-SMD_RA_MALE" urn="urn:adsk.eagle:footprint:37588/1" library_version="1">
<description>&lt;h3&gt;SMD - 6 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="7.62" y1="1.25" x2="-7.62" y2="1.25" width="0.127" layer="51"/>
<wire x1="-7.62" y1="1.25" x2="-7.62" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-7.62" y1="-1.25" x2="-6.35" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-6.35" y1="-1.25" x2="-3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="6.35" y2="-1.25" width="0.127" layer="51"/>
<wire x1="6.35" y1="-1.25" x2="7.62" y2="-1.25" width="0.127" layer="51"/>
<wire x1="7.62" y1="-1.25" x2="7.62" y2="1.25" width="0.127" layer="51"/>
<wire x1="6.35" y1="-1.25" x2="6.35" y2="-7.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="-1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-6.35" y1="-1.25" x2="-6.35" y2="-7.25" width="0.127" layer="51"/>
<smd name="4" x="1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="5" x="3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="6" x="6.35" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="3" x="-1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="1" x="-6.35" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<hole x="-5.08" y="0" drill="1.4"/>
<hole x="5.08" y="0" drill="1.4"/>
<text x="-1.524" y="0.381" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.016" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LOCK" urn="urn:adsk.eagle:footprint:37592/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.508" x2="-0.635" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.143" x2="0.635" y2="1.143" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.143" x2="1.27" y2="0.508" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.508" x2="1.905" y2="1.143" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.143" x2="3.175" y2="1.143" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.143" x2="3.81" y2="0.508" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.508" x2="4.445" y2="1.143" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.143" x2="5.715" y2="1.143" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.143" x2="6.35" y2="0.508" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.508" x2="6.985" y2="1.143" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.143" x2="8.255" y2="1.143" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.143" x2="8.89" y2="0.508" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.508" x2="9.525" y2="1.143" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.143" x2="10.795" y2="1.143" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.143" x2="11.43" y2="0.508" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.508" x2="12.065" y2="1.143" width="0.2032" layer="21"/>
<wire x1="12.065" y1="1.143" x2="13.335" y2="1.143" width="0.2032" layer="21"/>
<wire x1="13.335" y1="1.143" x2="13.97" y2="0.508" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.508" x2="13.97" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.762" x2="13.335" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.335" y1="-1.397" x2="12.065" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="12.065" y1="-1.397" x2="11.43" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.762" x2="10.795" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.397" x2="9.525" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.397" x2="8.89" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.762" x2="8.255" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.397" x2="6.985" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="6.985" y1="-1.397" x2="6.35" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.762" x2="5.715" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.397" x2="4.445" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.397" x2="3.81" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.762" x2="3.175" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.397" x2="1.905" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.397" x2="1.27" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.762" x2="0.635" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.397" x2="-0.635" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="-1.397" x2="-1.27" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.762" x2="-1.27" y2="0.508" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37740/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.524" y1="-0.127" x2="1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="4.064" y1="-0.127" x2="3.556" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="6.604" y1="-0.127" x2="6.096" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="9.144" y1="-0.127" x2="8.636" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="11.684" y1="-0.127" x2="11.176" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.8636" x2="-0.9906" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-1.1176" x2="-0.9906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.716" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.97" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-1.1176" x2="13.6906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.97" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.8636" x2="13.6906" y2="1.143" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51" rot="R90"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="-1.143" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.143" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6_LOCK" urn="urn:adsk.eagle:footprint:37741/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="13.97" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="13.97" y1="-2.54" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="12.7" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="12.7" y2="-1.27" width="0.127" layer="21"/>
<wire x1="12.7" y1="-1.27" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="-0.635" y2="1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="4.445" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.191" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX_1X6_RA_LOCK" urn="urn:adsk.eagle:footprint:37590/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
tPlace shows location of connector.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="-1.27" y2="0.635" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.175" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="12.7" y1="3.175" x2="0" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="0" y2="7.62" width="0.127" layer="21"/>
<wire x1="0" y1="7.62" x2="12.7" y2="7.62" width="0.127" layer="21"/>
<wire x1="12.7" y1="7.62" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="0.635" y2="-1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.127" drill="1.016" diameter="1.8796"/>
<text x="4.826" y="5.588" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="4.318" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_FEMALE_LOCK.010" urn="urn:adsk.eagle:footprint:37742/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin Locking Header&lt;/h3&gt;
Includes silk outline for 6 pin female header
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/SP-140520-XX-001.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="1.27" x2="13.97" y2="1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-1.27" x2="-1.27" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="1.27" x2="13.97" y2="-1.27" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="-0.3175" y1="-0.1905" x2="0.3175" y2="0.1905" layer="51"/>
<rectangle x1="2.2225" y1="-0.1905" x2="2.8575" y2="0.1905" layer="51"/>
<rectangle x1="4.7625" y1="-0.1905" x2="5.3975" y2="0.1905" layer="51"/>
<rectangle x1="7.3025" y1="-0.1905" x2="7.9375" y2="0.1905" layer="51"/>
<rectangle x1="9.8425" y1="-0.1905" x2="10.4775" y2="0.1905" layer="51"/>
<rectangle x1="12.3825" y1="-0.1905" x2="13.0175" y2="0.1905" layer="51"/>
<text x="-1.143" y="1.524" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.143" y="-2.159" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LONGPADS" urn="urn:adsk.eagle:footprint:37591/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
</package>
<package name="SCREWTERMINAL-3.5MM-6" urn="urn:adsk.eagle:footprint:37743/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -6 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="19.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="19.25" y1="3.4" x2="19.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-2.8" x2="19.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="19.25" y1="3.15" x2="19.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="19.75" y1="3.15" x2="19.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="19.75" y1="2.15" x2="19.25" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.032"/>
<pad name="4" x="10.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="5" x="14" y="0" drill="1.2" diameter="2.032"/>
<pad name="6" x="17.5" y="0" drill="1.2" diameter="2.032"/>
<text x="7.112" y="2.413" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="6.858" y="1.524" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-SMD-FEMALE" urn="urn:adsk.eagle:footprint:37744/1" library_version="1">
<description>&lt;h3&gt;Header - 6 pin Female SMD&lt;/h3&gt;
Right angle 0.1"
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/19686.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-7.5" y1="0.45" x2="-7.5" y2="-8.05" width="0.127" layer="21"/>
<wire x1="7.5" y1="0.45" x2="-7.5" y2="0.45" width="0.127" layer="21"/>
<wire x1="7.5" y1="-8.05" x2="7.5" y2="0.45" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-8.05" x2="7.5" y2="-8.05" width="0.127" layer="21"/>
<smd name="4" x="-1.27" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="5" x="-3.81" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="6" x="-6.35" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="3" x="1.27" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="2" x="3.81" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="1" x="6.35" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<text x="-1.524" y="-3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.778" y="-4.826" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_HOLES_ONLY" urn="urn:adsk.eagle:footprint:37745/1" library_version="1">
<description>&lt;h3&gt; 6 Pin Holes&lt;/h3&gt;
No silk, no plating
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="5.08" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="7.62" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="10.16" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="12.7" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<hole x="5.08" y="0" drill="1.4732"/>
<hole x="7.62" y="0" drill="1.4732"/>
<hole x="10.16" y="0" drill="1.4732"/>
<hole x="12.7" y="0" drill="1.4732"/>
</package>
<package name="1X06_SMD_STRAIGHT" urn="urn:adsk.eagle:footprint:37746/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.37" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="1.25" x2="1.37" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="-1.25" x2="-14.07" y2="1.25" width="0.127" layer="21"/>
<wire x1="0.85" y1="1.25" x2="1.37" y2="1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="1.25" x2="-10.883" y2="1.25" width="0.127" layer="21"/>
<wire x1="-13.55" y1="-1.25" x2="-14.07" y2="-1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="-1.25" x2="-1.817" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-4.377" y1="1.25" x2="-0.703" y2="1.25" width="0.127" layer="21"/>
<wire x1="-9.457" y1="1.25" x2="-5.783" y2="1.25" width="0.127" layer="21"/>
<wire x1="-3.329" y1="-1.25" x2="-6.831" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-8.409" y1="-1.25" x2="-11.911" y2="-1.25" width="0.127" layer="21"/>
<smd name="5" x="-10.16" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="3" x="-5.08" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="1" x="0" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="6" x="-12.7" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="4" x="-7.62" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-2.54" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<text x="-13.716" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-13.843" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_STRAIGHT_ALT" urn="urn:adsk.eagle:footprint:37747/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
Alternate pin configuration
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.37" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="21"/>
<wire x1="-13.55" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="1.25" x2="-1.817" y2="1.25" width="0.127" layer="21"/>
<wire x1="0.85" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="-1.25" x2="-10.883" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-8.323" y1="1.25" x2="-11.997" y2="1.25" width="0.127" layer="21"/>
<wire x1="-3.243" y1="1.25" x2="-6.917" y2="1.25" width="0.127" layer="21"/>
<wire x1="-9.371" y1="-1.25" x2="-5.869" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-4.291" y1="-1.25" x2="-0.789" y2="-1.25" width="0.127" layer="21"/>
<smd name="5" x="-10.16" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="3" x="-5.08" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1" x="0" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="6" x="-12.7" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="4" x="-7.62" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="2" x="-2.54" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<text x="-13.716" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-13.843" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_STRAIGHT_COMBO" urn="urn:adsk.eagle:footprint:37748/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header - Combined Footprint&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="12.7" y1="1.27" x2="12.7" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="10.16" y1="1.27" x2="10.16" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="7.62" y1="1.27" x2="7.62" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="5.08" y1="1.27" x2="5.08" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="2.54" y1="1.27" x2="2.54" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="0" y1="1.27" x2="0" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="-1.37" y1="-1.25" x2="-1.37" y2="1.25" width="0.1778" layer="21"/>
<wire x1="14.07" y1="1.25" x2="14.07" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-0.73" y1="-1.25" x2="-1.37" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="14.07" y1="-1.25" x2="13.4" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.4" y1="1.25" x2="14.07" y2="1.25" width="0.1778" layer="21"/>
<wire x1="-1.37" y1="1.25" x2="-0.73" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.949" y1="1.25" x2="11.911" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.949" y1="-1.29" x2="11.911" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="8.409" y1="1.25" x2="9.371" y2="1.25" width="0.1778" layer="21"/>
<wire x1="8.409" y1="-1.29" x2="9.371" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="5.869" y1="-1.29" x2="6.831" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="5.869" y1="1.25" x2="6.831" y2="1.25" width="0.1778" layer="21"/>
<wire x1="3.329" y1="-1.29" x2="4.291" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="3.329" y1="1.25" x2="4.291" y2="1.25" width="0.1778" layer="21"/>
<wire x1="0.789" y1="-1.29" x2="1.751" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="0.789" y1="1.25" x2="1.751" y2="1.25" width="0.1778" layer="21"/>
<smd name="5" x="10.16" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="3" x="5.08" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1" x="0" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="6" x="12.7" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="4" x="7.62" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="2" x="2.54" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1-2" x="0" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="2-2" x="2.54" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="3-2" x="5.08" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="4-2" x="7.62" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="5-2" x="10.16" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="6-2" x="12.7" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<text x="-0.508" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.508" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_MALE" urn="urn:adsk.eagle:footprint:37749/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Male Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="13.97" y2="-1.25" width="0.127" layer="51"/>
<wire x1="13.97" y1="-1.25" x2="13.97" y2="1.25" width="0.127" layer="51"/>
<wire x1="13.97" y1="1.25" x2="-1.27" y2="1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="1.25" x2="-1.27" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-1.27" y1="-1.25" x2="-0.635" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-1.27" y1="1.25" x2="-0.635" y2="1.25" width="0.1778" layer="21"/>
<wire x1="0.762" y1="1.25" x2="1.778" y2="1.25" width="0.1778" layer="21"/>
<wire x1="3.302" y1="1.25" x2="4.318" y2="1.25" width="0.1778" layer="21"/>
<wire x1="5.842" y1="1.25" x2="6.858" y2="1.25" width="0.1778" layer="21"/>
<wire x1="8.382" y1="1.25" x2="9.398" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.922" y1="1.25" x2="11.938" y2="1.25" width="0.1778" layer="21"/>
<wire x1="1.778" y1="-1.25" x2="0.762" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="4.318" y1="-1.25" x2="3.302" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="6.858" y1="-1.25" x2="5.842" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="9.398" y1="-1.25" x2="8.382" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="11.938" y1="-1.25" x2="10.922" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="-1.25" x2="13.97" y2="1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="-1.25" x2="13.335" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="1.25" x2="13.335" y2="1.25" width="0.1778" layer="21"/>
<circle x="0" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="5.08" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="7.62" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="10.16" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="12.7" y="0" radius="0.64" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="0" x2="0.32" y2="2.75" layer="51"/>
<rectangle x1="4.76" y1="0" x2="5.4" y2="2.75" layer="51"/>
<rectangle x1="9.84" y1="0" x2="10.48" y2="2.75" layer="51"/>
<rectangle x1="2.22" y1="-2.75" x2="2.86" y2="0" layer="51" rot="R180"/>
<rectangle x1="7.3" y1="-2.75" x2="7.94" y2="0" layer="51" rot="R180"/>
<rectangle x1="12.38" y1="-2.75" x2="13.02" y2="0" layer="51" rot="R180"/>
<smd name="1" x="0" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="2" x="2.54" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="3" x="5.08" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="4" x="7.62" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="5" x="10.16" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="6" x="12.7" y="0" dx="1.02" dy="6" layer="1"/>
<text x="-0.508" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.635" y="-3.937" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-1MM" urn="urn:adsk.eagle:footprint:37635/1" library_version="1">
<description>&lt;h3&gt;JST SH Vertical  6-Pin Connector -SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1mm&lt;/li&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;li&gt;EM-406&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2.54" y1="-1.651" x2="2.54" y2="-1.651" width="0.254" layer="21"/>
<wire x1="-4.318" y1="0.508" x2="-4.318" y2="1.905" width="0.254" layer="21"/>
<wire x1="3.302" y1="1.905" x2="4.318" y2="1.905" width="0.254" layer="21"/>
<wire x1="4.318" y1="1.905" x2="4.318" y2="0.508" width="0.254" layer="21"/>
<wire x1="-4.318" y1="1.905" x2="-3.302" y2="1.905" width="0.254" layer="21"/>
<smd name="1" x="-2.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="2" x="-1.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="3" x="-0.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="4" x="0.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="5" x="1.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="6" x="2.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="P$1" x="-3.84" y="-0.955" dx="1.2" dy="1.8" layer="1"/>
<smd name="P$2" x="3.76" y="-0.955" dx="1.2" dy="1.8" layer="1"/>
<text x="-1.397" y="-0.381" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<circle x="-3.6" y="2.47" radius="0.1047" width="0.4064" layer="21"/>
</package>
<package name="1X06_NO_SILK" urn="urn:adsk.eagle:footprint:37750/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_1.27MM" urn="urn:adsk.eagle:footprint:37751/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.381" y1="-0.889" x2="0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="-0.889" x2="0.635" y2="-0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="-0.635" x2="0.889" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="-0.889" x2="1.651" y2="-0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="-0.889" x2="1.905" y2="-0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="-0.635" x2="2.159" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="-0.889" x2="2.921" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="-0.889" x2="3.175" y2="-0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="-0.635" x2="3.429" y2="-0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="-0.889" x2="4.191" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="-0.889" x2="4.445" y2="-0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="-0.635" x2="4.699" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="-0.889" x2="5.461" y2="-0.889" width="0.127" layer="21"/>
<wire x1="5.461" y1="0.889" x2="4.699" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="0.889" x2="4.445" y2="0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="0.635" x2="4.191" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="0.889" x2="3.429" y2="0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="0.889" x2="3.175" y2="0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="0.635" x2="2.921" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="0.889" x2="2.159" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="0.889" x2="1.905" y2="0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="0.635" x2="1.651" y2="0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="0.889" x2="0.889" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="0.889" x2="0.635" y2="0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="0.635" x2="0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="0.889" x2="-0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="-0.381" y1="0.889" x2="-0.889" y2="0.381" width="0.127" layer="21"/>
<wire x1="-0.889" y1="-0.381" x2="-0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="-0.889" y1="0.381" x2="-0.889" y2="-0.381" width="0.127" layer="21"/>
<wire x1="5.461" y1="-0.889" x2="5.715" y2="-0.635" width="0.127" layer="21"/>
<wire x1="5.715" y1="-0.635" x2="5.969" y2="-0.889" width="0.127" layer="21"/>
<wire x1="5.969" y1="-0.889" x2="6.731" y2="-0.889" width="0.127" layer="21"/>
<wire x1="6.731" y1="0.889" x2="5.969" y2="0.889" width="0.127" layer="21"/>
<wire x1="5.969" y1="0.889" x2="5.715" y2="0.635" width="0.127" layer="21"/>
<wire x1="5.715" y1="0.635" x2="5.461" y2="0.889" width="0.127" layer="21"/>
<wire x1="6.731" y1="0.889" x2="7.239" y2="0.381" width="0.127" layer="21"/>
<wire x1="7.239" y1="0.381" x2="7.239" y2="-0.381" width="0.127" layer="21"/>
<wire x1="7.239" y1="-0.381" x2="6.731" y2="-0.889" width="0.127" layer="21"/>
<pad name="5" x="5.08" y="0" drill="0.508" diameter="1"/>
<pad name="4" x="3.81" y="0" drill="0.508" diameter="1"/>
<pad name="3" x="2.54" y="0" drill="0.508" diameter="1"/>
<pad name="2" x="1.27" y="0" drill="0.508" diameter="1"/>
<pad name="1" x="0" y="0" drill="0.508" diameter="1"/>
<pad name="6" x="6.35" y="0" drill="0.508" diameter="1"/>
<text x="-0.381" y="1.016" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.381" y="-1.651" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05" urn="urn:adsk.eagle:footprint:37722/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="9.525" y2="1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.27" x2="10.795" y2="1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.27" x2="11.43" y2="0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.635" x2="10.795" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.27" x2="9.525" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.27" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.635" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_1.27MM" urn="urn:adsk.eagle:footprint:37723/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.381" y1="-0.889" x2="0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="-0.889" x2="0.635" y2="-0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="-0.635" x2="0.889" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="-0.889" x2="1.651" y2="-0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="-0.889" x2="1.905" y2="-0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="-0.635" x2="2.159" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="-0.889" x2="2.921" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="-0.889" x2="3.175" y2="-0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="-0.635" x2="3.429" y2="-0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="-0.889" x2="4.191" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="-0.889" x2="4.445" y2="-0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="-0.635" x2="4.699" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="-0.889" x2="5.461" y2="-0.889" width="0.127" layer="21"/>
<wire x1="5.461" y1="0.889" x2="4.699" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="0.889" x2="4.445" y2="0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="0.635" x2="4.191" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="0.889" x2="3.429" y2="0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="0.889" x2="3.175" y2="0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="0.635" x2="2.921" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="0.889" x2="2.159" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="0.889" x2="1.905" y2="0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="0.635" x2="1.651" y2="0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="0.889" x2="0.889" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="0.889" x2="0.635" y2="0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="0.635" x2="0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="0.889" x2="-0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="-0.381" y1="0.889" x2="-0.889" y2="0.381" width="0.127" layer="21"/>
<wire x1="-0.889" y1="-0.381" x2="-0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="-0.889" y1="0.381" x2="-0.889" y2="-0.381" width="0.127" layer="21"/>
<wire x1="5.461" y1="0.889" x2="5.969" y2="0.381" width="0.127" layer="21"/>
<wire x1="5.969" y1="0.381" x2="5.969" y2="-0.381" width="0.127" layer="21"/>
<wire x1="5.969" y1="-0.381" x2="5.461" y2="-0.889" width="0.127" layer="21"/>
<pad name="5" x="5.08" y="0" drill="0.508" diameter="1"/>
<pad name="4" x="3.81" y="0" drill="0.508" diameter="1"/>
<pad name="3" x="2.54" y="0" drill="0.508" diameter="1"/>
<pad name="2" x="1.27" y="0" drill="0.508" diameter="1"/>
<pad name="1" x="0" y="0" drill="0.508" diameter="1"/>
<text x="-0.381" y="1.143" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.508" y="-1.651" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_LOCK" urn="urn:adsk.eagle:footprint:37724/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="9.525" y2="1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.27" x2="10.795" y2="1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.27" x2="11.43" y2="0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.635" x2="10.795" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.27" x2="9.525" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.27" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.635" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37725/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin Long Pad with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.524" y1="-0.127" x2="1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="4.064" y1="-0.127" x2="3.556" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="6.604" y1="-0.127" x2="6.096" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="9.144" y1="-0.127" x2="8.636" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.8636" x2="-0.9906" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-1.1176" x2="-0.9906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.127" x2="11.176" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.127" x2="11.43" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-1.1176" x2="11.1506" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.127" x2="11.43" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.8636" x2="11.1506" y2="1.143" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51" rot="R90"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<text x="-1.27" y="1.778" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.397" y="-2.413" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_LONGPADS" urn="urn:adsk.eagle:footprint:37726/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.635" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_1MM" urn="urn:adsk.eagle:footprint:37637/1" library_version="1">
<description>&lt;h3&gt;SMD - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.sparkfun.com/datasheets/GPS/EM408-SMDConnector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;li&gt;EM-408&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="2" y1="2.921" x2="-2.08" y2="2.921" width="0.254" layer="21"/>
<wire x1="3.778" y1="0.762" x2="3.778" y2="-0.635" width="0.254" layer="21"/>
<wire x1="-2.842" y1="-0.635" x2="-3.858" y2="-0.635" width="0.254" layer="21"/>
<wire x1="-3.858" y1="-0.635" x2="-3.858" y2="0.762" width="0.254" layer="21"/>
<wire x1="3.778" y1="-0.635" x2="2.762" y2="-0.635" width="0.254" layer="21"/>
<smd name="NC2" x="3.3" y="2.225" dx="1.2" dy="1.8" layer="1" rot="R180"/>
<smd name="NC1" x="-3.3" y="2.225" dx="1.2" dy="1.8" layer="1" rot="R180"/>
<smd name="5" x="2" y="0" dx="0.6" dy="1.55" layer="1" rot="R180"/>
<smd name="4" x="1" y="0" dx="0.6" dy="1.55" layer="1" rot="R180"/>
<smd name="3" x="0" y="0" dx="0.6" dy="1.55" layer="1" rot="R180"/>
<smd name="2" x="-1" y="0" dx="0.6" dy="1.55" layer="1" rot="R180"/>
<smd name="1" x="-2" y="0" dx="0.6" dy="1.55" layer="1" rot="R180"/>
<text x="-1.524" y="1.905" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.524" y="1.143" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<circle x="3.81" y="-1.27" radius="0" width="0.508" layer="21"/>
</package>
<package name="1X05_1MM_RA" urn="urn:adsk.eagle:footprint:37727/1" library_version="1">
<description>&lt;h3&gt;SMD - 5 Pin Right Angle&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="-4.6" x2="2" y2="-4.6" width="0.254" layer="21"/>
<wire x1="-3.5" y1="-2" x2="-3.5" y2="-0.35" width="0.254" layer="21"/>
<wire x1="2.75" y1="-0.35" x2="3.5" y2="-0.35" width="0.254" layer="21"/>
<wire x1="3.5" y1="-0.35" x2="3.5" y2="-2" width="0.254" layer="21"/>
<wire x1="-3.5" y1="-0.35" x2="-2.75" y2="-0.35" width="0.254" layer="21"/>
<circle x="-3" y="0.3" radius="0.1414" width="0.4" layer="21"/>
<smd name="NC2" x="-3.3" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="NC1" x="3.3" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="1" x="-2" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="2" x="-1" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="3" x="0" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="4" x="1" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="5" x="2" y="0" dx="0.6" dy="1.35" layer="1"/>
<text x="-1.397" y="-2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X05_NO_SILK" urn="urn:adsk.eagle:footprint:37728/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-5-PTH" urn="urn:adsk.eagle:footprint:37729/1" library_version="1">
<description>&lt;h3&gt;JST 5 Pin Right Angle Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="-4" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="-2" y="0" drill="0.7" diameter="1.6"/>
<pad name="3" x="0" y="0" drill="0.7" diameter="1.6"/>
<pad name="4" x="2" y="0" drill="0.7" diameter="1.6"/>
<pad name="5" x="4" y="0" drill="0.7" diameter="1.6"/>
<wire x1="-5.95" y1="-1.6" x2="-5.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-5.95" y1="6" x2="5.95" y2="6" width="0.2032" layer="21"/>
<wire x1="5.95" y1="6" x2="5.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-5.95" y1="-1.6" x2="-5.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="5.95" y1="-1.6" x2="5.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-5.3" y1="-1.6" x2="-5.3" y2="0" width="0.2032" layer="21"/>
<wire x1="5.3" y1="-1.6" x2="5.3" y2="0" width="0.2032" layer="21"/>
<text x="-1.397" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="2.413" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-5-PTH-VERT" urn="urn:adsk.eagle:footprint:37730/1" library_version="1">
<description>&lt;h3&gt;JST 5 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-5.95" y1="-1.52" x2="-5.95" y2="2.98" width="0.2032" layer="21"/>
<wire x1="-5.95" y1="2.98" x2="5.95" y2="2.98" width="0.2032" layer="21"/>
<wire x1="5.95" y1="-1.52" x2="1" y2="-1.52" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.52" x2="-5.95" y2="-1.52" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.02" x2="1" y2="-1.02" width="0.2032" layer="21"/>
<wire x1="1" y1="-1.02" x2="1" y2="-1.52" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.02" x2="-1" y2="-1.52" width="0.2032" layer="21"/>
<wire x1="5.95" y1="2.98" x2="5.95" y2="-1.52" width="0.2032" layer="21"/>
<pad name="1" x="-4" y="0.18" drill="0.7" diameter="1.6"/>
<pad name="2" x="-2" y="0.18" drill="0.7" diameter="1.6"/>
<pad name="3" x="0" y="0.18" drill="0.7" diameter="1.6"/>
<pad name="4" x="2" y="0.18" drill="0.7" diameter="1.6"/>
<pad name="5" x="4" y="0.18" drill="0.7" diameter="1.6"/>
<text x="-1.651" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.905" y="-2.54" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-5" urn="urn:adsk.eagle:footprint:37731/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -5 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="15.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="15.75" y1="3.4" x2="15.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="15.75" y1="-2.8" x2="15.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="15.75" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="15.75" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="15.75" y1="3.15" x2="16.25" y2="3.15" width="0.2032" layer="51"/>
<wire x1="16.25" y1="3.15" x2="16.25" y2="2.15" width="0.2032" layer="51"/>
<wire x1="16.25" y1="2.15" x2="15.75" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.032"/>
<pad name="4" x="10.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="5" x="14" y="0" drill="1.2" diameter="2.032"/>
<text x="5.588" y="2.413" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="5.334" y="1.524" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03" urn="urn:adsk.eagle:footprint:37678/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.635" x2="6.35" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X3" urn="urn:adsk.eagle:footprint:37679/1" library_version="1">
<description>&lt;h3&gt;PTH - 3 Pin Vertical Molex Polarized Header&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/01932.pdf"&gt; 4UCONN part # 01932 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="6.35" y1="3.048" x2="6.35" y2="-2.54" width="0.127" layer="21"/>
<wire x1="6.35" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="6.35" y1="-2.54" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<text x="1.143" y="2.159" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="0.889" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-3" urn="urn:adsk.eagle:footprint:37680/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="8.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="8.75" y1="3.4" x2="8.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-2.8" x2="8.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.75" y1="3.15" x2="9.25" y2="3.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="3.15" x2="9.25" y2="2.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="2.15" x2="8.75" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.413" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.413"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.413"/>
<text x="2.159" y="3.683" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="2.032" y="-4.572" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_LOCK" urn="urn:adsk.eagle:footprint:37681/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint&lt;/h3&gt;
Pins are staggered 0.005" off center to lock pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.635" x2="6.35" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37682/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pad w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.524" y1="-0.127" x2="1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="4.064" y1="-0.127" x2="3.556" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.8636" x2="-0.9906" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-1.1176" x2="-0.9906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.127" x2="6.096" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.127" x2="6.35" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-1.1176" x2="6.0706" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.127" x2="6.35" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.8636" x2="6.0706" y2="1.143" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<text x="-1.27" y="1.778" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.413" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X3_LOCK" urn="urn:adsk.eagle:footprint:37683/1" library_version="1">
<description>&lt;h3&gt;PTH - 3 Pin Vertical Molex Polarized Header&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/01932.pdf"&gt; 4UCONN part # 01932 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="6.35" y1="3.048" x2="6.35" y2="-2.54" width="0.127" layer="21"/>
<wire x1="6.35" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="6.35" y1="-2.54" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<rectangle x1="4.7879" y1="-0.2921" x2="5.3721" y2="0.2921" layer="51"/>
<text x="1.143" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="0.889" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S" urn="urn:adsk.eagle:footprint:37684/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH Locking&lt;/h3&gt;
Holes are offset 0.007" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="8.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="8.75" y1="3.4" x2="8.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-2.8" x2="8.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="8.75" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.75" y1="3.15" x2="9.25" y2="3.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="3.15" x2="9.25" y2="2.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="2.15" x2="8.75" y2="2.15" width="0.2032" layer="51"/>
<circle x="0" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="3.5" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="7" y="0" radius="0.425" width="0.001" layer="51"/>
<pad name="1" x="-0.1778" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="7.1778" y="0" drill="1.2" diameter="2.032"/>
<text x="2.032" y="3.683" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="1.905" y="-4.699" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_NO_SILK" urn="urn:adsk.eagle:footprint:37685/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_LONGPADS" urn="urn:adsk.eagle:footprint:37686/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.635" x2="6.35" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-3-PTH" urn="urn:adsk.eagle:footprint:37687/1" library_version="1">
<description>&lt;h3&gt;JST 3 Pin Right Angle Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.95" y1="-1.6" x2="-3.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-3.95" y1="6" x2="3.95" y2="6" width="0.2032" layer="21"/>
<wire x1="3.95" y1="6" x2="3.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-3.95" y1="-1.6" x2="-3.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="3.95" y1="-1.6" x2="3.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-3.3" y1="-1.6" x2="-3.3" y2="0" width="0.2032" layer="21"/>
<wire x1="3.3" y1="-1.6" x2="3.3" y2="0" width="0.2032" layer="21"/>
<pad name="1" x="-2" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="0" y="0" drill="0.7" diameter="1.6"/>
<pad name="3" x="2" y="0" drill="0.7" diameter="1.6"/>
<text x="-2.4" y="0.67" size="1.27" layer="51">+</text>
<text x="-0.4" y="0.67" size="1.27" layer="51">-</text>
<text x="1.7" y="0.87" size="0.8" layer="51">S</text>
<text x="-1.397" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="2.54" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_PP_HOLES_ONLY" urn="urn:adsk.eagle:footprint:37688/1" library_version="1">
<description>&lt;h3&gt;Pogo Pins - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="5.08" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.9" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.9" diameter="0.8128" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="0.9" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<hole x="5.08" y="0" drill="1.4732"/>
<text x="-1.27" y="1.143" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-1.778" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-5MM-3" urn="urn:adsk.eagle:footprint:37689/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.1" y1="4.2" x2="13.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="13.1" y1="4.2" x2="13.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="13.1" y1="-2.3" x2="13.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="13.1" y1="-3.3" x2="-3.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-3.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-2.3" x2="-3.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="13.1" y1="-2.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-1.35" x2="-3.7" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-1.35" x2="-3.7" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-2.35" x2="-3.1" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="13.1" y1="4" x2="13.7" y2="4" width="0.2032" layer="51"/>
<wire x1="13.7" y1="4" x2="13.7" y2="3" width="0.2032" layer="51"/>
<wire x1="13.7" y1="3" x2="13.1" y2="3" width="0.2032" layer="51"/>
<circle x="2.5" y="3.7" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.3" diameter="2.413" shape="square"/>
<pad name="2" x="5" y="0" drill="1.3" diameter="2.413"/>
<pad name="3" x="10" y="0" drill="1.3" diameter="2.413"/>
<text x="3.683" y="2.794" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="3.429" y="1.905" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_LOCK_NO_SILK" urn="urn:adsk.eagle:footprint:37690/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint w/out Silk Outline&lt;/h3&gt;
Holes are offset from center 0.005" to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-3-SMD" urn="urn:adsk.eagle:footprint:37691/1" library_version="1">
<description>&lt;h3&gt;JST 3 Pin Right Angle SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.99" y1="-2.07" x2="-4.99" y2="-5.57" width="0.2032" layer="21"/>
<wire x1="-4.99" y1="-5.57" x2="-4.19" y2="-5.57" width="0.2032" layer="21"/>
<wire x1="-4.19" y1="-5.57" x2="-4.19" y2="-3.07" width="0.2032" layer="21"/>
<wire x1="-4.19" y1="-3.07" x2="-2.99" y2="-3.07" width="0.2032" layer="21"/>
<wire x1="3.01" y1="-3.07" x2="4.21" y2="-3.07" width="0.2032" layer="21"/>
<wire x1="4.21" y1="-3.07" x2="4.21" y2="-5.57" width="0.2032" layer="21"/>
<wire x1="4.21" y1="-5.57" x2="5.01" y2="-5.57" width="0.2032" layer="21"/>
<wire x1="5.01" y1="-5.57" x2="5.01" y2="-2.07" width="0.2032" layer="21"/>
<wire x1="3.01" y1="1.93" x2="-2.99" y2="1.93" width="0.2032" layer="21"/>
<smd name="1" x="-1.99" y="-4.77" dx="1" dy="4.6" layer="1"/>
<smd name="3" x="2.01" y="-4.77" dx="1" dy="4.6" layer="1"/>
<smd name="NC1" x="-4.39" y="0.43" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<smd name="NC2" x="4.41" y="0.43" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<smd name="2" x="0.01" y="-4.77" dx="1" dy="4.6" layer="1"/>
<text x="-1.397" y="0.635" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03-1MM-RA" urn="urn:adsk.eagle:footprint:37692/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1" y1="-4.6" x2="1" y2="-4.6" width="0.254" layer="21"/>
<wire x1="-2.5" y1="-2" x2="-2.5" y2="-0.35" width="0.254" layer="21"/>
<wire x1="1.75" y1="-0.35" x2="2.4997" y2="-0.35" width="0.254" layer="21"/>
<wire x1="2.4997" y1="-0.35" x2="2.4997" y2="-2" width="0.254" layer="21"/>
<wire x1="-2.5" y1="-0.35" x2="-1.75" y2="-0.35" width="0.254" layer="21"/>
<circle x="-2" y="0.3" radius="0.1414" width="0.4" layer="21"/>
<smd name="NC2" x="-2.3" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="NC1" x="2.3" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="1" x="-1" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="2" x="0" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="3" x="1" y="0" dx="0.6" dy="1.35" layer="1"/>
<text x="-1.397" y="-1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-2.54" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_SMD_RA_FEMALE" urn="urn:adsk.eagle:footprint:37693/1" library_version="1">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Female Header&lt;/h3&gt;
Silk outline of pin location
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.935" y1="4.25" x2="-3.935" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="3.935" y1="4.25" x2="-3.935" y2="4.25" width="0.1778" layer="21"/>
<wire x1="3.935" y1="-4.25" x2="3.935" y2="4.25" width="0.1778" layer="21"/>
<wire x1="-3.935" y1="-4.25" x2="3.935" y2="-4.25" width="0.1778" layer="21"/>
<rectangle x1="-0.32" y1="6.8" x2="0.32" y2="7.65" layer="51"/>
<rectangle x1="2.22" y1="6.8" x2="2.86" y2="7.65" layer="51"/>
<rectangle x1="-2.86" y1="6.8" x2="-2.22" y2="7.65" layer="51"/>
<smd name="3" x="2.54" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="2" x="0" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="1" x="-2.54" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<text x="-1.524" y="0.889" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_SMD_RA_MALE" urn="urn:adsk.eagle:footprint:37694/1" library_version="1">
<description>&lt;h3&gt;SMD- 3 Pin Right Angle Male Headers&lt;/h3&gt;
No silk outline, but tDocu layer shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="3.81" y1="1.25" x2="-3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="-3.81" y1="1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="2.53" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="-0.01" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-2.55" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="2.53" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-0.01" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-2.55" y2="-7.25" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="4.15" x2="0.32" y2="5.95" layer="51"/>
<rectangle x1="-2.86" y1="4.15" x2="-2.22" y2="5.95" layer="51"/>
<rectangle x1="2.22" y1="4.15" x2="2.86" y2="5.95" layer="51"/>
<smd name="1" x="-2.54" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="2" x="0" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="3" x="2.54" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<text x="-1.524" y="0.254" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-0.889" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_SMD_RA_MALE_POST" urn="urn:adsk.eagle:footprint:37695/1" library_version="1">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Male Header w/ Alignment Posts&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/11026.pdf"&gt; 4UCONN part # 11026 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="3.81" y1="1.25" x2="-3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="-3.81" y1="1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="2.53" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="-0.01" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-2.55" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="2.53" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-0.01" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-2.55" y2="-7.25" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="4.15" x2="0.32" y2="5.95" layer="51"/>
<rectangle x1="-2.86" y1="4.15" x2="-2.22" y2="5.95" layer="51"/>
<rectangle x1="2.22" y1="4.15" x2="2.86" y2="5.95" layer="51"/>
<smd name="1" x="-2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="2" x="0" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="3" x="2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<hole x="-1.27" y="0" drill="1.6"/>
<hole x="1.27" y="0" drill="1.6"/>
<text x="-1.397" y="1.524" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-3-PTH-VERT" urn="urn:adsk.eagle:footprint:37696/1" library_version="1">
<description>&lt;h3&gt;JST 3 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.95" y1="-2.25" x2="-3.95" y2="2.25" width="0.2032" layer="21"/>
<wire x1="-3.95" y1="2.25" x2="3.95" y2="2.25" width="0.2032" layer="21"/>
<wire x1="3.95" y1="2.25" x2="3.95" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="3.95" y1="-2.25" x2="1" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-2.25" x2="-3.95" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.75" x2="1" y2="-1.75" width="0.2032" layer="21"/>
<wire x1="1" y1="-1.75" x2="1" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.75" x2="-1" y2="-2.25" width="0.2032" layer="21"/>
<pad name="1" x="-2" y="-0.55" drill="0.7" diameter="1.6"/>
<pad name="2" x="0" y="-0.55" drill="0.7" diameter="1.6"/>
<pad name="3" x="2" y="-0.55" drill="0.7" diameter="1.6"/>
<text x="-2.4" y="0.75" size="1.27" layer="51">+</text>
<text x="-0.4" y="0.75" size="1.27" layer="51">-</text>
<text x="1.7" y="0.95" size="0.8" layer="51">S</text>
<text x="-1.397" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X03_SMD_RA_MALE_POST_SMALLER" urn="urn:adsk.eagle:footprint:37697/1" library_version="1">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Male Header w/ Alignment Posts&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/11026.pdf"&gt; 4UCONN part # 11026 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="3.81" y1="1.25" x2="-3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="-3.81" y1="1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="2.53" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="-0.01" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-2.55" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="2.53" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-0.01" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-2.55" y2="-7.25" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="4.15" x2="0.32" y2="5.95" layer="51"/>
<rectangle x1="-2.86" y1="4.15" x2="-2.22" y2="5.95" layer="51"/>
<rectangle x1="2.22" y1="4.15" x2="2.86" y2="5.95" layer="51"/>
<smd name="1" x="-2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="2" x="0" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="3" x="2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<hole x="-1.27" y="0" drill="1.3589"/>
<hole x="1.27" y="0" drill="1.3589"/>
</package>
<package name="1X03_SMD_RA_MALE_POST_SMALLEST" urn="urn:adsk.eagle:footprint:37698/1" library_version="1">
<wire x1="3.81" y1="1.25" x2="-3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="-3.81" y1="1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="2.53" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="-0.01" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-2.55" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-3.81" y2="-1.25" width="0.1778" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="1.25" width="0.1778" layer="51"/>
<wire x1="2.53" y1="-1.25" x2="2.53" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-0.01" y1="-1.25" x2="-0.01" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-2.55" y1="-1.25" x2="-2.55" y2="-7.25" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="4.15" x2="0.32" y2="5.95" layer="51"/>
<rectangle x1="-2.86" y1="4.15" x2="-2.22" y2="5.95" layer="51"/>
<rectangle x1="2.22" y1="4.15" x2="2.86" y2="5.95" layer="51"/>
<smd name="1" x="-2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="2" x="0" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<smd name="3" x="2.54" y="5.07" dx="2.5" dy="1.27" layer="1" rot="R90"/>
<hole x="-1.27" y="0" drill="1.3462"/>
<hole x="1.27" y="0" drill="1.3462"/>
</package>
<package name="JST-3-PTH-NS" urn="urn:adsk.eagle:footprint:37699/1" library_version="1">
<description>&lt;h3&gt;JST 3 Pin Right Angle Plated Through Hole &amp;ndash; NO SILK&lt;/h3&gt;
&lt;p&gt;No silkscreen outline. tDoc layer (51) indicates connector footprint.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.95" y1="-1.6" x2="-3.95" y2="6" width="0.2032" layer="51"/>
<wire x1="-3.95" y1="6" x2="3.95" y2="6" width="0.2032" layer="51"/>
<wire x1="3.95" y1="6" x2="3.95" y2="-1.6" width="0.2032" layer="51"/>
<wire x1="-3.95" y1="-1.6" x2="-3.3" y2="-1.6" width="0.2032" layer="51"/>
<wire x1="3.95" y1="-1.6" x2="3.3" y2="-1.6" width="0.2032" layer="51"/>
<wire x1="-3.3" y1="-1.6" x2="-3.3" y2="0" width="0.2032" layer="51"/>
<wire x1="3.3" y1="-1.6" x2="3.3" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-2" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="0" y="0" drill="0.7" diameter="1.6"/>
<pad name="3" x="2" y="0" drill="0.7" diameter="1.6"/>
<text x="-2.4" y="0.67" size="1.27" layer="51">+</text>
<text x="-0.4" y="0.67" size="1.27" layer="51">-</text>
<text x="1.7" y="0.87" size="0.8" layer="51">S</text>
<text x="-1.397" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="2.54" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-3-NS" urn="urn:adsk.eagle:footprint:37700/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH &amp;ndash; NO SILK&lt;/h3&gt;
&lt;p&gt;No silkscreen outline. tDoc layer (51) indicates connector footprint.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="8.75" y2="3.4" width="0.2032" layer="51"/>
<wire x1="8.75" y1="3.4" x2="8.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="8.75" y1="-2.8" x2="8.75" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="8.75" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="51"/>
<wire x1="8.75" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.75" y1="3.15" x2="9.25" y2="3.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="3.15" x2="9.25" y2="2.15" width="0.2032" layer="51"/>
<wire x1="9.25" y1="2.15" x2="8.75" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.413"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.413"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.413"/>
<text x="2.159" y="3.683" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="2.032" y="-4.572" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="1X02" urn="urn:adsk.eagle:package:38039/1" type="box" library_version="1">
<description>Plated Through Hole
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X2" urn="urn:adsk.eagle:package:38040/1" type="box" library_version="1">
<description>Molex 2-Pin Plated Through-Hole
Specifications:
Pin count:2
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="MOLEX-1X2"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2" urn="urn:adsk.eagle:package:38050/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2"/>
</packageinstances>
</package3d>
<package3d name="JST-2-SMD" urn="urn:adsk.eagle:package:38042/1" type="box" library_version="1">
<description>JST-Right Angle Male Header SMT
Specifications:
Pin count: 2
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
JST_2MM_MALE
</description>
<packageinstances>
<packageinstance name="JST-2-SMD"/>
</packageinstances>
</package3d>
<package3d name="1X02_BIG" urn="urn:adsk.eagle:package:38043/1" type="box" library_version="1">
<description>Plated Through Hole
Specifications:
Pin count:2
Pin pitch:0.15"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_BIG"/>
</packageinstances>
</package3d>
<package3d name="JST-2-SMD-VERT" urn="urn:adsk.eagle:package:38052/1" type="box" library_version="1">
<description>JST-Vertical Male Header SMT 
Specifications:
Pin count: 2
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-SMD-VERT"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-5MM-2" urn="urn:adsk.eagle:package:38044/1" type="box" library_version="1">
<description>Screw Terminal  5mm Pitch -2 Pin PTH
Specifications:
Pin count: 2
Pin pitch: 5mm/197mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-5MM-2"/>
</packageinstances>
</package3d>
<package3d name="1X02_LOCK" urn="urn:adsk.eagle:package:38045/1" type="box" library_version="1">
<description>Plated Through Hole - Locking Footprint
Holes are staggered by 0.005" from center to hold pins while soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LOCK"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X2_LOCK" urn="urn:adsk.eagle:package:38046/1" type="box" library_version="1">
<description>Molex 2-Pin Plated Through-Hole Locking Footprint
Holes are offset from center by 0.005" to hold pins in place during soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="MOLEX-1X2_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X02_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38047/1" type="box" library_version="1">
<description>Plated Through Hole - Long Pads with Locking Footprint
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2_LOCK" urn="urn:adsk.eagle:package:38049/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking
Holes are offset from center 0.005" to hold pins in place during soldering. 
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X02_LONGPADS" urn="urn:adsk.eagle:package:38048/1" type="box" library_version="1">
<description>Plated Through Hole - Long Pads without Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X02_NO_SILK" urn="urn:adsk.eagle:package:38051/1" type="box" library_version="1">
<description>Plated Through Hole - No Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH" urn="urn:adsk.eagle:package:38053/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH"/>
</packageinstances>
</package3d>
<package3d name="1X02_XTRA_BIG" urn="urn:adsk.eagle:package:38054/1" type="box" library_version="1">
<description>Plated Through Hole - 0.1" holes
Specifications:
Pin count:2
Pin pitch:0.2"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_XTRA_BIG"/>
</packageinstances>
</package3d>
<package3d name="1X02_PP_HOLES_ONLY" urn="urn:adsk.eagle:package:38058/1" type="box" library_version="1">
<description>Pogo Pins Connector - No Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_PP_HOLES_ONLY"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2-NS" urn="urn:adsk.eagle:package:38055/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2-NS"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH-NS" urn="urn:adsk.eagle:package:38056/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole- No Silk
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
 No silk outline of connector. 
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH-NS"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH-KIT" urn="urn:adsk.eagle:package:38057/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole - KIT
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
 This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
 This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH-KIT"/>
</packageinstances>
</package3d>
<package3d name="SPRINGTERMINAL-2.54MM-2" urn="urn:adsk.eagle:package:38061/1" type="box" library_version="1">
<description>Spring Terminal- PCB Mount 2 Pin PTH
tDocu marks the spring arms
Specifications:
Pin count: 4
Pin pitch: 0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SPRINGTERMINAL-2.54MM-2"/>
</packageinstances>
</package3d>
<package3d name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:package:38059/1" type="box" library_version="1">
<description>2 Pin Screw Terminal - 2.54mm
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_2.54_SCREWTERM"/>
</packageinstances>
</package3d>
<package3d name="1X02_POKEHOME" urn="urn:adsk.eagle:package:38060/1" type="box" library_version="1">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
<packageinstances>
<packageinstance name="1X02_POKEHOME"/>
</packageinstances>
</package3d>
<package3d name="1X02_RA_PTH_FEMALE" urn="urn:adsk.eagle:package:38062/1" type="box" library_version="1">
<packageinstances>
<packageinstance name="1X02_RA_PTH_FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X06" urn="urn:adsk.eagle:package:38009/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6" urn="urn:adsk.eagle:package:38117/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6-RA" urn="urn:adsk.eagle:package:38118/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Right Angle
tPlace shows angle of connector. 
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6-RA"/>
</packageinstances>
</package3d>
<package3d name="1X06-SMD_RA_MALE" urn="urn:adsk.eagle:package:38004/1" type="box" library_version="1">
<description>SMD - 6 Pin Right Angle Male Header
tDocu layer shows pin locations.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06-SMD_RA_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X06_LOCK" urn="urn:adsk.eagle:package:38002/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Locking Footprint
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X06_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38121/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Locking Footprint with Long Pads
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6_LOCK" urn="urn:adsk.eagle:package:38123/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Locking Footprint
Holes are offset 0.005" from center to hold pins in place during soldering.  
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6_LOCK"/>
</packageinstances>
</package3d>
<package3d name="MOLEX_1X6_RA_LOCK" urn="urn:adsk.eagle:package:37992/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Right Angle Locking Footprint
Holes are offset 0.005" from center to hold pins in place during soldering.  
tPlace shows location of connector.
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX_1X6_RA_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X06_FEMALE_LOCK.010" urn="urn:adsk.eagle:package:38124/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin Locking Header
Includes silk outline for 6 pin female header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_FEMALE_LOCK.010"/>
</packageinstances>
</package3d>
<package3d name="1X06_LONGPADS" urn="urn:adsk.eagle:package:37991/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Long Pads
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-6" urn="urn:adsk.eagle:package:38122/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -6 Pin PTH
Specifications:
Pin count: 6
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-6"/>
</packageinstances>
</package3d>
<package3d name="1X06-SMD-FEMALE" urn="urn:adsk.eagle:package:38125/1" type="box" library_version="1">
<description>Header - 6 pin Female SMD
Right angle 0.1"
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06-SMD-FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X06_HOLES_ONLY" urn="urn:adsk.eagle:package:38126/1" type="box" library_version="1">
<description> 6 Pin Holes
No silk, no plating
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_HOLES_ONLY"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT" urn="urn:adsk.eagle:package:38139/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT_ALT" urn="urn:adsk.eagle:package:38141/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header
Alternate pin configuration
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT_ALT"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT_COMBO" urn="urn:adsk.eagle:package:38127/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header - Combined Footprint

Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT_COMBO"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_MALE" urn="urn:adsk.eagle:package:38128/1" type="box" library_version="1">
<description> 6 Pin SMD Male Header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X06-1MM" urn="urn:adsk.eagle:package:38023/1" type="box" library_version="1">
<description>JST SH Vertical  6-Pin Connector -SMD
Specifications:
Pin count:6
Pin pitch:1mm
Datasheet referenced for footprint

Example device(s):
CONN_06
EM-406
</description>
<packageinstances>
<packageinstance name="1X06-1MM"/>
</packageinstances>
</package3d>
<package3d name="1X06_NO_SILK" urn="urn:adsk.eagle:package:38130/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin No Silk Outline
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="1X06_1.27MM" urn="urn:adsk.eagle:package:38131/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin
Specifications:
Pin count:6
Pin pitch:1.27mm

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_1.27MM"/>
</packageinstances>
</package3d>
<package3d name="1X05" urn="urn:adsk.eagle:package:38104/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05"/>
</packageinstances>
</package3d>
<package3d name="1X05_1.27MM" urn="urn:adsk.eagle:package:38110/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin
Specifications:
Pin count:5
Pin pitch: 1.27mm

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_1.27MM"/>
</packageinstances>
</package3d>
<package3d name="1X05_LOCK" urn="urn:adsk.eagle:package:38105/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin with Locking Footprint
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X05_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38107/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin Long Pad with Locking Footprint
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X05_LONGPADS" urn="urn:adsk.eagle:package:38109/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin Long Pads
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X05_1MM" urn="urn:adsk.eagle:package:38026/1" type="box" library_version="1">
<description>SMD - 5 Pin
Specifications:
Pin count:5
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_05
EM-408
</description>
<packageinstances>
<packageinstance name="1X05_1MM"/>
</packageinstances>
</package3d>
<package3d name="1X05_1MM_RA" urn="urn:adsk.eagle:package:38106/1" type="box" library_version="1">
<description>SMD - 5 Pin Right Angle
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_1MM_RA"/>
</packageinstances>
</package3d>
<package3d name="1X05_NO_SILK" urn="urn:adsk.eagle:package:38108/1" type="box" library_version="1">
<description>Plated Through Hole - 5 Pin No Silk Outline
Specifications:
Pin count:5
Pin pitch:0.1"

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="1X05_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="JST-5-PTH" urn="urn:adsk.eagle:package:38120/1" type="box" library_version="1">
<description>JST 5 Pin Right Angle Plated Through Hole
Specifications:
Pin count: 5
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="JST-5-PTH"/>
</packageinstances>
</package3d>
<package3d name="JST-5-PTH-VERT" urn="urn:adsk.eagle:package:38111/1" type="box" library_version="1">
<description>JST 5 Pin Vertical Plated Through Hole
Specifications:
Pin count: 5
Pin pitch: 2mm

Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="JST-5-PTH-VERT"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-5" urn="urn:adsk.eagle:package:38112/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -5 Pin PTH
Specifications:
Pin count: 5
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_05
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-5"/>
</packageinstances>
</package3d>
<package3d name="1X03" urn="urn:adsk.eagle:package:38063/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X3" urn="urn:adsk.eagle:package:38064/1" type="box" library_version="1">
<description>PTH - 3 Pin Vertical Molex Polarized Header
Datasheet referenced for footprint: 4UCONN part # 01932 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="MOLEX-1X3"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-3" urn="urn:adsk.eagle:package:38072/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -3 Pin PTH
Specifications:
Pin count: 3
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-3"/>
</packageinstances>
</package3d>
<package3d name="1X03_LOCK" urn="urn:adsk.eagle:package:38071/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin Locking Footprint
Pins are staggered 0.005" off center to lock pins while soldering. 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X03_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38065/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin Long Pad w/ Locking Footprint
Holes are offset 0.005" from center to lock pins in place while soldering. 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X3_LOCK" urn="urn:adsk.eagle:package:38067/1" type="box" library_version="1">
<description>PTH - 3 Pin Vertical Molex Polarized Header
Pins are offset 0.005" from center to lock pins in place during soldering. 
Datasheet referenced for footprint: 4UCONN part # 01932 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="MOLEX-1X3_LOCK"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-3_LOCK.007S" urn="urn:adsk.eagle:package:38066/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -3 Pin PTH Locking
Holes are offset 0.007" from center to hold pins in place during soldering. 
Specifications:
Pin count: 3
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-3_LOCK.007S"/>
</packageinstances>
</package3d>
<package3d name="1X03_NO_SILK" urn="urn:adsk.eagle:package:38076/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin No Silk Outline
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="1X03_LONGPADS" urn="urn:adsk.eagle:package:38068/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin Long Pads
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="JST-3-PTH" urn="urn:adsk.eagle:package:38069/1" type="box" library_version="1">
<description>JST 3 Pin Right Angle Plated Through Hole
Specifications:
Pin count:3
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="JST-3-PTH"/>
</packageinstances>
</package3d>
<package3d name="1X03_PP_HOLES_ONLY" urn="urn:adsk.eagle:package:38073/1" type="box" library_version="1">
<description>Pogo Pins - 3 Pin
Specifications:
Pin count:3

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_PP_HOLES_ONLY"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-5MM-3" urn="urn:adsk.eagle:package:38070/1" type="box" library_version="1">
<description>Screw Terminal  5mm Pitch -3 Pin PTH
Specifications:
Pin count: 3
Pin pitch: 5mm/197mil

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-5MM-3"/>
</packageinstances>
</package3d>
<package3d name="1X03_LOCK_NO_SILK" urn="urn:adsk.eagle:package:38074/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin Locking Footprint w/out Silk Outline
Holes are offset from center 0.005" to lock pins in place while soldering. 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_LOCK_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="JST-3-SMD" urn="urn:adsk.eagle:package:38075/1" type="box" library_version="1">
<description>JST 3 Pin Right Angle SMT
Specifications:
Pin count:3
Pin pitch:2mm

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="JST-3-SMD"/>
</packageinstances>
</package3d>
<package3d name="1X03-1MM-RA" urn="urn:adsk.eagle:package:38077/1" type="box" library_version="1">
<description>Plated Through Hole - 3 Pin SMD
Specifications:
Pin count:3

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03-1MM-RA"/>
</packageinstances>
</package3d>
<package3d name="1X03_SMD_RA_FEMALE" urn="urn:adsk.eagle:package:38081/1" type="box" library_version="1">
<description>SMD - 3 Pin Right Angle Female Header
Silk outline of pin location
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_SMD_RA_FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X03_SMD_RA_MALE" urn="urn:adsk.eagle:package:38078/1" type="box" library_version="1">
<description>SMD- 3 Pin Right Angle Male Headers
No silk outline, but tDocu layer shows pin location. 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_SMD_RA_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X03_SMD_RA_MALE_POST" urn="urn:adsk.eagle:package:38079/1" type="box" library_version="1">
<description>SMD - 3 Pin Right Angle Male Header w/ Alignment Posts
Datasheet referenced for footprint: 4UCONN part # 11026 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_SMD_RA_MALE_POST"/>
</packageinstances>
</package3d>
<package3d name="JST-3-PTH-VERT" urn="urn:adsk.eagle:package:38080/1" type="box" library_version="1">
<description>JST 3 Pin Vertical Plated Through Hole
Specifications:
Pin count:3
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="JST-3-PTH-VERT"/>
</packageinstances>
</package3d>
<package3d name="1X03_SMD_RA_MALE_POST_SMALLER" urn="urn:adsk.eagle:package:38082/1" type="box" library_version="1">
<description>SMD - 3 Pin Right Angle Male Header w/ Alignment Posts
Datasheet referenced for footprint: 4UCONN part # 11026 
Specifications:
Pin count:3
Pin pitch:0.1"

Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="1X03_SMD_RA_MALE_POST_SMALLER"/>
</packageinstances>
</package3d>
<package3d name="1X03_SMD_RA_MALE_POST_SMALLEST" urn="urn:adsk.eagle:package:38083/1" type="box" library_version="1">
<packageinstances>
<packageinstance name="1X03_SMD_RA_MALE_POST_SMALLEST"/>
</packageinstances>
</package3d>
<package3d name="JST-3-PTH-NS" urn="urn:adsk.eagle:package:38084/1" type="box" library_version="1">
<description>JST 3 Pin Right Angle Plated Through Hole &amp;ndash; NO SILK
No silkscreen outline. tDoc layer (51) indicates connector footprint.
Specifications:
Pin count:3
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="JST-3-PTH-NS"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-3-NS" urn="urn:adsk.eagle:package:38088/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -3 Pin PTH &amp;ndash; NO SILK
No silkscreen outline. tDoc layer (51) indicates connector footprint.
Specifications:
Pin count: 3
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_03
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-3-NS"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="CONN_02" urn="urn:adsk.eagle:symbol:37653/1" library_version="1">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<wire x1="3.81" y1="-2.54" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="1.27" y1="2.54" x2="2.54" y2="2.54" width="0.6096" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.6096" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="3.81" y1="-2.54" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<text x="-2.54" y="-4.826" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-2.54" y="5.588" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
<symbol name="CONN_06" urn="urn:adsk.eagle:symbol:37638/1" library_version="1">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;</description>
<wire x1="1.27" y1="-7.62" x2="-5.08" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="0" x2="0" y2="0" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="-2.54" x2="0" y2="-2.54" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="-5.08" x2="0" y2="-5.08" width="0.6096" layer="94"/>
<wire x1="-5.08" y1="10.16" x2="-5.08" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="1.27" y1="-7.62" x2="1.27" y2="10.16" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="10.16" x2="1.27" y2="10.16" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="5.08" x2="0" y2="5.08" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="2.54" x2="0" y2="2.54" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="7.62" x2="0" y2="7.62" width="0.6096" layer="94"/>
<text x="-5.08" y="-9.906" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-5.08" y="10.668" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="5.08" y="-5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="5.08" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="3" x="5.08" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="4" x="5.08" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="5" x="5.08" y="5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="6" x="5.08" y="7.62" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
<symbol name="CONN_05" urn="urn:adsk.eagle:symbol:37721/1" library_version="1">
<description>&lt;h3&gt;5 Pin Connection&lt;/h3&gt;</description>
<wire x1="3.81" y1="-7.62" x2="-2.54" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.6096" layer="94"/>
<wire x1="1.27" y1="-2.54" x2="2.54" y2="-2.54" width="0.6096" layer="94"/>
<wire x1="1.27" y1="-5.08" x2="2.54" y2="-5.08" width="0.6096" layer="94"/>
<wire x1="-2.54" y1="7.62" x2="-2.54" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="3.81" y1="-7.62" x2="3.81" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-2.54" y1="7.62" x2="3.81" y2="7.62" width="0.4064" layer="94"/>
<wire x1="1.27" y1="5.08" x2="2.54" y2="5.08" width="0.6096" layer="94"/>
<wire x1="1.27" y1="2.54" x2="2.54" y2="2.54" width="0.6096" layer="94"/>
<text x="-2.54" y="-9.906" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-2.54" y="8.128" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="7.62" y="-5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="3" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="4" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="5" x="7.62" y="5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
<symbol name="CONN_03" urn="urn:adsk.eagle:symbol:37677/1" library_version="1">
<description>&lt;h3&gt;3 Pin Connection&lt;/h3&gt;</description>
<wire x1="3.81" y1="-5.08" x2="-2.54" y2="-5.08" width="0.4064" layer="94"/>
<wire x1="1.27" y1="2.54" x2="2.54" y2="2.54" width="0.6096" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.6096" layer="94"/>
<wire x1="1.27" y1="-2.54" x2="2.54" y2="-2.54" width="0.6096" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="-5.08" width="0.4064" layer="94"/>
<wire x1="3.81" y1="-5.08" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<text x="-2.54" y="-7.366" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-2.54" y="5.588" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="7.62" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="3" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CONN_02" urn="urn:adsk.eagle:component:38323/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="CONN_02" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38039/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38040/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38050/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38042/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38043/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38052/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38044/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08432" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38045/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38046/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38047/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38049/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38048/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38051/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38053/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863" constant="no"/>
<attribute name="SKU" value="PRT-09914" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38054/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38058/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38055/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38056/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38057/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38061/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38059/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_POKEHOME" package="1X02_POKEHOME">
<connects>
<connect gate="G$1" pin="1" pad="P1 P3"/>
<connect gate="G$1" pin="2" pad="P2 P4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38060/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
</technology>
</technologies>
</device>
<device name="PTH_RA_FEMALE" package="1X02_RA_PTH_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38062/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13700"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06" urn="urn:adsk.eagle:component:38332/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9280"&gt; Arduino Stackable Header - 6 Pin&lt;/a&gt; (PRT-09280)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06" x="-2.54" y="0"/>
</gates>
<devices>
<device name="SILK_FEMALE_PTH" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38009/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38117/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38118/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38004/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08971" constant="no"/>
<attribute name="VALUE" value="RA 6Pin SMD" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38002/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38121/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38123/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX_1X6_RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:37992/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38124/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:37991/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38122/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38125/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09668"/>
</technology>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X06_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38126/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-FEMALE" package="1X06_SMD_STRAIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38139/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT-FEMALE" package="1X06_SMD_STRAIGHT_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38141/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-COMBO-FEMALE" package="1X06_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38127/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD_MALE" package="1X06_SMD_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38128/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11293"/>
</technology>
</technologies>
</device>
<device name="SMD-1MM" package="1X06-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38023/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08249" constant="no"/>
<attribute name="SF_ID" value="GPS-00579" constant="no"/>
</technology>
</technologies>
</device>
<device name="NO_SILK_FEMALE_PTH" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38130/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="1.27MM" package="1X06_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38131/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK_NO_POP" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38130/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_05" urn="urn:adsk.eagle:component:38330/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="G$1" symbol="CONN_05" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38104/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38110/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X05_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38105/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X05_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38107/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X05_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38109/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X05_1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38026/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08528" constant="no"/>
<attribute name="SF_ID" value="GPS-08288" constant="no"/>
</technology>
</technologies>
</device>
<device name="SMD2" package="1X05_1MM_RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38106/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X05_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38108/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST" package="JST-5-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38120/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09917" constant="no"/>
</technology>
</technologies>
</device>
<device name="JST-VERT" package="JST-5-PTH-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38111/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38112/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="Combine 8288+8399" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_03" urn="urn:adsk.eagle:component:38324/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13875"&gt; Stackable Header - 3 Pin (Female, 0.1")&lt;/a&gt; (PRT-13875)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="J$1" symbol="CONN_03" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38063/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38064/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08625" constant="no"/>
<attribute name="SF_ID" value="PRT-08096" constant="no"/>
</technology>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38072/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08288" constant="no"/>
<attribute name="SF_ID" value="PRT-08235" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38071/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38065/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38067/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08625" constant="no"/>
<attribute name="SF_ID" value="PRT-08096" constant="no"/>
</technology>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38066/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08288" constant="no"/>
<attribute name="SF_ID" value="PRT-08235" constant="no"/>
</technology>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38076/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X03_LONGPADS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38068/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-3-PTH">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38069/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WIRE-10037" constant="no"/>
<attribute name="SF_ID" value="PRT-09915" constant="no"/>
</technology>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X03_PP_HOLES_ONLY">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38073/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCREW-5MM" package="SCREWTERMINAL-5MM-3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38070/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10134" constant="no"/>
<attribute name="SF_SKU" value="PRT-08433" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38074/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SMD" package="JST-3-SMD">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38075/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12591" constant="no"/>
<attribute name="VALUE" value="3-PIN SMD" constant="no"/>
</technology>
</technologies>
</device>
<device name="SMD" package="1X03-1MM-RA">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38077/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_RA_FEMALE" package="1X03_SMD_RA_FEMALE">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38081/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10926"/>
<attribute name="VALUE" value="1x3 RA Female .1&quot;"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_MALE" package="1X03_SMD_RA_MALE">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38078/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10925"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_MALE_POST" package="1X03_SMD_RA_MALE_POST">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38079/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-3-PTH-VERT">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38080/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13230" constant="no"/>
</technology>
</technologies>
</device>
<device name="1X03_SMD_RA_MALE_POST_SMALLER" package="1X03_SMD_RA_MALE_POST_SMALLER">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38082/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11912" constant="no"/>
</technology>
</technologies>
</device>
<device name="1X03_SMD_RA_MALE_POST_SMALLEST" package="1X03_SMD_RA_MALE_POST_SMALLEST">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38083/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-NS" package="JST-3-PTH-NS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38084/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW-NS" package="SCREWTERMINAL-3.5MM-3-NS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38088/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Capacitor" urn="urn:adsk.eagle:library:16290819">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC1005X60" urn="urn:adsk.eagle:footprint:16290849/2" library_version="4">
<description>Chip, 1.00 X 0.50 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.60 mm&lt;/p&gt;</description>
<wire x1="0.55" y1="0.6286" x2="-0.55" y2="0.6286" width="0.127" layer="21"/>
<wire x1="0.55" y1="-0.6286" x2="-0.55" y2="-0.6286" width="0.127" layer="21"/>
<wire x1="0.55" y1="-0.3" x2="-0.55" y2="-0.3" width="0.12" layer="51"/>
<wire x1="-0.55" y1="-0.3" x2="-0.55" y2="0.3" width="0.12" layer="51"/>
<wire x1="-0.55" y1="0.3" x2="0.55" y2="0.3" width="0.12" layer="51"/>
<wire x1="0.55" y1="0.3" x2="0.55" y2="-0.3" width="0.12" layer="51"/>
<smd name="1" x="-0.4846" y="0" dx="0.56" dy="0.6291" layer="1"/>
<smd name="2" x="0.4846" y="0" dx="0.56" dy="0.6291" layer="1"/>
<text x="0" y="1.2636" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.2636" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC1110X102" urn="urn:adsk.eagle:footprint:16290845/2" library_version="4">
<description>Chip, 1.17 X 1.02 X 1.02 mm body
&lt;p&gt;Chip package with body size 1.17 X 1.02 X 1.02 mm&lt;/p&gt;</description>
<wire x1="0.66" y1="0.9552" x2="-0.66" y2="0.9552" width="0.127" layer="21"/>
<wire x1="0.66" y1="-0.9552" x2="-0.66" y2="-0.9552" width="0.127" layer="21"/>
<wire x1="0.66" y1="-0.635" x2="-0.66" y2="-0.635" width="0.12" layer="51"/>
<wire x1="-0.66" y1="-0.635" x2="-0.66" y2="0.635" width="0.12" layer="51"/>
<wire x1="-0.66" y1="0.635" x2="0.66" y2="0.635" width="0.12" layer="51"/>
<wire x1="0.66" y1="0.635" x2="0.66" y2="-0.635" width="0.12" layer="51"/>
<smd name="1" x="-0.5388" y="0" dx="0.6626" dy="1.2823" layer="1"/>
<smd name="2" x="0.5388" y="0" dx="0.6626" dy="1.2823" layer="1"/>
<text x="0" y="1.5902" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.5902" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC1608X85" urn="urn:adsk.eagle:footprint:16290847/2" library_version="4">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
<wire x1="0.875" y1="0.7991" x2="-0.875" y2="0.7991" width="0.127" layer="21"/>
<wire x1="0.875" y1="-0.7991" x2="-0.875" y2="-0.7991" width="0.127" layer="21"/>
<wire x1="0.875" y1="-0.475" x2="-0.875" y2="-0.475" width="0.12" layer="51"/>
<wire x1="-0.875" y1="-0.475" x2="-0.875" y2="0.475" width="0.12" layer="51"/>
<wire x1="-0.875" y1="0.475" x2="0.875" y2="0.475" width="0.12" layer="51"/>
<wire x1="0.875" y1="0.475" x2="0.875" y2="-0.475" width="0.12" layer="51"/>
<smd name="1" x="-0.7746" y="0" dx="0.9209" dy="0.9702" layer="1"/>
<smd name="2" x="0.7746" y="0" dx="0.9209" dy="0.9702" layer="1"/>
<text x="0" y="1.4341" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.4341" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC2012X110" urn="urn:adsk.eagle:footprint:16290848/2" library_version="4">
<description>Chip, 2.00 X 1.25 X 1.10 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
<wire x1="1.1" y1="1.0467" x2="-1.1" y2="1.0467" width="0.127" layer="21"/>
<wire x1="1.1" y1="-1.0467" x2="-1.1" y2="-1.0467" width="0.127" layer="21"/>
<wire x1="1.1" y1="-0.725" x2="-1.1" y2="-0.725" width="0.12" layer="51"/>
<wire x1="-1.1" y1="-0.725" x2="-1.1" y2="0.725" width="0.12" layer="51"/>
<wire x1="-1.1" y1="0.725" x2="1.1" y2="0.725" width="0.12" layer="51"/>
<wire x1="1.1" y1="0.725" x2="1.1" y2="-0.725" width="0.12" layer="51"/>
<smd name="1" x="-0.8754" y="0" dx="1.1646" dy="1.4653" layer="1"/>
<smd name="2" x="0.8754" y="0" dx="1.1646" dy="1.4653" layer="1"/>
<text x="0" y="1.6817" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.6817" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC3216X135" urn="urn:adsk.eagle:footprint:16290836/2" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="1.2217" x2="-1.7" y2="1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-1.2217" x2="-1.7" y2="-1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<smd name="2" x="1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<text x="0" y="1.8567" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.8567" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC3225X135" urn="urn:adsk.eagle:footprint:16290843/2" library_version="4">
<description>Chip, 3.20 X 2.50 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.50 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="1.6717" x2="-1.7" y2="1.6717" width="0.127" layer="21"/>
<wire x1="1.7" y1="-1.6717" x2="-1.7" y2="-1.6717" width="0.12" layer="21"/>
<wire x1="1.7" y1="-1.35" x2="-1.7" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-1.35" x2="-1.7" y2="1.35" width="0.12" layer="51"/>
<wire x1="-1.7" y1="1.35" x2="1.7" y2="1.35" width="0.12" layer="51"/>
<wire x1="1.7" y1="1.35" x2="1.7" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-1.4754" y="0" dx="1.1646" dy="2.7153" layer="1"/>
<smd name="2" x="1.4754" y="0" dx="1.1646" dy="2.7153" layer="1"/>
<text x="0" y="2.3067" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.3067" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC4532X135" urn="urn:adsk.eagle:footprint:16290841/2" library_version="4">
<description>Chip, 4.50 X 3.20 X 1.35 mm body
&lt;p&gt;Chip package with body size 4.50 X 3.20 X 1.35 mm&lt;/p&gt;</description>
<wire x1="2.4" y1="2.0217" x2="-2.4" y2="2.0217" width="0.127" layer="21"/>
<wire x1="2.4" y1="-2.0217" x2="-2.4" y2="-2.0217" width="0.127" layer="21"/>
<wire x1="2.4" y1="-1.7" x2="-2.4" y2="-1.7" width="0.12" layer="51"/>
<wire x1="-2.4" y1="-1.7" x2="-2.4" y2="1.7" width="0.12" layer="51"/>
<wire x1="-2.4" y1="1.7" x2="2.4" y2="1.7" width="0.12" layer="51"/>
<wire x1="2.4" y1="1.7" x2="2.4" y2="-1.7" width="0.12" layer="51"/>
<smd name="1" x="-2.0565" y="0" dx="1.3973" dy="3.4153" layer="1"/>
<smd name="2" x="2.0565" y="0" dx="1.3973" dy="3.4153" layer="1"/>
<text x="0" y="2.6567" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.6567" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM3216X180" urn="urn:adsk.eagle:footprint:16290835/2" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<wire x1="-1.7" y1="0.9084" x2="1.7" y2="0.9084" width="0.127" layer="21"/>
<wire x1="-1.7" y1="-0.9084" x2="1.7" y2="-0.9084" width="0.127" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<smd name="2" x="1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<text x="0" y="1.5434" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.5434" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM3528X210" urn="urn:adsk.eagle:footprint:16290844/2" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<wire x1="-1.85" y1="1.5" x2="1.85" y2="1.5" width="0.127" layer="21"/>
<wire x1="-1.85" y1="-1.5" x2="1.85" y2="-1.5" width="0.127" layer="21"/>
<wire x1="1.85" y1="-1.5" x2="-1.85" y2="-1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-1.5" x2="-1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="1.5" x2="1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="1.85" y1="1.5" x2="1.85" y2="-1.5" width="0.12" layer="51"/>
<smd name="1" x="-1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<smd name="2" x="1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<text x="0" y="2.135" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.135" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM6032X280" urn="urn:adsk.eagle:footprint:16290839/2" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<wire x1="-3.15" y1="1.75" x2="3.15" y2="1.75" width="0.127" layer="21"/>
<wire x1="-3.15" y1="-1.75" x2="3.15" y2="-1.75" width="0.127" layer="21"/>
<wire x1="3.15" y1="-1.75" x2="-3.15" y2="-1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="-1.75" x2="-3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="1.75" x2="3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="3.15" y1="1.75" x2="3.15" y2="-1.75" width="0.12" layer="51"/>
<smd name="1" x="-2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<smd name="2" x="2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<text x="0" y="2.385" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.385" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM7343X310" urn="urn:adsk.eagle:footprint:16290840/2" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.127" layer="21"/>
<wire x1="-3.8" y1="-2.3" x2="3.8" y2="-2.3" width="0.127" layer="21"/>
<wire x1="3.8" y1="-2.3" x2="-3.8" y2="-2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="-2.3" x2="-3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="3.8" y1="2.3" x2="3.8" y2="-2.3" width="0.12" layer="51"/>
<smd name="1" x="-3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<smd name="2" x="3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<text x="0" y="2.935" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.935" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC4564X110" urn="urn:adsk.eagle:footprint:16290837/2" library_version="4">
<description>Chip, 4.50 X 6.40 X 1.10 mm body
&lt;p&gt;Chip package with body size 4.50 X 6.40 X 1.10 mm&lt;/p&gt;</description>
<wire x1="2.4" y1="3.7179" x2="-2.4" y2="3.7179" width="0.127" layer="21"/>
<wire x1="2.4" y1="-3.7179" x2="-2.4" y2="-3.7179" width="0.127" layer="21"/>
<wire x1="2.4" y1="-3.4" x2="-2.4" y2="-3.4" width="0.12" layer="51"/>
<wire x1="-2.4" y1="-3.4" x2="-2.4" y2="3.4" width="0.12" layer="51"/>
<wire x1="-2.4" y1="3.4" x2="2.4" y2="3.4" width="0.12" layer="51"/>
<wire x1="2.4" y1="3.4" x2="2.4" y2="-3.4" width="0.12" layer="51"/>
<smd name="1" x="-2.0565" y="0" dx="1.3973" dy="6.8078" layer="1"/>
<smd name="2" x="2.0565" y="0" dx="1.3973" dy="6.8078" layer="1"/>
<text x="0" y="4.3529" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.3529" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPRD550W60D1025H1250B" urn="urn:adsk.eagle:footprint:16290829/2" library_version="4">
<description>Radial Non-Polarized Capacitor, 5.50 mm pitch, 10.25 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 10.25 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="5.25" width="0.127" layer="21"/>
<circle x="0" y="0" radius="5.25" width="0.12" layer="51"/>
<pad name="1" x="-2.75" y="0" drill="0.8" diameter="1.4"/>
<pad name="2" x="2.75" y="0" drill="0.8" diameter="1.4"/>
<text x="0" y="5.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPRD2261W240D5080H5555B" urn="urn:adsk.eagle:footprint:16290850/2" library_version="4">
<description>Radial Non-Polarized Capacitor, 22.61 mm pitch, 50.80 mm body diameter, 55.55 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 22.61 mm pitch (lead spacing), 2.40 mm lead diameter, 50.80 mm body diameter and 55.55 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="25.79" width="0.127" layer="21"/>
<circle x="0" y="0" radius="25.79" width="0.12" layer="51"/>
<pad name="1" x="-11.305" y="0" drill="2.6" diameter="3.9"/>
<pad name="2" x="11.305" y="0" drill="2.6" diameter="3.9"/>
<text x="0" y="26.425" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-26.425" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="CAPC1005X60" urn="urn:adsk.eagle:package:16290895/2" type="model" library_version="4">
<description>Chip, 1.00 X 0.50 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.60 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1005X60"/>
</packageinstances>
</package3d>
<package3d name="CAPC1110X102" urn="urn:adsk.eagle:package:16290904/2" type="model" library_version="4">
<description>Chip, 1.17 X 1.02 X 1.02 mm body
&lt;p&gt;Chip package with body size 1.17 X 1.02 X 1.02 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1110X102"/>
</packageinstances>
</package3d>
<package3d name="CAPC1608X85" urn="urn:adsk.eagle:package:16290898/2" type="model" library_version="4">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1608X85"/>
</packageinstances>
</package3d>
<package3d name="CAPC2012X110" urn="urn:adsk.eagle:package:16290897/2" type="model" library_version="4">
<description>Chip, 2.00 X 1.25 X 1.10 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC2012X110"/>
</packageinstances>
</package3d>
<package3d name="CAPC3216X135" urn="urn:adsk.eagle:package:16290893/2" type="model" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC3216X135"/>
</packageinstances>
</package3d>
<package3d name="CAPC3225X135" urn="urn:adsk.eagle:package:16290903/2" type="model" library_version="4">
<description>Chip, 3.20 X 2.50 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.50 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC3225X135"/>
</packageinstances>
</package3d>
<package3d name="CAPC4532X135" urn="urn:adsk.eagle:package:16290900/2" type="model" library_version="4">
<description>Chip, 4.50 X 3.20 X 1.35 mm body
&lt;p&gt;Chip package with body size 4.50 X 3.20 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC4532X135"/>
</packageinstances>
</package3d>
<package3d name="CAPM3216X180" urn="urn:adsk.eagle:package:16290894/2" type="model" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM3216X180"/>
</packageinstances>
</package3d>
<package3d name="CAPM3528X210" urn="urn:adsk.eagle:package:16290902/2" type="model" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM3528X210"/>
</packageinstances>
</package3d>
<package3d name="CAPM6032X280" urn="urn:adsk.eagle:package:16290896/2" type="model" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM6032X280"/>
</packageinstances>
</package3d>
<package3d name="CAPM7343X310" urn="urn:adsk.eagle:package:16290891/2" type="model" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM7343X310"/>
</packageinstances>
</package3d>
<package3d name="CAPC4564X110L" urn="urn:adsk.eagle:package:16290887/3" type="model" library_version="4">
<description>Chip, 4.50 X 6.40 X 1.10 mm body
&lt;p&gt;Chip package with body size 4.50 X 6.40 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC4564X110"/>
</packageinstances>
</package3d>
<package3d name="CAPRD550W60D1025H1250B" urn="urn:adsk.eagle:package:16290858/2" type="model" library_version="4">
<description>Radial Non-Polarized Capacitor, 5.50 mm pitch, 10.25 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 10.25 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPRD550W60D1025H1250B"/>
</packageinstances>
</package3d>
<package3d name="CAPRD2261W240D5080H5555B" urn="urn:adsk.eagle:package:16290864/2" type="model" library_version="4">
<description>Radial Non-Polarized Capacitor, 22.61 mm pitch, 50.80 mm body diameter, 55.55 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 22.61 mm pitch (lead spacing), 2.40 mm lead diameter, 50.80 mm body diameter and 55.55 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPRD2261W240D5080H5555B"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="C" urn="urn:adsk.eagle:symbol:16290820/1" library_version="4">
<description>Capacitor</description>
<rectangle x1="-2.032" y1="-2.032" x2="2.032" y2="-1.524" layer="94"/>
<rectangle x1="-2.032" y1="-1.016" x2="2.032" y2="-0.508" layer="94"/>
<wire x1="0" y1="0" x2="0" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="0" y1="-2.54" x2="0" y2="-2.032" width="0.1524" layer="94"/>
<pin name="1" x="0" y="2.54" visible="off" length="short" direction="pas" swaplevel="1" rot="R270"/>
<pin name="2" x="0" y="-5.08" visible="off" length="short" direction="pas" swaplevel="1" rot="R90"/>
<text x="2.54" y="2.54" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-2.54" size="1.778" layer="97">&gt;SPICEMODEL</text>
<text x="2.54" y="0" size="1.778" layer="96">&gt;VALUE</text>
<text x="2.54" y="-5.08" size="1.778" layer="97">&gt;SPICEEXTRA</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="C" urn="urn:adsk.eagle:component:16290909/4" prefix="C" uservalue="yes" library_version="4">
<description>&lt;B&gt;Capacitor - Generic</description>
<gates>
<gate name="G$1" symbol="C" x="0" y="0"/>
</gates>
<devices>
<device name="CHIP-0402(1005-METRIC)" package="CAPC1005X60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290895/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0504(1310-METRIC)" package="CAPC1110X102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290904/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0603(1608-METRIC)" package="CAPC1608X85">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290898/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0805(2012-METRIC)" package="CAPC2012X110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290897/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1206(3216-METRIC)" package="CAPC3216X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290893/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1210(3225-METRIC)" package="CAPC3225X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290903/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1812(4532-METRIC)" package="CAPC4532X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290900/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-1206(3216-METRIC)" package="CAPM3216X180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290894/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-1411(3528-METRIC)" package="CAPM3528X210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290902/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2412(6032-METRIC)" package="CAPM6032X280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290896/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2917(7343-METRIC)" package="CAPM7343X310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290891/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1825(4564-METRIC)" package="CAPC4564X110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290887/3"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-12.5MM-DIA" package="CAPRD550W60D1025H1250B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290858/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-55.5MM-DIA" package="CAPRD2261W240D5080H5555B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290864/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="C">
<pinmap gate="G$1" pin="1" pinorder="1"/>
<pinmap gate="G$1" pin="2" pinorder="2"/>
</pinmapping>
</spice>
</deviceset>
</devicesets>
</library>
<library name="Diode" urn="urn:adsk.eagle:library:16378169">
<description>&lt;B&gt;PN Junction, BridgeRectifier, Zener, Schottky, Switching</description>
<packages>
<package name="DIOMELF3516" urn="urn:adsk.eagle:footprint:16378178/1" library_version="6">
<description>MELF, 3.50 mm length, 1.65 mm diameter
&lt;p&gt;MELF Diode package with 3.50 mm length and 1.65 mm diameter&lt;/p&gt;</description>
<wire x1="0.983" y1="1.239" x2="-2.5717" y2="1.239" width="0.12" layer="21"/>
<wire x1="-2.5717" y1="1.239" x2="-2.5717" y2="-1.239" width="0.12" layer="21"/>
<wire x1="-2.5717" y1="-1.239" x2="0.983" y2="-1.239" width="0.12" layer="21"/>
<wire x1="1.85" y1="-0.85" x2="-1.85" y2="-0.85" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-0.85" x2="-1.85" y2="0.85" width="0.12" layer="51"/>
<wire x1="-1.85" y1="0.85" x2="1.85" y2="0.85" width="0.12" layer="51"/>
<wire x1="1.85" y1="0.85" x2="1.85" y2="-0.85" width="0.12" layer="51"/>
<smd name="1" x="-1.6203" y="0" dx="1.2747" dy="1.85" layer="1"/>
<smd name="2" x="1.6203" y="0" dx="1.2747" dy="1.85" layer="1"/>
<text x="0" y="1.874" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.874" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIOMELF5024" urn="urn:adsk.eagle:footprint:16378176/1" library_version="6">
<description>MELF, 5.00 mm length, 2.49 mm diameter
&lt;p&gt;MELF Diode package with 5.00 mm length and 2.49 mm diameter&lt;/p&gt;</description>
<wire x1="1.8515" y1="1.659" x2="-3.3217" y2="1.659" width="0.12" layer="21"/>
<wire x1="-3.3217" y1="1.659" x2="-3.3217" y2="-1.659" width="0.12" layer="21"/>
<wire x1="-3.3217" y1="-1.659" x2="1.8515" y2="-1.659" width="0.12" layer="21"/>
<wire x1="2.6" y1="-1.27" x2="-2.6" y2="-1.27" width="0.12" layer="51"/>
<wire x1="-2.6" y1="-1.27" x2="-2.6" y2="1.27" width="0.12" layer="51"/>
<wire x1="-2.6" y1="1.27" x2="2.6" y2="1.27" width="0.12" layer="51"/>
<wire x1="2.6" y1="1.27" x2="2.6" y2="-1.27" width="0.12" layer="51"/>
<smd name="1" x="-2.4296" y="0" dx="1.1561" dy="2.69" layer="1"/>
<smd name="2" x="2.4296" y="0" dx="1.1561" dy="2.69" layer="1"/>
<text x="0" y="2.294" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.294" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOD3715X135" urn="urn:adsk.eagle:footprint:9427064/1" library_version="6">
<description>SOD, 3.70 mm span, 2.70 X 1.55 X 1.35 mm body
&lt;p&gt;SOD package with 3.70 mm span with body size 2.70 X 1.55 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.425" y1="0.85" x2="-2.5991" y2="0.85" width="0.12" layer="21"/>
<wire x1="-2.5991" y1="0.85" x2="-2.5991" y2="-0.85" width="0.12" layer="21"/>
<wire x1="-2.5991" y1="-0.85" x2="1.425" y2="-0.85" width="0.12" layer="21"/>
<wire x1="1.425" y1="-0.85" x2="-1.425" y2="-0.85" width="0.12" layer="51"/>
<wire x1="-1.425" y1="-0.85" x2="-1.425" y2="0.85" width="0.12" layer="51"/>
<wire x1="-1.425" y1="0.85" x2="1.425" y2="0.85" width="0.12" layer="51"/>
<wire x1="1.425" y1="0.85" x2="1.425" y2="-0.85" width="0.12" layer="51"/>
<smd name="1" x="-1.7215" y="0" dx="1.1272" dy="0.7839" layer="1"/>
<smd name="2" x="1.7215" y="0" dx="1.1272" dy="0.7839" layer="1"/>
<text x="0" y="1.485" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.485" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOD6126X290" urn="urn:adsk.eagle:footprint:9427065/1" library_version="6">
<description>SOD, 6.10 mm span, 4.33 X 2.60 X 2.90 mm body
&lt;p&gt;SOD package with 6.10 mm span with body size 4.33 X 2.60 X 2.90 mm&lt;/p&gt;</description>
<wire x1="2.3" y1="1.475" x2="-3.9179" y2="1.475" width="0.12" layer="21"/>
<wire x1="-3.9179" y1="1.475" x2="-3.9179" y2="-1.475" width="0.12" layer="21"/>
<wire x1="-3.9179" y1="-1.475" x2="2.3" y2="-1.475" width="0.12" layer="21"/>
<wire x1="2.3" y1="-1.475" x2="-2.3" y2="-1.475" width="0.12" layer="51"/>
<wire x1="-2.3" y1="-1.475" x2="-2.3" y2="1.475" width="0.12" layer="51"/>
<wire x1="-2.3" y1="1.475" x2="2.3" y2="1.475" width="0.12" layer="51"/>
<wire x1="2.3" y1="1.475" x2="2.3" y2="-1.475" width="0.12" layer="51"/>
<smd name="1" x="-2.7048" y="0" dx="1.7981" dy="1.7253" layer="1"/>
<smd name="2" x="2.7048" y="0" dx="1.7981" dy="1.7253" layer="1"/>
<text x="0" y="2.11" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.11" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOD6126X350" urn="urn:adsk.eagle:footprint:9933385/1" library_version="6">
<description>SOD, 6.10 mm span, 4.20 X 2.65 X 3.50 mm body
&lt;p&gt;SOD package with 6.10 mm span with body size 4.20 X 2.65 X 3.50 mm&lt;/p&gt;</description>
<wire x1="2.225" y1="1.65" x2="-3.9179" y2="1.65" width="0.12" layer="21"/>
<wire x1="-3.9179" y1="1.65" x2="-3.9179" y2="-1.65" width="0.12" layer="21"/>
<wire x1="-3.9179" y1="-1.65" x2="2.225" y2="-1.65" width="0.12" layer="21"/>
<wire x1="2.225" y1="-1.65" x2="-2.225" y2="-1.65" width="0.12" layer="51"/>
<wire x1="-2.225" y1="-1.65" x2="-2.225" y2="1.65" width="0.12" layer="51"/>
<wire x1="-2.225" y1="1.65" x2="2.225" y2="1.65" width="0.12" layer="51"/>
<wire x1="2.225" y1="1.65" x2="2.225" y2="-1.65" width="0.12" layer="51"/>
<smd name="1" x="-2.7048" y="0" dx="1.7981" dy="1.7689" layer="1"/>
<smd name="2" x="2.7048" y="0" dx="1.7981" dy="1.7689" layer="1"/>
<text x="0" y="2.285" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.285" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOD6236X265" urn="urn:adsk.eagle:footprint:9427053/1" library_version="6">
<description>SOD, 6.22 mm span, 4.33 X 3.63 X 2.65 mm body
&lt;p&gt;SOD package with 6.22 mm span with body size 4.33 X 3.63 X 2.65 mm&lt;/p&gt;</description>
<wire x1="2.3" y1="1.975" x2="-3.9196" y2="1.975" width="0.12" layer="21"/>
<wire x1="-3.9196" y1="1.975" x2="-3.9196" y2="-1.975" width="0.12" layer="21"/>
<wire x1="-3.9196" y1="-1.975" x2="2.3" y2="-1.975" width="0.12" layer="21"/>
<wire x1="2.3" y1="-1.975" x2="-2.3" y2="-1.975" width="0.12" layer="51"/>
<wire x1="-2.3" y1="-1.975" x2="-2.3" y2="1.975" width="0.12" layer="51"/>
<wire x1="-2.3" y1="1.975" x2="2.3" y2="1.975" width="0.12" layer="51"/>
<wire x1="2.3" y1="1.975" x2="2.3" y2="-1.975" width="0.12" layer="51"/>
<smd name="1" x="-2.7561" y="0" dx="1.699" dy="2.2839" layer="1"/>
<smd name="2" x="2.7561" y="0" dx="1.699" dy="2.2839" layer="1"/>
<text x="0" y="2.61" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.61" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SOD9959X265" urn="urn:adsk.eagle:footprint:9427066/1" library_version="6">
<description>SOD, 9.93 mm span, 6.88 X 5.90 X 2.65 mm body
&lt;p&gt;SOD package with 9.93 mm span with body size 6.88 X 5.90 X 2.65 mm&lt;/p&gt;</description>
<wire x1="3.575" y1="3.125" x2="-5.7696" y2="3.125" width="0.12" layer="21"/>
<wire x1="-5.7696" y1="3.125" x2="-5.7696" y2="-3.125" width="0.12" layer="21"/>
<wire x1="-5.7696" y1="-3.125" x2="3.575" y2="-3.125" width="0.12" layer="21"/>
<wire x1="3.575" y1="-3.125" x2="-3.575" y2="-3.125" width="0.12" layer="51"/>
<wire x1="-3.575" y1="-3.125" x2="-3.575" y2="3.125" width="0.12" layer="51"/>
<wire x1="-3.575" y1="3.125" x2="3.575" y2="3.125" width="0.12" layer="51"/>
<wire x1="3.575" y1="3.125" x2="3.575" y2="-3.125" width="0.12" layer="51"/>
<smd name="1" x="-4.5203" y="0" dx="1.8706" dy="3.2802" layer="1"/>
<smd name="2" x="4.5203" y="0" dx="1.8706" dy="3.2802" layer="1"/>
<text x="0" y="3.76" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-3.76" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL2513X70" urn="urn:adsk.eagle:footprint:9427167/1" library_version="6">
<description>SODFL, 2.50 mm span, 1.90 X 1.30 X 0.70 mm body
&lt;p&gt;SODFL package with 2.50 mm span with body size 1.90 X 1.30 X 0.70 mm&lt;/p&gt;</description>
<wire x1="1" y1="0.7009" x2="-1.8717" y2="0.7009" width="0.12" layer="21"/>
<wire x1="-1.8717" y1="0.7009" x2="-1.8717" y2="-0.7009" width="0.12" layer="21"/>
<wire x1="-1.8717" y1="-0.7009" x2="1" y2="-0.7009" width="0.12" layer="21"/>
<wire x1="1" y1="-0.7" x2="-1" y2="-0.7" width="0.12" layer="51"/>
<wire x1="-1" y1="-0.7" x2="-1" y2="0.7" width="0.12" layer="51"/>
<wire x1="-1" y1="0.7" x2="1" y2="0.7" width="0.12" layer="51"/>
<wire x1="1" y1="0.7" x2="1" y2="-0.7" width="0.12" layer="51"/>
<smd name="1" x="-1.065" y="0" dx="0.9854" dy="0.7739" layer="1"/>
<smd name="2" x="1.065" y="0" dx="0.9854" dy="0.7739" layer="1"/>
<text x="0" y="1.3359" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.3359" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL2513X75" urn="urn:adsk.eagle:footprint:9427168/1" library_version="6">
<description>SODFL, 2.50 mm span, 2.20 X 1.30 X 0.75 mm body
&lt;p&gt;SODFL package with 2.50 mm span with body size 2.20 X 1.30 X 0.75 mm&lt;/p&gt;</description>
<wire x1="1.15" y1="0.7009" x2="-1.8717" y2="0.7009" width="0.12" layer="21"/>
<wire x1="-1.8717" y1="0.7009" x2="-1.8717" y2="-0.7009" width="0.12" layer="21"/>
<wire x1="-1.8717" y1="-0.7009" x2="1.15" y2="-0.7009" width="0.12" layer="21"/>
<wire x1="1.15" y1="-0.7" x2="-1.15" y2="-0.7" width="0.12" layer="51"/>
<wire x1="-1.15" y1="-0.7" x2="-1.15" y2="0.7" width="0.12" layer="51"/>
<wire x1="-1.15" y1="0.7" x2="1.15" y2="0.7" width="0.12" layer="51"/>
<wire x1="1.15" y1="0.7" x2="1.15" y2="-0.7" width="0.12" layer="51"/>
<smd name="1" x="-0.7394" y="0" dx="1.6364" dy="1.003" layer="1"/>
<smd name="2" x="0.7394" y="0" dx="1.0027" dy="0.7739" layer="1"/>
<text x="0" y="1.3359" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.3359" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL3718X115" urn="urn:adsk.eagle:footprint:9427170/1" library_version="6">
<description>SODFL, 3.70 mm span, 2.80 X 1.80 X 1.15 mm body
&lt;p&gt;SODFL package with 3.70 mm span with body size 2.80 X 1.80 X 1.15 mm&lt;/p&gt;</description>
<wire x1="1.45" y1="0.9946" x2="-2.4717" y2="0.9946" width="0.12" layer="21"/>
<wire x1="-2.4717" y1="0.9946" x2="-2.4717" y2="-0.9946" width="0.12" layer="21"/>
<wire x1="-2.4717" y1="-0.9946" x2="1.45" y2="-0.9946" width="0.12" layer="21"/>
<wire x1="1.45" y1="-0.95" x2="-1.45" y2="-0.95" width="0.12" layer="51"/>
<wire x1="-1.45" y1="-0.95" x2="-1.45" y2="0.95" width="0.12" layer="51"/>
<wire x1="-1.45" y1="0.95" x2="1.45" y2="0.95" width="0.12" layer="51"/>
<wire x1="1.45" y1="0.95" x2="1.45" y2="-0.95" width="0.12" layer="51"/>
<smd name="1" x="-1.6004" y="0" dx="1.1146" dy="1.3612" layer="1"/>
<smd name="2" x="1.6004" y="0" dx="1.1146" dy="1.3612" layer="1"/>
<text x="0" y="1.6296" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.6296" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL3718X140" urn="urn:adsk.eagle:footprint:9427171/1" library_version="6">
<description>SODFL, 3.70 mm span, 2.80 X 1.80 X 1.40 mm body
&lt;p&gt;SODFL package with 3.70 mm span with body size 2.80 X 1.80 X 1.40 mm&lt;/p&gt;</description>
<wire x1="1.45" y1="0.9946" x2="-2.4717" y2="0.9946" width="0.12" layer="21"/>
<wire x1="-2.4717" y1="0.9946" x2="-2.4717" y2="-0.9946" width="0.12" layer="21"/>
<wire x1="-2.4717" y1="-0.9946" x2="1.45" y2="-0.9946" width="0.12" layer="21"/>
<wire x1="1.45" y1="-0.95" x2="-1.45" y2="-0.95" width="0.12" layer="51"/>
<wire x1="-1.45" y1="-0.95" x2="-1.45" y2="0.95" width="0.12" layer="51"/>
<wire x1="-1.45" y1="0.95" x2="1.45" y2="0.95" width="0.12" layer="51"/>
<wire x1="1.45" y1="0.95" x2="1.45" y2="-0.95" width="0.12" layer="51"/>
<smd name="1" x="-1.5233" y="0" dx="1.2688" dy="1.3612" layer="1"/>
<smd name="2" x="1.5233" y="0" dx="1.2688" dy="1.3612" layer="1"/>
<text x="0" y="1.6296" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.6296" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL5336X110" urn="urn:adsk.eagle:footprint:9427173/1" library_version="6">
<description>SODFL, 5.35 mm span, 4.33 X 3.63 X 1.10 mm body
&lt;p&gt;SODFL package with 5.35 mm span with body size 4.33 X 3.63 X 1.10 mm&lt;/p&gt;</description>
<wire x1="2.3" y1="1.975" x2="-3.3202" y2="1.975" width="0.12" layer="21"/>
<wire x1="-3.3202" y1="1.975" x2="-3.3202" y2="-1.975" width="0.12" layer="21"/>
<wire x1="-3.3202" y1="-1.975" x2="2.3" y2="-1.975" width="0.12" layer="21"/>
<wire x1="2.3" y1="-1.975" x2="-2.3" y2="-1.975" width="0.12" layer="51"/>
<wire x1="-2.3" y1="-1.975" x2="-2.3" y2="1.975" width="0.12" layer="51"/>
<wire x1="-2.3" y1="1.975" x2="2.3" y2="1.975" width="0.12" layer="51"/>
<wire x1="2.3" y1="1.975" x2="2.3" y2="-1.975" width="0.12" layer="51"/>
<smd name="1" x="-2.1302" y="0" dx="1.752" dy="2.2239" layer="1"/>
<smd name="2" x="2.1302" y="0" dx="1.752" dy="2.2239" layer="1"/>
<text x="0" y="2.61" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.61" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL7959X110" urn="urn:adsk.eagle:footprint:9427174/1" library_version="6">
<description>SODFL, 7.95 mm span, 6.88 X 5.90 X 1.10 mm body
&lt;p&gt;SODFL package with 7.95 mm span with body size 6.88 X 5.90 X 1.10 mm&lt;/p&gt;</description>
<wire x1="3.575" y1="3.125" x2="-4.5967" y2="3.125" width="0.12" layer="21"/>
<wire x1="-4.5967" y1="3.125" x2="-4.5967" y2="-3.125" width="0.12" layer="21"/>
<wire x1="-4.5967" y1="-3.125" x2="3.575" y2="-3.125" width="0.12" layer="21"/>
<wire x1="3.575" y1="-3.125" x2="-3.575" y2="-3.125" width="0.12" layer="51"/>
<wire x1="-3.575" y1="-3.125" x2="-3.575" y2="3.125" width="0.12" layer="51"/>
<wire x1="-3.575" y1="3.125" x2="3.575" y2="3.125" width="0.12" layer="51"/>
<wire x1="3.575" y1="3.125" x2="3.575" y2="-3.125" width="0.12" layer="51"/>
<smd name="1" x="-3.4233" y="0" dx="1.7188" dy="3.2202" layer="1"/>
<smd name="2" x="3.4233" y="0" dx="1.7188" dy="3.2202" layer="1"/>
<text x="0" y="3.76" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-3.76" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL5226X110" urn="urn:adsk.eagle:footprint:9427175/1" library_version="6">
<description>SODFL, 5.20 mm span, 4.28 X 2.60 X 1.10 mm body
&lt;p&gt;SODFL package with 5.20 mm span with body size 4.28 X 2.60 X 1.10 mm&lt;/p&gt;</description>
<wire x1="2.3" y1="1.475" x2="-3.3179" y2="1.475" width="0.12" layer="21"/>
<wire x1="-3.3179" y1="1.475" x2="-3.3179" y2="-1.475" width="0.12" layer="21"/>
<wire x1="-3.3179" y1="-1.475" x2="2.3" y2="-1.475" width="0.12" layer="21"/>
<wire x1="2.3" y1="-1.475" x2="-2.3" y2="-1.475" width="0.12" layer="51"/>
<wire x1="-2.3" y1="-1.475" x2="-2.3" y2="1.475" width="0.12" layer="51"/>
<wire x1="-2.3" y1="1.475" x2="2.3" y2="1.475" width="0.12" layer="51"/>
<wire x1="2.3" y1="1.475" x2="2.3" y2="-1.475" width="0.12" layer="51"/>
<smd name="1" x="-2.0722" y="0" dx="1.8634" dy="1.6653" layer="1"/>
<smd name="2" x="2.0722" y="0" dx="1.8634" dy="1.6653" layer="1"/>
<text x="0" y="2.11" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.11" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL4725X110" urn="urn:adsk.eagle:footprint:9427177/1" library_version="6">
<description>SODFL, 4.70 mm span, 3.80 X 2.50 X 1.10 mm body
&lt;p&gt;SODFL package with 4.70 mm span with body size 3.80 X 2.50 X 1.10 mm&lt;/p&gt;</description>
<wire x1="2" y1="1.35" x2="-3.0192" y2="1.35" width="0.12" layer="21"/>
<wire x1="-3.0192" y1="1.35" x2="-3.0192" y2="-1.35" width="0.12" layer="21"/>
<wire x1="-3.0192" y1="-1.35" x2="2" y2="-1.35" width="0.12" layer="21"/>
<wire x1="2" y1="-1.35" x2="-2" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-2" y1="-1.35" x2="-2" y2="1.35" width="0.12" layer="51"/>
<wire x1="-2" y1="1.35" x2="2" y2="1.35" width="0.12" layer="51"/>
<wire x1="2" y1="1.35" x2="2" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-2.11" y="0" dx="1.1904" dy="2.0153" layer="1"/>
<smd name="2" x="2.11" y="0" dx="1.1904" dy="2.0153" layer="1"/>
<text x="0" y="1.985" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.985" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SODFL1608X70" urn="urn:adsk.eagle:footprint:16378177/1" library_version="6">
<description>SODFL, 1.60 mm span, 1.20 X 0.80 X 0.70 mm body
&lt;p&gt;SODFL package with 1.60 mm span with body size 1.20 X 0.80 X 0.70 mm&lt;/p&gt;</description>
<wire x1="0.65" y1="0.514" x2="-1.3786" y2="0.514" width="0.12" layer="21"/>
<wire x1="-1.3786" y1="0.514" x2="-1.3786" y2="-0.514" width="0.12" layer="21"/>
<wire x1="-1.3786" y1="-0.514" x2="0.65" y2="-0.514" width="0.12" layer="21"/>
<wire x1="0.65" y1="-0.45" x2="-0.65" y2="-0.45" width="0.12" layer="51"/>
<wire x1="-0.65" y1="-0.45" x2="-0.65" y2="0.45" width="0.12" layer="51"/>
<wire x1="-0.65" y1="0.45" x2="0.65" y2="0.45" width="0.12" layer="51"/>
<wire x1="0.65" y1="0.45" x2="0.65" y2="-0.45" width="0.12" layer="51"/>
<smd name="1" x="-0.7956" y="0" dx="0.538" dy="0.4" layer="1"/>
<smd name="2" x="0.7956" y="0" dx="0.538" dy="0.4" layer="1"/>
<text x="0" y="1.149" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.149" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIOM5226X290N" urn="urn:adsk.eagle:footprint:16378179/1" library_version="6">
<description>Molded Body, 5.20 X 2.60 X 2.90 mm body
&lt;p&gt;Molded Body package with body size 5.20 X 2.60 X 2.90 mm&lt;/p&gt;</description>
<wire x1="2.8" y1="1.475" x2="-3.6179" y2="1.475" width="0.12" layer="21"/>
<wire x1="-3.6179" y1="1.475" x2="-3.6179" y2="-1.475" width="0.12" layer="21"/>
<wire x1="-3.6179" y1="-1.475" x2="2.8" y2="-1.475" width="0.12" layer="21"/>
<wire x1="2.8" y1="-1.475" x2="-2.8" y2="-1.475" width="0.12" layer="51"/>
<wire x1="-2.8" y1="-1.475" x2="-2.8" y2="1.475" width="0.12" layer="51"/>
<wire x1="-2.8" y1="1.475" x2="2.8" y2="1.475" width="0.12" layer="51"/>
<wire x1="2.8" y1="1.475" x2="2.8" y2="-1.475" width="0.12" layer="51"/>
<smd name="1" x="-2.1079" y="0" dx="2.392" dy="1.5653" layer="1"/>
<smd name="2" x="2.1079" y="0" dx="2.392" dy="1.5653" layer="1"/>
<text x="0" y="2.11" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.11" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIOM5336X265N" urn="urn:adsk.eagle:footprint:16378175/1" library_version="6">
<description>Molded Body, 5.35 X 3.63 X 2.65 mm body
&lt;p&gt;Molded Body package with body size 5.35 X 3.63 X 2.65 mm&lt;/p&gt;</description>
<wire x1="2.8" y1="1.975" x2="-3.6202" y2="1.975" width="0.12" layer="21"/>
<wire x1="-3.6202" y1="1.975" x2="-3.6202" y2="-1.975" width="0.12" layer="21"/>
<wire x1="-3.6202" y1="-1.975" x2="2.8" y2="-1.975" width="0.12" layer="21"/>
<wire x1="2.8" y1="-1.975" x2="-2.8" y2="-1.975" width="0.12" layer="51"/>
<wire x1="-2.8" y1="-1.975" x2="-2.8" y2="1.975" width="0.12" layer="51"/>
<wire x1="-2.8" y1="1.975" x2="2.8" y2="1.975" width="0.12" layer="51"/>
<wire x1="2.8" y1="1.975" x2="2.8" y2="-1.975" width="0.12" layer="51"/>
<smd name="1" x="-2.1641" y="0" dx="2.2841" dy="2.1239" layer="1"/>
<smd name="2" x="2.1641" y="0" dx="2.2841" dy="2.1239" layer="1"/>
<text x="0" y="2.61" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.61" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIOM7959X625N" urn="urn:adsk.eagle:footprint:16378174/1" library_version="6">
<description>Molded Body, 7.95 X 5.90 X 6.25 mm body
&lt;p&gt;Molded Body package with body size 7.95 X 5.90 X 6.25 mm&lt;/p&gt;</description>
<wire x1="4.075" y1="3.125" x2="-4.8967" y2="3.125" width="0.12" layer="21"/>
<wire x1="-4.8967" y1="3.125" x2="-4.8967" y2="-3.125" width="0.12" layer="21"/>
<wire x1="-4.8967" y1="-3.125" x2="4.075" y2="-3.125" width="0.12" layer="21"/>
<wire x1="4.075" y1="-3.125" x2="-4.075" y2="-3.125" width="0.12" layer="51"/>
<wire x1="-4.075" y1="-3.125" x2="-4.075" y2="3.125" width="0.12" layer="51"/>
<wire x1="-4.075" y1="3.125" x2="4.075" y2="3.125" width="0.12" layer="51"/>
<wire x1="4.075" y1="3.125" x2="4.075" y2="-3.125" width="0.12" layer="51"/>
<smd name="1" x="-3.4567" y="0" dx="2.2518" dy="3.1202" layer="1"/>
<smd name="2" x="3.4567" y="0" dx="2.2518" dy="3.1202" layer="1"/>
<text x="0" y="3.76" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-3.76" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DIOMELF3516L" urn="urn:adsk.eagle:package:16378190/2" type="model" library_version="6">
<description>MELF, 3.50 mm length, 1.65 mm diameter
&lt;p&gt;MELF Diode package with 3.50 mm length and 1.65 mm diameter&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOMELF3516"/>
</packageinstances>
</package3d>
<package3d name="DIOMELF5024" urn="urn:adsk.eagle:package:16378191/1" type="model" library_version="6">
<description>MELF, 5.00 mm length, 2.49 mm diameter
&lt;p&gt;MELF Diode package with 5.00 mm length and 2.49 mm diameter&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOMELF5024"/>
</packageinstances>
</package3d>
<package3d name="SOD3715X135" urn="urn:adsk.eagle:package:9427058/2" type="model" library_version="6">
<description>SOD, 3.70 mm span, 2.70 X 1.55 X 1.35 mm body
&lt;p&gt;SOD package with 3.70 mm span with body size 2.70 X 1.55 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOD3715X135"/>
</packageinstances>
</package3d>
<package3d name="SOD6126X290" urn="urn:adsk.eagle:package:9427057/2" type="model" library_version="6">
<description>SOD, 6.10 mm span, 4.33 X 2.60 X 2.90 mm body
&lt;p&gt;SOD package with 6.10 mm span with body size 4.33 X 2.60 X 2.90 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOD6126X290"/>
</packageinstances>
</package3d>
<package3d name="SOD6126X350" urn="urn:adsk.eagle:package:9932483/2" type="model" library_version="6">
<description>SOD, 6.10 mm span, 4.20 X 2.65 X 3.50 mm body
&lt;p&gt;SOD package with 6.10 mm span with body size 4.20 X 2.65 X 3.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOD6126X350"/>
</packageinstances>
</package3d>
<package3d name="SOD6236X265" urn="urn:adsk.eagle:package:9427046/2" type="model" library_version="6">
<description>SOD, 6.22 mm span, 4.33 X 3.63 X 2.65 mm body
&lt;p&gt;SOD package with 6.22 mm span with body size 4.33 X 3.63 X 2.65 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOD6236X265"/>
</packageinstances>
</package3d>
<package3d name="SOD9959X265" urn="urn:adsk.eagle:package:9427056/2" type="model" library_version="6">
<description>SOD, 9.93 mm span, 6.88 X 5.90 X 2.65 mm body
&lt;p&gt;SOD package with 9.93 mm span with body size 6.88 X 5.90 X 2.65 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOD9959X265"/>
</packageinstances>
</package3d>
<package3d name="SODFL2513X70" urn="urn:adsk.eagle:package:9427155/2" type="model" library_version="6">
<description>SODFL, 2.50 mm span, 1.90 X 1.30 X 0.70 mm body
&lt;p&gt;SODFL package with 2.50 mm span with body size 1.90 X 1.30 X 0.70 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL2513X70"/>
</packageinstances>
</package3d>
<package3d name="SODFL2513X75" urn="urn:adsk.eagle:package:9427154/2" type="model" library_version="6">
<description>SODFL, 2.50 mm span, 2.20 X 1.30 X 0.75 mm body
&lt;p&gt;SODFL package with 2.50 mm span with body size 2.20 X 1.30 X 0.75 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL2513X75"/>
</packageinstances>
</package3d>
<package3d name="SODFL3718X115" urn="urn:adsk.eagle:package:9427153/2" type="model" library_version="6">
<description>SODFL, 3.70 mm span, 2.80 X 1.80 X 1.15 mm body
&lt;p&gt;SODFL package with 3.70 mm span with body size 2.80 X 1.80 X 1.15 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL3718X115"/>
</packageinstances>
</package3d>
<package3d name="SODFL3718X140" urn="urn:adsk.eagle:package:9427152/2" type="model" library_version="6">
<description>SODFL, 3.70 mm span, 2.80 X 1.80 X 1.40 mm body
&lt;p&gt;SODFL package with 3.70 mm span with body size 2.80 X 1.80 X 1.40 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL3718X140"/>
</packageinstances>
</package3d>
<package3d name="SODFL5336X110" urn="urn:adsk.eagle:package:9427151/2" type="model" library_version="6">
<description>SODFL, 5.35 mm span, 4.33 X 3.63 X 1.10 mm body
&lt;p&gt;SODFL package with 5.35 mm span with body size 4.33 X 3.63 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL5336X110"/>
</packageinstances>
</package3d>
<package3d name="SODFL7959X110" urn="urn:adsk.eagle:package:9427150/2" type="model" library_version="6">
<description>SODFL, 7.95 mm span, 6.88 X 5.90 X 1.10 mm body
&lt;p&gt;SODFL package with 7.95 mm span with body size 6.88 X 5.90 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL7959X110"/>
</packageinstances>
</package3d>
<package3d name="SODFL5226X110" urn="urn:adsk.eagle:package:9427148/2" type="model" library_version="6">
<description>SODFL, 5.20 mm span, 4.28 X 2.60 X 1.10 mm body
&lt;p&gt;SODFL package with 5.20 mm span with body size 4.28 X 2.60 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL5226X110"/>
</packageinstances>
</package3d>
<package3d name="SODFL4725X110" urn="urn:adsk.eagle:package:9427149/2" type="model" library_version="6">
<description>SODFL, 4.70 mm span, 3.80 X 2.50 X 1.10 mm body
&lt;p&gt;SODFL package with 4.70 mm span with body size 3.80 X 2.50 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL4725X110"/>
</packageinstances>
</package3d>
<package3d name="SODFL1608X70" urn="urn:adsk.eagle:package:16378187/1" type="model" library_version="6">
<description>SODFL, 1.60 mm span, 1.20 X 0.80 X 0.70 mm body
&lt;p&gt;SODFL package with 1.60 mm span with body size 1.20 X 0.80 X 0.70 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SODFL1608X70"/>
</packageinstances>
</package3d>
<package3d name="DIOM5226X290N" urn="urn:adsk.eagle:package:16378188/1" type="model" library_version="6">
<description>Molded Body, 5.20 X 2.60 X 2.90 mm body
&lt;p&gt;Molded Body package with body size 5.20 X 2.60 X 2.90 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM5226X290N"/>
</packageinstances>
</package3d>
<package3d name="DIOM5336X265N" urn="urn:adsk.eagle:package:16378189/1" type="model" library_version="6">
<description>Molded Body, 5.35 X 3.63 X 2.65 mm body
&lt;p&gt;Molded Body package with body size 5.35 X 3.63 X 2.65 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM5336X265N"/>
</packageinstances>
</package3d>
<package3d name="DIOM7959X625N" urn="urn:adsk.eagle:package:16378186/1" type="model" library_version="6">
<description>Molded Body, 7.95 X 5.90 X 6.25 mm body
&lt;p&gt;Molded Body package with body size 7.95 X 5.90 X 6.25 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM7959X625N"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="DIODE" urn="urn:adsk.eagle:symbol:16378170/2" library_version="6">
<description>Diode</description>
<pin name="A" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1"/>
<pin name="C" x="5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1" rot="R180"/>
<text x="0" y="5.08" size="1.778" layer="95" align="center">&gt;NAME</text>
<text x="0" y="-5.08" size="1.778" layer="95" align="center">&gt;VALUE</text>
<text x="0" y="-7.62" size="1.778" layer="95" align="center">&gt;SPICEMODEL</text>
<text x="0" y="-10.16" size="1.778" layer="95" align="center">&gt;SPICEEXTRA</text>
<wire x1="-2.54" y1="-2.54" x2="-2.54" y2="2.54" width="0.254" layer="94"/>
<wire x1="-2.54" y1="2.54" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="-2.54" y2="-2.54" width="0.254" layer="94"/>
<wire x1="2.54" y1="2.54" x2="2.54" y2="-2.54" width="0.254" layer="94"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DIODE" urn="urn:adsk.eagle:component:16378193/4" prefix="D" library_version="6">
<description>&lt;B&gt;Diode Rectifier - Generic</description>
<gates>
<gate name="G$1" symbol="DIODE" x="0" y="0"/>
</gates>
<devices>
<device name="DO-213AA(SOD-80)" package="DIOMELF3516">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378190/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-213AB(5025-METRIC)" package="DIOMELF5024">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378191/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-215-AD" package="SOD3715X135">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427058/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-215-AC" package="SOD6126X290">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427057/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-215-BA" package="SOD6126X350">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9932483/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-215-AA" package="SOD6236X265">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427046/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-215-AB" package="SOD9959X265">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427056/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-219-AC(SOD323F)" package="SODFL2513X70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427155/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-219-AD" package="SODFL2513X75">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427154/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-219-AB(SOD123F)" package="SODFL3718X115">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427153/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-219-AA" package="SODFL3718X140">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427152/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-221-AA" package="SODFL5336X110">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427151/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-221-AB" package="SODFL7959X110">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427150/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-221-AC" package="SODFL5226X110">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427148/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-221-AD" package="SODFL4725X110">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:9427149/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="SODFL(1608-METRIC)" package="SODFL1608X70">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378187/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-214AC(SMA)" package="DIOM5226X290N">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378188/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-214AA(SMB)" package="DIOM5336X265N">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378189/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="DO-214AB(SMC)" package="DIOM7959X625N">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378186/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Diode" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="FORWARD_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="REVERSE_VOLTAGE" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="Rectifier" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="D">
<pinmap gate="G$1" pin="A" pinorder="1"/>
<pinmap gate="G$1" pin="C" pinorder="2"/>
</pinmapping>
<model name="DMOD">
**********************
* Autodesk EAGLE - Spice Model File
* Date: 9/17/17
* basic diode intrinsic model
**********************
.MODEL DMOD D</model>
</spice>
</deviceset>
</devicesets>
</library>
<library name="Transistor" urn="urn:adsk.eagle:library:16378713">
<description>&lt;B&gt;BJT, JFET, MOSFET, UJT, Darlington</description>
<packages>
<package name="SOT23" urn="urn:adsk.eagle:footprint:28669/1" library_version="4">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
<wire x1="1.4224" y1="0.6604" x2="1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="1.4224" y1="-0.6604" x2="-1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="-0.6604" x2="-1.4224" y2="0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="0.6604" x2="1.4224" y2="0.6604" width="0.1524" layer="51"/>
<smd name="3" x="0" y="1.1" dx="1" dy="1.4" layer="1"/>
<smd name="2" x="0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<smd name="1" x="-0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<text x="-1.905" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.2286" y1="0.7112" x2="0.2286" y2="1.2954" layer="51"/>
<rectangle x1="0.7112" y1="-1.2954" x2="1.1684" y2="-0.7112" layer="51"/>
<rectangle x1="-1.1684" y1="-1.2954" x2="-0.7112" y2="-0.7112" layer="51"/>
</package>
<package name="TO92" urn="urn:adsk.eagle:footprint:28459/1" library_version="4">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
<wire x1="-2.0946" y1="-1.651" x2="-2.6549" y2="-0.254" width="0.127" layer="21" curve="-32.781"/>
<wire x1="-2.6549" y1="-0.254" x2="-0.7863" y2="2.5485" width="0.127" layer="21" curve="-78.3185"/>
<wire x1="0.7863" y1="2.5484" x2="2.0945" y2="-1.651" width="0.127" layer="21" curve="-111.1"/>
<wire x1="-2.0945" y1="-1.651" x2="2.0945" y2="-1.651" width="0.127" layer="21"/>
<wire x1="-2.2537" y1="-0.254" x2="-0.2863" y2="-0.254" width="0.127" layer="51"/>
<wire x1="-2.6549" y1="-0.254" x2="-2.2537" y2="-0.254" width="0.127" layer="21"/>
<wire x1="-0.2863" y1="-0.254" x2="0.2863" y2="-0.254" width="0.127" layer="21"/>
<wire x1="2.2537" y1="-0.254" x2="2.6549" y2="-0.254" width="0.127" layer="21"/>
<wire x1="0.2863" y1="-0.254" x2="2.2537" y2="-0.254" width="0.127" layer="51"/>
<wire x1="-0.7863" y1="2.5485" x2="0.7863" y2="2.5485" width="0.127" layer="51" curve="-34.2936"/>
<pad name="1" x="1.27" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="0" y="1.905" drill="0.8128" shape="octagon"/>
<pad name="3" x="-1.27" y="0" drill="0.8128" shape="octagon"/>
<text x="3.175" y="0.635" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="3.175" y="-1.27" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<text x="-0.635" y="0.635" size="1.27" layer="51" ratio="10">2</text>
<text x="-2.159" y="0" size="1.27" layer="51" ratio="10">3</text>
<text x="1.143" y="0" size="1.27" layer="51" ratio="10">1</text>
</package>
<package name="TO220BV" urn="urn:adsk.eagle:footprint:29371/1" library_version="4">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
<wire x1="4.699" y1="-4.318" x2="4.953" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="4.699" y1="-4.318" x2="-4.699" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-4.064" x2="-4.699" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="5.08" y1="-1.143" x2="4.953" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-4.064" x2="-5.08" y2="-1.143" width="0.1524" layer="21"/>
<circle x="-4.4958" y="-3.7084" radius="0.254" width="0" layer="21"/>
<pad name="G" x="-2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="D" x="0" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="S" x="2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<text x="-5.08" y="-6.0452" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-5.08" y="-7.62" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<rectangle x1="-5.334" y1="-0.762" x2="5.334" y2="0" layer="21"/>
<rectangle x1="-5.334" y1="-1.27" x2="-3.429" y2="-0.762" layer="21"/>
<rectangle x1="-1.651" y1="-1.27" x2="-0.889" y2="-0.762" layer="21"/>
<rectangle x1="-3.429" y1="-1.27" x2="-1.651" y2="-0.762" layer="51"/>
<rectangle x1="0.889" y1="-1.27" x2="1.651" y2="-0.762" layer="21"/>
<rectangle x1="3.429" y1="-1.27" x2="5.334" y2="-0.762" layer="21"/>
<rectangle x1="-0.889" y1="-1.27" x2="0.889" y2="-0.762" layer="51"/>
<rectangle x1="1.651" y1="-1.27" x2="3.429" y2="-0.762" layer="51"/>
</package>
</packages>
<packages3d>
<package3d name="SOT23" urn="urn:adsk.eagle:package:28738/2" type="model" library_version="4">
<description>SOT-23</description>
<packageinstances>
<packageinstance name="SOT23"/>
</packageinstances>
</package3d>
<package3d name="TO92" urn="urn:adsk.eagle:package:16378726/2" type="model" library_version="4">
<description>TO 92</description>
<packageinstances>
<packageinstance name="TO92"/>
</packageinstances>
</package3d>
<package3d name="TO220BV" urn="urn:adsk.eagle:package:29484/4" type="model" library_version="5">
<description>Molded Package
grid 2.54 mm</description>
<packageinstances>
<packageinstance name="TO220BV"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="MFNS" urn="urn:adsk.eagle:symbol:16378716/2" library_version="4">
<wire x1="-1.1176" y1="2.413" x2="-1.1176" y2="-2.54" width="0.254" layer="94"/>
<wire x1="-1.1176" y1="-2.54" x2="-2.54" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="0.5334" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="0.508" y1="-1.905" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="2.54" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="5.08" y2="1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="1.905" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="-1.905" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="2.54" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="4.445" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="4.445" y1="-0.635" x2="5.715" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="5.715" y1="-0.635" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.715" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.969" y2="1.016" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="4.191" y2="0.508" width="0.1524" layer="94"/>
<wire x1="0.508" y1="0" x2="1.778" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="1.778" y1="-0.508" x2="1.778" y2="0.508" width="0.1524" layer="94"/>
<wire x1="1.778" y1="0.508" x2="0.508" y2="0" width="0.1524" layer="94"/>
<wire x1="1.651" y1="0" x2="2.54" y2="0" width="0.1524" layer="94"/>
<wire x1="1.651" y1="0.254" x2="0.762" y2="0" width="0.3048" layer="94"/>
<wire x1="0.762" y1="0" x2="1.651" y2="-0.254" width="0.3048" layer="94"/>
<wire x1="1.651" y1="-0.254" x2="1.651" y2="0" width="0.3048" layer="94"/>
<wire x1="1.651" y1="0" x2="1.397" y2="0" width="0.3048" layer="94"/>
<circle x="2.54" y="-1.905" radius="0.127" width="0.4064" layer="94"/>
<circle x="2.54" y="1.905" radius="0.127" width="0.4064" layer="94"/>
<text x="6.35" y="1.27" size="1.778" layer="95">&gt;NAME</text>
<text x="6.35" y="-1.27" size="1.778" layer="96">&gt;VALUE</text>
<text x="1.27" y="2.54" size="0.8128" layer="93">D</text>
<text x="1.27" y="-3.175" size="0.8128" layer="93">S</text>
<text x="-2.54" y="-1.27" size="0.8128" layer="93">G</text>
<rectangle x1="-0.254" y1="-2.54" x2="0.508" y2="-1.27" layer="94"/>
<rectangle x1="-0.254" y1="1.27" x2="0.508" y2="2.54" layer="94"/>
<rectangle x1="-0.254" y1="-0.889" x2="0.508" y2="0.889" layer="94"/>
<pin name="G" x="-2.54" y="-2.54" visible="off" length="point" direction="pas"/>
<pin name="D" x="2.54" y="5.08" visible="off" length="short" direction="pas" rot="R270"/>
<pin name="S" x="2.54" y="-5.08" visible="off" length="short" direction="pas" rot="R90"/>
</symbol>
<symbol name="MFPS" urn="urn:adsk.eagle:symbol:16378717/2" library_version="4">
<wire x1="-1.016" y1="-2.54" x2="-1.016" y2="2.54" width="0.254" layer="94"/>
<wire x1="-1.016" y1="2.54" x2="-2.54" y2="2.54" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="0.5334" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="0" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="0.508" y1="1.905" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-2.54" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="1.905" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="2.54" y2="2.54" width="0.1524" layer="94"/>
<wire x1="2.2352" y1="0" x2="2.286" y2="0" width="0.1524" layer="94"/>
<wire x1="2.286" y1="0" x2="2.54" y2="0" width="0.1524" layer="94"/>
<wire x1="2.286" y1="0" x2="1.016" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="1.016" y1="-0.508" x2="1.016" y2="0.508" width="0.1524" layer="94"/>
<wire x1="1.016" y1="0.508" x2="2.286" y2="0" width="0.1524" layer="94"/>
<wire x1="1.143" y1="0" x2="0.254" y2="0" width="0.1524" layer="94"/>
<wire x1="1.143" y1="0.254" x2="2.032" y2="0" width="0.3048" layer="94"/>
<wire x1="2.032" y1="0" x2="1.143" y2="-0.254" width="0.3048" layer="94"/>
<wire x1="1.143" y1="-0.254" x2="1.143" y2="0" width="0.3048" layer="94"/>
<wire x1="1.143" y1="0" x2="1.397" y2="0" width="0.3048" layer="94"/>
<wire x1="5.08" y1="1.905" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.715" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="5.715" y1="-0.635" x2="4.445" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="4.445" y1="-0.635" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="4.445" y2="0.762" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="4.191" y2="1.016" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.969" y2="0.508" width="0.1524" layer="94"/>
<circle x="2.54" y="1.905" radius="0.127" width="0.4064" layer="94"/>
<circle x="2.54" y="-1.905" radius="0.127" width="0.4064" layer="94"/>
<text x="6.35" y="1.27" size="1.778" layer="95">&gt;NAME</text>
<text x="6.35" y="-1.27" size="1.778" layer="96">&gt;VALUE</text>
<text x="1.524" y="-3.302" size="0.8128" layer="93">D</text>
<text x="1.524" y="2.54" size="0.8128" layer="93">S</text>
<text x="-2.286" y="1.27" size="0.8128" layer="93">G</text>
<rectangle x1="-0.254" y1="1.27" x2="0.508" y2="2.54" layer="94"/>
<rectangle x1="-0.254" y1="-2.54" x2="0.508" y2="-1.27" layer="94"/>
<rectangle x1="-0.254" y1="-0.889" x2="0.508" y2="0.889" layer="94"/>
<pin name="G" x="-2.54" y="2.54" visible="off" length="point" direction="pas"/>
<pin name="D" x="2.54" y="-5.08" visible="off" length="short" direction="pas" rot="R90"/>
<pin name="S" x="2.54" y="5.08" visible="off" length="short" direction="pas" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NMOSFET" urn="urn:adsk.eagle:component:16378730/4" prefix="Q" library_version="5">
<description>&lt;b&gt; N-Channel MOSFET - Generic</description>
<gates>
<gate name="G$1" symbol="MFNS" x="-2.54" y="0"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:28738/2"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
<device name="TO92" package="TO92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378726/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
<device name="TO220" package="TO220BV">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:29484/4"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMOSFET_" urn="urn:adsk.eagle:component:16378732/4" prefix="Q" library_version="5">
<description>&lt;b&gt;P-Channel MOSFET - Popular parts&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MFPS" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:28738/2"/>
</package3dinstances>
<technologies>
<technology name="BSS84">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="MOSFET P-CH 50V 130MA SOT-23"/>
<attribute name="DRAIN_CURRENT" value="130mA" constant="no"/>
<attribute name="MANUFACTURER" value="ON Semiconductor" constant="no"/>
<attribute name="MPN" value="BSS84" constant="no"/>
<attribute name="OPERATING_TEMP" value="-55°C ~ 150°C" constant="no"/>
<attribute name="PART_STATUS" value="Active" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="Yes" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="360mW" constant="no"/>
<attribute name="TYPE" value="P-Channel" constant="no"/>
<attribute name="VALUE" value="BSS84" constant="no"/>
</technology>
<technology name="IRLML5203">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="MOSFET P-CH 30V 3A SOT-23" constant="no"/>
<attribute name="DRAIN_CURRENT" value="3A" constant="no"/>
<attribute name="MANUFACTURER" value="Infineon Technologies" constant="no"/>
<attribute name="MPN" value="IRLML5203TRPBF" constant="no"/>
<attribute name="OPERATING_TEMP" value="-55°C ~ 150°C" constant="no"/>
<attribute name="PART_STATUS" value="Active" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="Yes" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="1.25W" constant="no"/>
<attribute name="TYPE" value="P-Channel" constant="no"/>
<attribute name="VALUE" value="IRLML5203" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="eagle-ltspice" urn="urn:adsk.eagle:library:217">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0204/7" urn="urn:adsk.eagle:footprint:13215/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
<wire x1="3.81" y1="0" x2="2.921" y2="0" width="0.508" layer="51"/>
<wire x1="-3.81" y1="0" x2="-2.921" y2="0" width="0.508" layer="51"/>
<wire x1="-2.54" y1="0.762" x2="-2.286" y2="1.016" width="0.1524" layer="21" curve="-90"/>
<wire x1="-2.54" y1="-0.762" x2="-2.286" y2="-1.016" width="0.1524" layer="21" curve="90"/>
<wire x1="2.286" y1="-1.016" x2="2.54" y2="-0.762" width="0.1524" layer="21" curve="90"/>
<wire x1="2.286" y1="1.016" x2="2.54" y2="0.762" width="0.1524" layer="21" curve="-90"/>
<wire x1="-2.54" y1="-0.762" x2="-2.54" y2="0.762" width="0.1524" layer="21"/>
<wire x1="-2.286" y1="1.016" x2="-1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="-1.778" y1="0.889" x2="-1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="-2.286" y1="-1.016" x2="-1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="-1.778" y1="-0.889" x2="-1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="0.889" x2="1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="0.889" x2="-1.778" y2="0.889" width="0.1524" layer="21"/>
<wire x1="1.778" y1="-0.889" x2="1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="-0.889" x2="-1.778" y2="-0.889" width="0.1524" layer="21"/>
<wire x1="2.286" y1="1.016" x2="1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="2.286" y1="-1.016" x2="1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="2.54" y1="-0.762" x2="2.54" y2="0.762" width="0.1524" layer="21"/>
<rectangle x1="2.54" y1="-0.254" x2="2.921" y2="0.254" layer="21"/>
<rectangle x1="-2.921" y1="-0.254" x2="-2.54" y2="0.254" layer="21"/>
<pad name="1" x="-3.81" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="3.81" y="0" drill="0.8128" shape="octagon"/>
<text x="-2.54" y="1.2954" size="0.9906" layer="25" ratio="10">&gt;NAME</text>
<text x="-1.6256" y="-0.4826" size="0.9906" layer="27" ratio="10">&gt;VALUE</text>
</package>
<package name="0207/10" urn="urn:adsk.eagle:footprint:13216/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
<wire x1="5.08" y1="0" x2="4.064" y2="0" width="0.6096" layer="51"/>
<wire x1="-5.08" y1="0" x2="-4.064" y2="0" width="0.6096" layer="51"/>
<wire x1="-3.175" y1="0.889" x2="-2.921" y2="1.143" width="0.1524" layer="21" curve="-90"/>
<wire x1="-3.175" y1="-0.889" x2="-2.921" y2="-1.143" width="0.1524" layer="21" curve="90"/>
<wire x1="2.921" y1="-1.143" x2="3.175" y2="-0.889" width="0.1524" layer="21" curve="90"/>
<wire x1="2.921" y1="1.143" x2="3.175" y2="0.889" width="0.1524" layer="21" curve="-90"/>
<wire x1="-3.175" y1="-0.889" x2="-3.175" y2="0.889" width="0.1524" layer="21"/>
<wire x1="-2.921" y1="1.143" x2="-2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="-2.413" y1="1.016" x2="-2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="-2.921" y1="-1.143" x2="-2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="-2.413" y1="-1.016" x2="-2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="1.016" x2="2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="1.016" x2="-2.413" y2="1.016" width="0.1524" layer="21"/>
<wire x1="2.413" y1="-1.016" x2="2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="-1.016" x2="-2.413" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="2.921" y1="1.143" x2="2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="2.921" y1="-1.143" x2="2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="3.175" y1="-0.889" x2="3.175" y2="0.889" width="0.1524" layer="21"/>
<rectangle x1="3.175" y1="-0.3048" x2="4.0386" y2="0.3048" layer="21"/>
<rectangle x1="-4.0386" y1="-0.3048" x2="-3.175" y2="0.3048" layer="21"/>
<pad name="1" x="-5.08" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="5.08" y="0" drill="0.8128" shape="octagon"/>
<text x="-3.048" y="1.524" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-2.2606" y="-0.635" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
</package>
<package name="R0201" urn="urn:adsk.eagle:footprint:13233/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
<rectangle x1="-0.3" y1="-0.15" x2="-0.15" y2="0.15" layer="51"/>
<rectangle x1="0.15" y1="-0.15" x2="0.3" y2="0.15" layer="51"/>
<rectangle x1="-0.15" y1="-0.15" x2="0.15" y2="0.15" layer="21"/>
<smd name="1" x="-0.255" y="0" dx="0.28" dy="0.43" layer="1"/>
<smd name="2" x="0.255" y="0" dx="0.28" dy="0.43" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0402" urn="urn:adsk.eagle:footprint:13234/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.245" y1="0.224" x2="0.245" y2="0.224" width="0.1524" layer="51"/>
<wire x1="0.245" y1="-0.224" x2="-0.245" y2="-0.224" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.483" x2="1.473" y2="0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.483" x2="1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.483" x2="-1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.483" x2="-1.473" y2="0.483" width="0.0508" layer="39"/>
<rectangle x1="-0.554" y1="-0.3048" x2="-0.254" y2="0.2951" layer="51"/>
<rectangle x1="0.2588" y1="-0.3048" x2="0.5588" y2="0.2951" layer="51"/>
<rectangle x1="-0.1999" y1="-0.4001" x2="0.1999" y2="0.4001" layer="35"/>
<smd name="1" x="-0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<smd name="2" x="0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0603" urn="urn:adsk.eagle:footprint:13235/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.432" y1="-0.356" x2="0.432" y2="-0.356" width="0.1524" layer="51"/>
<wire x1="0.432" y1="0.356" x2="-0.432" y2="0.356" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.983" x2="1.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.983" x2="1.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.983" x2="-1.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.983" x2="-1.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4318" y1="-0.4318" x2="0.8382" y2="0.4318" layer="51"/>
<rectangle x1="-0.8382" y1="-0.4318" x2="-0.4318" y2="0.4318" layer="51"/>
<rectangle x1="-0.1999" y1="-0.4001" x2="0.1999" y2="0.4001" layer="35"/>
<smd name="1" x="-0.85" y="0" dx="1" dy="1.1" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1" dy="1.1" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0805" urn="urn:adsk.eagle:footprint:13236/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
<wire x1="-0.41" y1="0.635" x2="0.41" y2="0.635" width="0.1524" layer="51"/>
<wire x1="-0.41" y1="-0.635" x2="0.41" y2="-0.635" width="0.1524" layer="51"/>
<wire x1="-1.973" y1="0.983" x2="1.973" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="0.983" x2="1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="-0.983" x2="-1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.973" y1="-0.983" x2="-1.973" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4064" y1="-0.6985" x2="1.0564" y2="0.7015" layer="51"/>
<rectangle x1="-1.0668" y1="-0.6985" x2="-0.4168" y2="0.7015" layer="51"/>
<rectangle x1="-0.1999" y1="-0.5001" x2="0.1999" y2="0.5001" layer="35"/>
<smd name="1" x="-0.95" y="0" dx="1.3" dy="1.5" layer="1"/>
<smd name="2" x="0.95" y="0" dx="1.3" dy="1.5" layer="1"/>
<text x="-0.635" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1005" urn="urn:adsk.eagle:footprint:13237/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.245" y1="0.224" x2="0.245" y2="0.224" width="0.1524" layer="51"/>
<wire x1="0.245" y1="-0.224" x2="-0.245" y2="-0.224" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.483" x2="1.473" y2="0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.483" x2="1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.483" x2="-1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.483" x2="-1.473" y2="0.483" width="0.0508" layer="39"/>
<rectangle x1="-0.554" y1="-0.3048" x2="-0.254" y2="0.2951" layer="51"/>
<rectangle x1="0.2588" y1="-0.3048" x2="0.5588" y2="0.2951" layer="51"/>
<rectangle x1="-0.1999" y1="-0.3" x2="0.1999" y2="0.3" layer="35"/>
<smd name="1" x="-0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<smd name="2" x="0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1206" urn="urn:adsk.eagle:footprint:13238/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="0.9525" y1="-0.8128" x2="-0.9652" y2="-0.8128" width="0.1524" layer="51"/>
<wire x1="0.9525" y1="0.8128" x2="-0.9652" y2="0.8128" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="0.983" x2="2.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="0.983" x2="2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-0.983" x2="-2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-0.983" x2="-2.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="-1.6891" y1="-0.8763" x2="-0.9525" y2="0.8763" layer="51"/>
<rectangle x1="0.9525" y1="-0.8763" x2="1.6891" y2="0.8763" layer="51"/>
<rectangle x1="-0.3" y1="-0.7" x2="0.3" y2="0.7" layer="35"/>
<smd name="1" x="-1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<smd name="2" x="1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<text x="-1.27" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.27" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1210" urn="urn:adsk.eagle:footprint:13239/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="1.219" x2="0.939" y2="1.219" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-1.219" x2="0.939" y2="-1.219" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="1.483" x2="2.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="1.483" x2="2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-1.483" x2="-2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-1.483" x2="-2.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-1.3081" x2="-0.9009" y2="1.2918" layer="51"/>
<rectangle x1="0.9144" y1="-1.3081" x2="1.6645" y2="1.2918" layer="51"/>
<rectangle x1="-0.3" y1="-0.8999" x2="0.3" y2="0.8999" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1218" urn="urn:adsk.eagle:footprint:13240/1" library_version="1">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
<wire x1="-0.913" y1="-2.219" x2="0.939" y2="-2.219" width="0.1524" layer="51"/>
<wire x1="0.913" y1="2.219" x2="-0.939" y2="2.219" width="0.1524" layer="51"/>
<rectangle x1="-1.651" y1="-2.3" x2="-0.9009" y2="2.3" layer="51"/>
<rectangle x1="0.9144" y1="-2.3" x2="1.6645" y2="2.3" layer="51"/>
<smd name="1" x="-1.475" y="0" dx="1.05" dy="4.9" layer="1"/>
<smd name="2" x="1.475" y="0" dx="1.05" dy="4.9" layer="1"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2010" urn="urn:adsk.eagle:footprint:13241/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-1.662" y1="1.245" x2="1.662" y2="1.245" width="0.1524" layer="51"/>
<wire x1="-1.637" y1="-1.245" x2="1.687" y2="-1.245" width="0.1524" layer="51"/>
<wire x1="-3.473" y1="1.483" x2="3.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="1.483" x2="3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="-1.483" x2="-3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-3.473" y1="-1.483" x2="-3.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-2.4892" y1="-1.3208" x2="-1.6393" y2="1.3292" layer="51"/>
<rectangle x1="1.651" y1="-1.3208" x2="2.5009" y2="1.3292" layer="51"/>
<smd name="1" x="-2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<smd name="2" x="2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<text x="-3.175" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.175" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2012" urn="urn:adsk.eagle:footprint:13242/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.41" y1="0.635" x2="0.41" y2="0.635" width="0.1524" layer="51"/>
<wire x1="-0.41" y1="-0.635" x2="0.41" y2="-0.635" width="0.1524" layer="51"/>
<wire x1="-1.973" y1="0.983" x2="1.973" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="0.983" x2="1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="-0.983" x2="-1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.973" y1="-0.983" x2="-1.973" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4064" y1="-0.6985" x2="1.0564" y2="0.7015" layer="51"/>
<rectangle x1="-1.0668" y1="-0.6985" x2="-0.4168" y2="0.7015" layer="51"/>
<rectangle x1="-0.1001" y1="-0.5999" x2="0.1001" y2="0.5999" layer="35"/>
<smd name="1" x="-0.85" y="0" dx="1.3" dy="1.5" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1.3" dy="1.5" layer="1"/>
<text x="-0.635" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2512" urn="urn:adsk.eagle:footprint:13243/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-2.362" y1="1.473" x2="2.387" y2="1.473" width="0.1524" layer="51"/>
<wire x1="-2.362" y1="-1.473" x2="2.387" y2="-1.473" width="0.1524" layer="51"/>
<wire x1="-3.973" y1="1.983" x2="3.973" y2="1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="1.983" x2="3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="-1.983" x2="-3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="-3.973" y1="-1.983" x2="-3.973" y2="1.983" width="0.0508" layer="39"/>
<rectangle x1="-3.2004" y1="-1.5494" x2="-2.3505" y2="1.5507" layer="51"/>
<rectangle x1="2.3622" y1="-1.5494" x2="3.2121" y2="1.5507" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-2.8" y="0" dx="1.8" dy="3.2" layer="1"/>
<smd name="2" x="2.8" y="0" dx="1.8" dy="3.2" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R3216" urn="urn:adsk.eagle:footprint:13244/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="0.8" x2="0.888" y2="0.8" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-0.8" x2="0.888" y2="-0.8" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="0.983" x2="2.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="0.983" x2="2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-0.983" x2="-2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-0.983" x2="-2.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-0.8763" x2="-0.9009" y2="0.8738" layer="51"/>
<rectangle x1="0.889" y1="-0.8763" x2="1.6391" y2="0.8738" layer="51"/>
<rectangle x1="-0.3" y1="-0.7" x2="0.3" y2="0.7" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="1.8" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="1.8" layer="1"/>
<text x="-1.905" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R3225" urn="urn:adsk.eagle:footprint:13245/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="1.219" x2="0.939" y2="1.219" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-1.219" x2="0.939" y2="-1.219" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="1.483" x2="2.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="1.483" x2="2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-1.483" x2="-2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-1.483" x2="-2.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-1.3081" x2="-0.9009" y2="1.2918" layer="51"/>
<rectangle x1="0.9144" y1="-1.3081" x2="1.6645" y2="1.2918" layer="51"/>
<rectangle x1="-0.3" y1="-1" x2="0.3" y2="1" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R4527" urn="urn:adsk.eagle:footprint:13246/1" library_version="1">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
<wire x1="-5.675" y1="-3.375" x2="5.65" y2="-3.375" width="0.2032" layer="21"/>
<wire x1="5.65" y1="-3.375" x2="5.65" y2="3.375" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.375" x2="-5.675" y2="3.375" width="0.2032" layer="21"/>
<wire x1="-5.675" y1="3.375" x2="-5.675" y2="-3.375" width="0.2032" layer="51"/>
<smd name="1" x="-4.575" y="0" dx="3.94" dy="5.84" layer="1"/>
<smd name="2" x="4.575" y="0" dx="3.94" dy="5.84" layer="1"/>
<text x="-5.715" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.715" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R5025" urn="urn:adsk.eagle:footprint:13247/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-1.662" y1="1.245" x2="1.662" y2="1.245" width="0.1524" layer="51"/>
<wire x1="-1.637" y1="-1.245" x2="1.687" y2="-1.245" width="0.1524" layer="51"/>
<wire x1="-3.473" y1="1.483" x2="3.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="1.483" x2="3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="-1.483" x2="-3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-3.473" y1="-1.483" x2="-3.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-2.4892" y1="-1.3208" x2="-1.6393" y2="1.3292" layer="51"/>
<rectangle x1="1.651" y1="-1.3208" x2="2.5009" y2="1.3292" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<smd name="2" x="2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<text x="-3.175" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.175" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R6332" urn="urn:adsk.eagle:footprint:13248/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
<wire x1="-2.362" y1="1.473" x2="2.387" y2="1.473" width="0.1524" layer="51"/>
<wire x1="-2.362" y1="-1.473" x2="2.387" y2="-1.473" width="0.1524" layer="51"/>
<wire x1="-3.973" y1="1.983" x2="3.973" y2="1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="1.983" x2="3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="-1.983" x2="-3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="-3.973" y1="-1.983" x2="-3.973" y2="1.983" width="0.0508" layer="39"/>
<rectangle x1="-3.2004" y1="-1.5494" x2="-2.3505" y2="1.5507" layer="51"/>
<rectangle x1="2.3622" y1="-1.5494" x2="3.2121" y2="1.5507" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-3.1" y="0" dx="1" dy="3.2" layer="1"/>
<smd name="2" x="3.1" y="0" dx="1" dy="3.2" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="0204/7" urn="urn:adsk.eagle:package:13274/1" type="box" library_version="1">
<description>RESISTOR
type 0204, grid 7.5 mm</description>
<packageinstances>
<packageinstance name="0204/7"/>
</packageinstances>
</package3d>
<package3d name="0207/10" urn="urn:adsk.eagle:package:13275/1" type="box" library_version="1">
<description>RESISTOR
type 0207, grid 10 mm</description>
<packageinstances>
<packageinstance name="0207/10"/>
</packageinstances>
</package3d>
<package3d name="R0201" urn="urn:adsk.eagle:package:13294/1" type="box" library_version="1">
<description>RESISTOR chip
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
<packageinstances>
<packageinstance name="R0201"/>
</packageinstances>
</package3d>
<package3d name="R0402" urn="urn:adsk.eagle:package:13296/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0402"/>
</packageinstances>
</package3d>
<package3d name="R0603" urn="urn:adsk.eagle:package:13302/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0603"/>
</packageinstances>
</package3d>
<package3d name="R0805" urn="urn:adsk.eagle:package:13300/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0805"/>
</packageinstances>
</package3d>
<package3d name="R1005" urn="urn:adsk.eagle:package:13297/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1005"/>
</packageinstances>
</package3d>
<package3d name="R1206" urn="urn:adsk.eagle:package:13301/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1206"/>
</packageinstances>
</package3d>
<package3d name="R1210" urn="urn:adsk.eagle:package:13299/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1210"/>
</packageinstances>
</package3d>
<package3d name="R1218" urn="urn:adsk.eagle:package:13303/1" type="box" library_version="1">
<description>CRCW1218 Thick Film, Rectangular Chip Resistors
Source: http://www.vishay.com .. dcrcw.pdf</description>
<packageinstances>
<packageinstance name="R1218"/>
</packageinstances>
</package3d>
<package3d name="R2010" urn="urn:adsk.eagle:package:13309/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2010"/>
</packageinstances>
</package3d>
<package3d name="R2012" urn="urn:adsk.eagle:package:13306/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2012"/>
</packageinstances>
</package3d>
<package3d name="R2512" urn="urn:adsk.eagle:package:13304/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2512"/>
</packageinstances>
</package3d>
<package3d name="R3216" urn="urn:adsk.eagle:package:13305/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R3216"/>
</packageinstances>
</package3d>
<package3d name="R3225" urn="urn:adsk.eagle:package:13311/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R3225"/>
</packageinstances>
</package3d>
<package3d name="R5025" urn="urn:adsk.eagle:package:13308/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R5025"/>
</packageinstances>
</package3d>
<package3d name="R6332" urn="urn:adsk.eagle:package:13307/1" type="box" library_version="1">
<description>RESISTOR
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
<packageinstances>
<packageinstance name="R6332"/>
</packageinstances>
</package3d>
<package3d name="R4527" urn="urn:adsk.eagle:package:13310/2" type="model" library_version="3">
<description>Package 4527
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
<packageinstances>
<packageinstance name="R4527"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="R" urn="urn:adsk.eagle:symbol:13232/1" library_version="1">
<wire x1="-2.54" y1="-0.889" x2="2.54" y2="-0.889" width="0.254" layer="94"/>
<wire x1="2.54" y1="0.889" x2="-2.54" y2="0.889" width="0.254" layer="94"/>
<wire x1="2.54" y1="-0.889" x2="2.54" y2="0.889" width="0.254" layer="94"/>
<wire x1="-2.54" y1="-0.889" x2="-2.54" y2="0.889" width="0.254" layer="94"/>
<pin name="1" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1"/>
<pin name="2" x="5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1" rot="R180"/>
<text x="-3.81" y="1.4986" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.81" y="-3.302" size="1.778" layer="96">&gt;VALUE</text>
<text x="-5.08" y="0" size="0.4064" layer="99" align="center">SpiceOrder 1</text>
<text x="5.08" y="0" size="0.4064" layer="99" align="center">SpiceOrder 2</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="R" urn="urn:adsk.eagle:component:13322/2" prefix="R" uservalue="yes" library_version="3">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="R" x="0" y="0"/>
</gates>
<devices>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13274/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13275/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0201" package="R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13294/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13296/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13302/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13300/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13297/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13301/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13299/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1218" package="R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13303/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13309/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13306/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13304/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13305/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13311/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R4527" package="R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13310/2"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13308/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13307/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="eScooter">
<packages>
<package name="DIOM5027X220N" urn="urn:adsk.eagle:footprint:21928331/1">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<wire x1="2.5" y1="1.35" x2="-3.3699" y2="1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="1.35" x2="-3.3699" y2="-1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="-1.35" x2="2.5" y2="-1.35" width="0.12" layer="21"/>
<wire x1="2.5" y1="-1.35" x2="-2.5" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="-1.35" x2="-2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="1.35" x2="2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="2.5" y1="1.35" x2="2.5" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<smd name="2" x="2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<text x="0" y="1.985" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.985" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SON254P1750X4300X120-30M" urn="urn:adsk.eagle:footprint:21849939/1">
<description>30-SON (DFN), 2.54 mm pitch, 43.00 X 17.50 X 1.20 mm body
&lt;p&gt;30-pin SON (DFN) package with 2.54 mm pitch with body size 43.00 X 17.50 X 1.20 mm&lt;/p&gt;</description>
<circle x="-9.254" y="18.9349" radius="0.25" width="0" layer="21"/>
<wire x1="-8.75" y1="18.6849" x2="-8.75" y2="21.5" width="0.12" layer="21"/>
<wire x1="-8.75" y1="21.5" x2="8.75" y2="21.5" width="0.12" layer="21"/>
<wire x1="8.75" y1="21.5" x2="8.75" y2="18.6849" width="0.12" layer="21"/>
<wire x1="-8.75" y1="-18.6849" x2="-8.75" y2="-21.5" width="0.12" layer="21"/>
<wire x1="-8.75" y1="-21.5" x2="8.75" y2="-21.5" width="0.12" layer="21"/>
<wire x1="8.75" y1="-21.5" x2="8.75" y2="-18.6849" width="0.12" layer="21"/>
<wire x1="8.75" y1="-21.5" x2="-8.75" y2="-21.5" width="0.12" layer="51"/>
<wire x1="-8.75" y1="-21.5" x2="-8.75" y2="21.5" width="0.12" layer="51"/>
<wire x1="-8.75" y1="21.5" x2="8.75" y2="21.5" width="0.12" layer="51"/>
<wire x1="8.75" y1="21.5" x2="8.75" y2="-21.5" width="0.12" layer="51"/>
<smd name="1" x="-7.95" y="17.78" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="2" x="-7.95" y="15.24" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="3" x="-7.95" y="12.7" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="4" x="-7.95" y="10.16" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="5" x="-7.95" y="7.62" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="6" x="-7.95" y="5.08" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="7" x="-7.95" y="2.54" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="8" x="-7.95" y="0" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="9" x="-7.95" y="-2.54" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="10" x="-7.95" y="-5.08" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="11" x="-7.95" y="-7.62" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="12" x="-7.95" y="-10.16" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="13" x="-7.95" y="-12.7" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="14" x="-7.95" y="-15.24" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="15" x="-7.95" y="-17.78" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="16" x="7.95" y="-17.78" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="17" x="7.95" y="-15.24" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="18" x="7.95" y="-12.7" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="19" x="7.95" y="-10.16" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="20" x="7.95" y="-7.62" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="21" x="7.95" y="-5.08" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="22" x="7.95" y="-2.54" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="23" x="7.95" y="0" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="24" x="7.95" y="2.54" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="25" x="7.95" y="5.08" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="26" x="7.95" y="7.62" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="27" x="7.95" y="10.16" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="28" x="7.95" y="12.7" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="29" x="7.95" y="15.24" dx="2.5118" dy="1.3018" layer="1"/>
<smd name="30" x="7.95" y="17.78" dx="2.5118" dy="1.3018" layer="1"/>
<text x="0" y="22.135" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-22.135" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DIOM5027X220N" urn="urn:adsk.eagle:package:21928182/1" type="model">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM5027X220N"/>
</packageinstances>
</package3d>
<package3d name="SON254P1750X4300X120-30M" urn="urn:adsk.eagle:package:21849926/1" type="model">
<description>30-SON (DFN), 2.54 mm pitch, 43.00 X 17.50 X 1.20 mm body
&lt;p&gt;30-pin SON (DFN) package with 2.54 mm pitch with body size 43.00 X 17.50 X 1.20 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SON254P1750X4300X120-30M"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="TVS_DIODE">
<wire x1="0" y1="0" x2="-1.27" y2="1.524" width="0.254" layer="94"/>
<wire x1="1.27" y1="1.524" x2="0" y2="0" width="0.254" layer="94"/>
<wire x1="-1.778" y1="-0.508" x2="-1.27" y2="0" width="0.254" layer="94"/>
<wire x1="-1.27" y1="0" x2="1.27" y2="0" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="1.778" y2="0.508" width="0.254" layer="94"/>
<wire x1="0" y1="0" x2="-1.27" y2="-1.524" width="0.254" layer="94"/>
<wire x1="1.27" y1="-1.524" x2="0" y2="0" width="0.254" layer="94"/>
<wire x1="-1.27" y1="1.524" x2="1.27" y2="1.524" width="0.254" layer="94"/>
<wire x1="-1.27" y1="-1.524" x2="1.27" y2="-1.524" width="0.254" layer="94"/>
<pin name="P$1" x="0" y="4.064" visible="off" length="short" rot="R270"/>
<pin name="P$2" x="0" y="-4.064" visible="off" length="short" rot="R90"/>
<text x="2.54" y="2.54" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-2.54" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="ARDUINO">
<wire x1="-10.16" y1="20.32" x2="-10.16" y2="-20.32" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-20.32" x2="10.16" y2="-20.32" width="0.254" layer="94"/>
<wire x1="10.16" y1="-20.32" x2="10.16" y2="20.32" width="0.254" layer="94"/>
<wire x1="10.16" y1="20.32" x2="-10.16" y2="20.32" width="0.254" layer="94"/>
<pin name="D13" x="-15.24" y="17.78" length="middle"/>
<pin name="3V3" x="-15.24" y="15.24" length="middle" direction="pwr"/>
<pin name="REF" x="-15.24" y="12.7" length="middle"/>
<pin name="A0" x="-15.24" y="10.16" length="middle"/>
<pin name="A1" x="-15.24" y="7.62" length="middle"/>
<pin name="A2" x="-15.24" y="5.08" length="middle"/>
<pin name="A3" x="-15.24" y="2.54" length="middle"/>
<pin name="A4" x="-15.24" y="0" length="middle"/>
<pin name="A5" x="-15.24" y="-2.54" length="middle"/>
<pin name="A6" x="-15.24" y="-5.08" length="middle"/>
<pin name="A7" x="-15.24" y="-7.62" length="middle"/>
<pin name="5V" x="-15.24" y="-10.16" length="middle" direction="pwr"/>
<pin name="RST" x="-15.24" y="-12.7" length="middle" direction="in"/>
<pin name="GND" x="-15.24" y="-15.24" length="middle" direction="pwr"/>
<pin name="VIN" x="-15.24" y="-17.78" length="middle" direction="pwr"/>
<pin name="TX1" x="15.24" y="-17.78" length="middle" direction="out" rot="R180"/>
<pin name="RX0" x="15.24" y="-15.24" length="middle" direction="in" rot="R180"/>
<pin name="RST2" x="15.24" y="-12.7" length="middle" direction="in" rot="R180"/>
<pin name="GND2" x="15.24" y="-10.16" length="middle" direction="pwr" rot="R180"/>
<pin name="D2" x="15.24" y="-7.62" length="middle" rot="R180"/>
<pin name="D3" x="15.24" y="-5.08" length="middle" rot="R180"/>
<pin name="D4" x="15.24" y="-2.54" length="middle" rot="R180"/>
<pin name="D5" x="15.24" y="0" length="middle" rot="R180"/>
<pin name="D6" x="15.24" y="2.54" length="middle" rot="R180"/>
<pin name="D7" x="15.24" y="5.08" length="middle" rot="R180"/>
<pin name="D8" x="15.24" y="7.62" length="middle" rot="R180"/>
<pin name="D9" x="15.24" y="10.16" length="middle" rot="R180"/>
<pin name="D10" x="15.24" y="12.7" length="middle" rot="R180"/>
<pin name="D11" x="15.24" y="15.24" length="middle" rot="R180"/>
<pin name="D12" x="15.24" y="17.78" length="middle" rot="R180"/>
<text x="-5.08" y="22.86" size="1.778" layer="95">&gt;NAME</text>
<text x="-5.08" y="-25.4" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="TVS_DIODE">
<description>TVS protective diode</description>
<gates>
<gate name="D$1" symbol="TVS_DIODE" x="0" y="0"/>
</gates>
<devices>
<device name="SMA" package="DIOM5027X220N">
<connects>
<connect gate="D$1" pin="P$1" pad="1"/>
<connect gate="D$1" pin="P$2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:21928182/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO">
<description>Ardino nano</description>
<gates>
<gate name="G$1" symbol="ARDUINO" x="0" y="0"/>
</gates>
<devices>
<device name="ARDUINO_NANO" package="SON254P1750X4300X120-30M">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="5V" pad="12"/>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="9"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="11"/>
<connect gate="G$1" pin="D10" pad="28"/>
<connect gate="G$1" pin="D11" pad="29"/>
<connect gate="G$1" pin="D12" pad="30"/>
<connect gate="G$1" pin="D13" pad="1"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="D8" pad="26"/>
<connect gate="G$1" pin="D9" pad="27"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="GND2" pad="19"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="RST" pad="13"/>
<connect gate="G$1" pin="RST2" pad="18"/>
<connect gate="G$1" pin="RX0" pad="17"/>
<connect gate="G$1" pin="TX1" pad="16"/>
<connect gate="G$1" pin="VIN" pad="15"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:21849926/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1" urn="urn:adsk.eagle:library:371">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND" urn="urn:adsk.eagle:symbol:26925/1" library_version="1">
<wire x1="-1.905" y1="0" x2="1.905" y2="0" width="0.254" layer="94"/>
<text x="-2.54" y="-2.54" size="1.778" layer="96">&gt;VALUE</text>
<pin name="GND" x="0" y="2.54" visible="off" length="short" direction="sup" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" urn="urn:adsk.eagle:component:26954/1" prefix="GND" library_version="1">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND" x="0" y="0"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM" urn="urn:adsk.eagle:footprint:40103/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
<wire x1="3.048" y1="1.016" x2="3.048" y2="2.54" width="0.2032" layer="51"/>
<wire x1="3.048" y1="2.54" x2="2.54" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.54" y1="-3.048" x2="3.048" y2="-2.54" width="0.2032" layer="51"/>
<wire x1="3.048" y1="-2.54" x2="3.048" y2="-1.016" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="3.048" x2="-3.048" y2="2.54" width="0.2032" layer="51"/>
<wire x1="-3.048" y1="2.54" x2="-3.048" y2="1.016" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-3.048" x2="-3.048" y2="-2.54" width="0.2032" layer="51"/>
<wire x1="-3.048" y1="-2.54" x2="-3.048" y2="-1.016" width="0.2032" layer="51"/>
<wire x1="2.54" y1="-3.048" x2="2.159" y2="-3.048" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-3.048" x2="-2.159" y2="-3.048" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="3.048" x2="-2.159" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.54" y1="3.048" x2="2.159" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.159" y1="3.048" x2="-2.159" y2="3.048" width="0.2032" layer="21"/>
<wire x1="-2.159" y1="-3.048" x2="2.159" y2="-3.048" width="0.2032" layer="21"/>
<wire x1="3.048" y1="0.998" x2="3.048" y2="-1.016" width="0.2032" layer="21"/>
<wire x1="-3.048" y1="1.028" x2="-3.048" y2="-1.016" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="1.27" x2="-2.54" y2="0.508" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-0.508" x2="-2.54" y2="-1.27" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="0.508" x2="-2.159" y2="-0.381" width="0.2032" layer="51"/>
<circle x="0" y="0" radius="1.778" width="0.2032" layer="21"/>
<pad name="1" x="-3.2512" y="2.2606" drill="1.016" diameter="1.8796"/>
<pad name="2" x="3.2512" y="2.2606" drill="1.016" diameter="1.8796"/>
<pad name="3" x="-3.2512" y="-2.2606" drill="1.016" diameter="1.8796"/>
<pad name="4" x="3.2512" y="-2.2606" drill="1.016" diameter="1.8796"/>
<text x="0" y="3.302" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-3.175" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_4.5MM" urn="urn:adsk.eagle:footprint:40104/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.5mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://spec_sheets.e-switch.com/specs/P010338.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
<wire x1="1.905" y1="1.27" x2="1.905" y2="0.445" width="0.127" layer="51"/>
<wire x1="1.905" y1="0.445" x2="2.16" y2="-0.01" width="0.127" layer="51"/>
<wire x1="1.905" y1="-0.23" x2="1.905" y2="-1.115" width="0.127" layer="51"/>
<wire x1="-2.25" y1="2.25" x2="2.25" y2="2.25" width="0.127" layer="51"/>
<wire x1="2.25" y1="2.25" x2="2.25" y2="-2.25" width="0.127" layer="51"/>
<wire x1="2.25" y1="-2.25" x2="-2.25" y2="-2.25" width="0.127" layer="51"/>
<wire x1="-2.25" y1="-2.25" x2="-2.25" y2="2.25" width="0.127" layer="51"/>
<wire x1="-2.2" y1="0.8" x2="-2.2" y2="-0.8" width="0.2032" layer="21"/>
<wire x1="1.3" y1="2.2" x2="-1.3" y2="2.2" width="0.2032" layer="21"/>
<wire x1="2.2" y1="-0.8" x2="2.2" y2="0.8" width="0.2032" layer="21"/>
<wire x1="-1.3" y1="-2.2" x2="1.3" y2="-2.2" width="0.2032" layer="21"/>
<wire x1="2.2" y1="0.8" x2="1.8" y2="0.8" width="0.2032" layer="21"/>
<wire x1="2.2" y1="-0.8" x2="1.8" y2="-0.8" width="0.2032" layer="21"/>
<wire x1="-1.8" y1="0.8" x2="-2.2" y2="0.8" width="0.2032" layer="21"/>
<wire x1="-1.8" y1="-0.8" x2="-2.2" y2="-0.8" width="0.2032" layer="21"/>
<circle x="0" y="0" radius="1.27" width="0.2032" layer="21"/>
<smd name="1" x="2.225" y="1.75" dx="1.1" dy="0.7" layer="1" rot="R90"/>
<smd name="2" x="2.225" y="-1.75" dx="1.1" dy="0.7" layer="1" rot="R90"/>
<smd name="3" x="-2.225" y="-1.75" dx="1.1" dy="0.7" layer="1" rot="R90"/>
<smd name="4" x="-2.225" y="1.75" dx="1.1" dy="0.7" layer="1" rot="R90"/>
<text x="0" y="2.413" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-2.413" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_PTH_12MM" urn="urn:adsk.eagle:footprint:40105/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-5050)&lt;/p&gt;</description>
<wire x1="5" y1="-1.3" x2="5" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="5" y1="-0.7" x2="4.5" y2="-0.2" width="0.2032" layer="51"/>
<wire x1="5" y1="0.2" x2="5" y2="1" width="0.2032" layer="51"/>
<wire x1="-6" y1="4" x2="-6" y2="5" width="0.2032" layer="21"/>
<wire x1="-5" y1="6" x2="5" y2="6" width="0.2032" layer="21"/>
<wire x1="6" y1="5" x2="6" y2="4" width="0.2032" layer="21"/>
<wire x1="6" y1="1" x2="6" y2="-1" width="0.2032" layer="21"/>
<wire x1="6" y1="-4" x2="6" y2="-5" width="0.2032" layer="21"/>
<wire x1="5" y1="-6" x2="-5" y2="-6" width="0.2032" layer="21"/>
<wire x1="-6" y1="-5" x2="-6" y2="-4" width="0.2032" layer="21"/>
<wire x1="-6" y1="-1" x2="-6" y2="1" width="0.2032" layer="21"/>
<wire x1="-6" y1="5" x2="-5" y2="6" width="0.2032" layer="21" curve="-90"/>
<wire x1="5" y1="6" x2="6" y2="5" width="0.2032" layer="21" curve="-90"/>
<wire x1="6" y1="-5" x2="5" y2="-6" width="0.2032" layer="21" curve="-90"/>
<wire x1="-5" y1="-6" x2="-6" y2="-5" width="0.2032" layer="21" curve="-90"/>
<circle x="0" y="0" radius="3.5" width="0.2032" layer="21"/>
<circle x="-4.5" y="4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="4.5" y="4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="4.5" y="-4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="-4.5" y="-4.5" radius="0.3" width="0.7" layer="21"/>
<pad name="4" x="-6.25" y="2.5" drill="1.2" diameter="2.159"/>
<pad name="2" x="-6.25" y="-2.5" drill="1.2" diameter="2.159"/>
<pad name="1" x="6.25" y="-2.5" drill="1.2" diameter="2.159"/>
<pad name="3" x="6.25" y="2.5" drill="1.2" diameter="2.159"/>
<text x="0" y="6.223" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-6.223" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM" urn="urn:adsk.eagle:footprint:40106/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<wire x1="-3" y1="1.1" x2="-3" y2="-1.1" width="0.127" layer="51"/>
<wire x1="3" y1="1.1" x2="3" y2="-1.1" width="0.127" layer="51"/>
<wire x1="-2.75" y1="1.75" x2="-3" y2="1.5" width="0.2032" layer="21" curve="90"/>
<wire x1="-2.75" y1="1.75" x2="2.75" y2="1.75" width="0.2032" layer="21"/>
<wire x1="2.75" y1="1.75" x2="3" y2="1.5" width="0.2032" layer="21" curve="-90"/>
<wire x1="3" y1="-1.5" x2="2.75" y2="-1.75" width="0.2032" layer="21" curve="-90"/>
<wire x1="2.75" y1="-1.75" x2="-2.75" y2="-1.75" width="0.2032" layer="21"/>
<wire x1="-3" y1="-1.5" x2="-2.75" y2="-1.75" width="0.2032" layer="21" curve="90"/>
<wire x1="-3" y1="-1.5" x2="-3" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-3" y1="1.1" x2="-3" y2="1.5" width="0.2032" layer="21"/>
<wire x1="3" y1="1.1" x2="3" y2="1.5" width="0.2032" layer="21"/>
<wire x1="3" y1="-1.5" x2="3" y2="-1.1" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="0.75" x2="1.5" y2="0.75" width="0.2032" layer="21"/>
<wire x1="1.5" y1="-0.75" x2="-1.5" y2="-0.75" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="-0.75" x2="-1.5" y2="0.75" width="0.2032" layer="21"/>
<wire x1="1.5" y1="-0.75" x2="1.5" y2="0.75" width="0.2032" layer="21"/>
<wire x1="-2" y1="0" x2="-1" y2="0" width="0.127" layer="51"/>
<wire x1="-1" y1="0" x2="0.1" y2="0.5" width="0.127" layer="51"/>
<wire x1="0.3" y1="0" x2="2" y2="0" width="0.127" layer="51"/>
<smd name="1" x="-3.15" y="0" dx="2.3" dy="1.6" layer="1" rot="R180"/>
<smd name="2" x="3.15" y="0" dx="2.3" dy="1.6" layer="1" rot="R180"/>
<text x="0" y="1.905" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.905" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_6.2MM_TALL" urn="urn:adsk.eagle:footprint:40107/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.apem.com/files/apem/brochures/ADTS6-ADTSM-KTSC6.pdf"&gt;Datasheet&lt;/a&gt; (ADTSM63NVTR)&lt;/p&gt;</description>
<wire x1="-3" y1="-3" x2="3" y2="-3" width="0.2032" layer="21"/>
<wire x1="3" y1="-3" x2="3" y2="3" width="0.2032" layer="21"/>
<wire x1="3" y1="3" x2="-3" y2="3" width="0.2032" layer="21"/>
<wire x1="-3" y1="3" x2="-3" y2="-3" width="0.2032" layer="21"/>
<circle x="0" y="0" radius="1.75" width="0.2032" layer="21"/>
<smd name="A1" x="-3.975" y="-2.25" dx="1.3" dy="1.55" layer="1" rot="R90"/>
<smd name="A2" x="3.975" y="-2.25" dx="1.3" dy="1.55" layer="1" rot="R90"/>
<smd name="B1" x="-3.975" y="2.25" dx="1.3" dy="1.55" layer="1" rot="R90"/>
<smd name="B2" x="3.975" y="2.25" dx="1.3" dy="1.55" layer="1" rot="R90"/>
<text x="0" y="3.175" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-3.175" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT" urn="urn:adsk.eagle:footprint:40108/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
<wire x1="1.5" y1="-3.8" x2="-1.5" y2="-3.8" width="0.127" layer="51"/>
<wire x1="-3.65" y1="-2" x2="-3.65" y2="3.5" width="0.127" layer="51"/>
<wire x1="-3.65" y1="3.5" x2="-3" y2="3.5" width="0.127" layer="51"/>
<wire x1="3" y1="3.5" x2="3.65" y2="3.5" width="0.127" layer="51"/>
<wire x1="3.65" y1="3.5" x2="3.65" y2="-2" width="0.127" layer="51"/>
<wire x1="-3" y1="2" x2="3" y2="2" width="0.127" layer="51"/>
<wire x1="-3" y1="2" x2="-3" y2="3.5" width="0.127" layer="51"/>
<wire x1="3" y1="2" x2="3" y2="3.5" width="0.127" layer="51"/>
<wire x1="-3.65" y1="-2" x2="-1.5" y2="-2" width="0.127" layer="51"/>
<wire x1="-1.5" y1="-2" x2="1.5" y2="-2" width="0.127" layer="51"/>
<wire x1="1.5" y1="-2" x2="3.65" y2="-2" width="0.127" layer="51"/>
<wire x1="1.5" y1="-2" x2="1.5" y2="-3.8" width="0.127" layer="51"/>
<wire x1="-1.5" y1="-2" x2="-1.5" y2="-3.8" width="0.127" layer="51"/>
<wire x1="-3.777" y1="1" x2="-3.777" y2="-2.127" width="0.2032" layer="21"/>
<wire x1="-3.777" y1="-2.127" x2="3.777" y2="-2.127" width="0.2032" layer="21"/>
<wire x1="3.777" y1="-2.127" x2="3.777" y2="1" width="0.2032" layer="21"/>
<wire x1="2" y1="2.127" x2="-2" y2="2.127" width="0.2032" layer="21"/>
<pad name="ANCHOR1" x="-3.5" y="2.5" drill="1.2" diameter="2.2" stop="no"/>
<pad name="ANCHOR2" x="3.5" y="2.5" drill="1.2" diameter="2.2" stop="no"/>
<pad name="1" x="-2.5" y="0" drill="0.8" diameter="1.7" stop="no"/>
<pad name="2" x="2.5" y="0" drill="0.8" diameter="1.7" stop="no"/>
<circle x="2.5" y="0" radius="0.4445" width="0" layer="29"/>
<circle x="-2.5" y="0" radius="0.4445" width="0" layer="29"/>
<circle x="-3.5" y="2.5" radius="0.635" width="0" layer="29"/>
<circle x="3.5" y="2.5" radius="0.635" width="0" layer="29"/>
<circle x="-3.5" y="2.5" radius="1.143" width="0" layer="30"/>
<circle x="2.5" y="0" radius="0.889" width="0" layer="30"/>
<circle x="-2.5" y="0" radius="0.889" width="0" layer="30"/>
<circle x="3.5" y="2.5" radius="1.143" width="0" layer="30"/>
<text x="0" y="2.286" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_12MM" urn="urn:adsk.eagle:footprint:40109/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/N301102.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<wire x1="5" y1="-1.3" x2="5" y2="-0.7" width="0.2032" layer="51"/>
<wire x1="5" y1="-0.7" x2="4.5" y2="-0.2" width="0.2032" layer="51"/>
<wire x1="5" y1="0.2" x2="5" y2="1" width="0.2032" layer="51"/>
<wire x1="-6" y1="4" x2="-6" y2="5" width="0.2032" layer="21"/>
<wire x1="-5" y1="6" x2="5" y2="6" width="0.2032" layer="21"/>
<wire x1="6" y1="5" x2="6" y2="4" width="0.2032" layer="21"/>
<wire x1="6" y1="1" x2="6" y2="-1" width="0.2032" layer="21"/>
<wire x1="6" y1="-4" x2="6" y2="-5" width="0.2032" layer="21"/>
<wire x1="5" y1="-6" x2="-5" y2="-6" width="0.2032" layer="21"/>
<wire x1="-6" y1="-5" x2="-6" y2="-4" width="0.2032" layer="21"/>
<wire x1="-6" y1="-1" x2="-6" y2="1" width="0.2032" layer="21"/>
<wire x1="-6" y1="-5" x2="-5" y2="-6" width="0.2032" layer="21"/>
<wire x1="6" y1="-5" x2="5" y2="-6" width="0.2032" layer="21"/>
<wire x1="6" y1="5" x2="5" y2="6" width="0.2032" layer="21"/>
<wire x1="-5" y1="6" x2="-6" y2="5" width="0.2032" layer="21"/>
<circle x="0" y="0" radius="3.5" width="0.2032" layer="21"/>
<circle x="-4.5" y="4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="4.5" y="4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="4.5" y="-4.5" radius="0.3" width="0.7" layer="21"/>
<circle x="-4.5" y="-4.5" radius="0.3" width="0.7" layer="21"/>
<smd name="4" x="-6.975" y="2.5" dx="1.6" dy="1.55" layer="1"/>
<smd name="2" x="-6.975" y="-2.5" dx="1.6" dy="1.55" layer="1"/>
<smd name="1" x="6.975" y="-2.5" dx="1.6" dy="1.55" layer="1"/>
<smd name="3" x="6.975" y="2.5" dx="1.6" dy="1.55" layer="1"/>
<text x="0" y="6.223" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-6.223" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM_KIT" urn="urn:adsk.eagle:footprint:40110/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
<wire x1="3.048" y1="1.016" x2="3.048" y2="2.54" width="0.2032" layer="51"/>
<wire x1="3.048" y1="2.54" x2="2.54" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.54" y1="-3.048" x2="3.048" y2="-2.54" width="0.2032" layer="51"/>
<wire x1="3.048" y1="-2.54" x2="3.048" y2="-1.016" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="3.048" x2="-3.048" y2="2.54" width="0.2032" layer="51"/>
<wire x1="-3.048" y1="2.54" x2="-3.048" y2="1.016" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-3.048" x2="-3.048" y2="-2.54" width="0.2032" layer="51"/>
<wire x1="-3.048" y1="-2.54" x2="-3.048" y2="-1.016" width="0.2032" layer="51"/>
<wire x1="2.54" y1="-3.048" x2="2.159" y2="-3.048" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-3.048" x2="-2.159" y2="-3.048" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="3.048" x2="-2.159" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.54" y1="3.048" x2="2.159" y2="3.048" width="0.2032" layer="51"/>
<wire x1="2.159" y1="3.048" x2="-2.159" y2="3.048" width="0.2032" layer="21"/>
<wire x1="-2.159" y1="-3.048" x2="2.159" y2="-3.048" width="0.2032" layer="21"/>
<wire x1="3.048" y1="0.998" x2="3.048" y2="-1.016" width="0.2032" layer="21"/>
<wire x1="-3.048" y1="1.028" x2="-3.048" y2="-1.016" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="1.27" x2="-2.54" y2="0.508" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-0.508" x2="-2.54" y2="-1.27" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="0.508" x2="-2.159" y2="-0.381" width="0.2032" layer="51"/>
<circle x="0" y="0" radius="1.778" width="0.2032" layer="21"/>
<pad name="1" x="-3.2512" y="2.2606" drill="1.016" diameter="1.8796" stop="no"/>
<pad name="2" x="3.2512" y="2.2606" drill="1.016" diameter="1.8796" stop="no"/>
<pad name="3" x="-3.2512" y="-2.2606" drill="1.016" diameter="1.8796" stop="no"/>
<pad name="4" x="3.2512" y="-2.2606" drill="1.016" diameter="1.8796" stop="no"/>
<polygon width="0.127" layer="30">
<vertex x="-3.2664" y="3.142"/>
<vertex x="-3.2589" y="3.1445" curve="89.986886"/>
<vertex x="-4.1326" y="2.286"/>
<vertex x="-4.1351" y="2.2657" curve="90.00652"/>
<vertex x="-3.2563" y="1.392"/>
<vertex x="-3.2487" y="1.3869" curve="90.006616"/>
<vertex x="-2.3826" y="2.2403"/>
<vertex x="-2.3775" y="2.2683" curve="89.98711"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-3.2462" y="2.7026"/>
<vertex x="-3.2589" y="2.7051" curve="90.026544"/>
<vertex x="-3.6881" y="2.2733"/>
<vertex x="-3.6881" y="2.2632" curve="89.974074"/>
<vertex x="-3.2562" y="1.8213"/>
<vertex x="-3.2259" y="1.8186" curve="90.051271"/>
<vertex x="-2.8093" y="2.2658"/>
<vertex x="-2.8093" y="2.2606" curve="90.012964"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="3.2411" y="3.1395"/>
<vertex x="3.2486" y="3.142" curve="89.986886"/>
<vertex x="2.3749" y="2.2835"/>
<vertex x="2.3724" y="2.2632" curve="90.00652"/>
<vertex x="3.2512" y="1.3895"/>
<vertex x="3.2588" y="1.3844" curve="90.006616"/>
<vertex x="4.1249" y="2.2378"/>
<vertex x="4.13" y="2.2658" curve="89.98711"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="3.2613" y="2.7001"/>
<vertex x="3.2486" y="2.7026" curve="90.026544"/>
<vertex x="2.8194" y="2.2708"/>
<vertex x="2.8194" y="2.2607" curve="89.974074"/>
<vertex x="3.2513" y="1.8188"/>
<vertex x="3.2816" y="1.8161" curve="90.051271"/>
<vertex x="3.6982" y="2.2633"/>
<vertex x="3.6982" y="2.2581" curve="90.012964"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="-3.2613" y="-1.3868"/>
<vertex x="-3.2538" y="-1.3843" curve="89.986886"/>
<vertex x="-4.1275" y="-2.2428"/>
<vertex x="-4.13" y="-2.2631" curve="90.00652"/>
<vertex x="-3.2512" y="-3.1368"/>
<vertex x="-3.2436" y="-3.1419" curve="90.006616"/>
<vertex x="-2.3775" y="-2.2885"/>
<vertex x="-2.3724" y="-2.2605" curve="89.98711"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-3.2411" y="-1.8262"/>
<vertex x="-3.2538" y="-1.8237" curve="90.026544"/>
<vertex x="-3.683" y="-2.2555"/>
<vertex x="-3.683" y="-2.2656" curve="89.974074"/>
<vertex x="-3.2511" y="-2.7075"/>
<vertex x="-3.2208" y="-2.7102" curve="90.051271"/>
<vertex x="-2.8042" y="-2.263"/>
<vertex x="-2.8042" y="-2.2682" curve="90.012964"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="3.2411" y="-1.3843"/>
<vertex x="3.2486" y="-1.3818" curve="89.986886"/>
<vertex x="2.3749" y="-2.2403"/>
<vertex x="2.3724" y="-2.2606" curve="90.00652"/>
<vertex x="3.2512" y="-3.1343"/>
<vertex x="3.2588" y="-3.1394" curve="90.006616"/>
<vertex x="4.1249" y="-2.286"/>
<vertex x="4.13" y="-2.258" curve="89.98711"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="3.2613" y="-1.8237"/>
<vertex x="3.2486" y="-1.8212" curve="90.026544"/>
<vertex x="2.8194" y="-2.253"/>
<vertex x="2.8194" y="-2.2631" curve="89.974074"/>
<vertex x="3.2513" y="-2.705"/>
<vertex x="3.2816" y="-2.7077" curve="90.051271"/>
<vertex x="3.6982" y="-2.2605"/>
<vertex x="3.6982" y="-2.2657" curve="90.012964"/>
</polygon>
<text x="0" y="3.175" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-3.175" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_5.2MM" urn="urn:adsk.eagle:footprint:40111/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/SMD-Button.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
<wire x1="-1.54" y1="-2.54" x2="-2.54" y2="-1.54" width="0.2032" layer="51"/>
<wire x1="-2.54" y1="-1.24" x2="-2.54" y2="1.27" width="0.2032" layer="21"/>
<wire x1="-2.54" y1="1.54" x2="-1.54" y2="2.54" width="0.2032" layer="51"/>
<wire x1="-1.54" y1="2.54" x2="1.54" y2="2.54" width="0.2032" layer="21"/>
<wire x1="1.54" y1="2.54" x2="2.54" y2="1.54" width="0.2032" layer="51"/>
<wire x1="2.54" y1="1.24" x2="2.54" y2="-1.24" width="0.2032" layer="21"/>
<wire x1="2.54" y1="-1.54" x2="1.54" y2="-2.54" width="0.2032" layer="51"/>
<wire x1="1.54" y1="-2.54" x2="-1.54" y2="-2.54" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="1.905" y2="0.445" width="0.127" layer="51"/>
<wire x1="1.905" y1="0.445" x2="2.16" y2="-0.01" width="0.127" layer="51"/>
<wire x1="1.905" y1="-0.23" x2="1.905" y2="-1.115" width="0.127" layer="51"/>
<circle x="0" y="0" radius="1.27" width="0.2032" layer="21"/>
<smd name="1" x="-2.794" y="1.905" dx="0.762" dy="1.524" layer="1" rot="R90"/>
<smd name="2" x="2.794" y="1.905" dx="0.762" dy="1.524" layer="1" rot="R90"/>
<smd name="3" x="-2.794" y="-1.905" dx="0.762" dy="1.524" layer="1" rot="R90"/>
<smd name="4" x="2.794" y="-1.905" dx="0.762" dy="1.524" layer="1" rot="R90"/>
<text x="0" y="2.667" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_RIGHT_ANGLE" urn="urn:adsk.eagle:footprint:40112/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
<hole x="0" y="0.9" drill="0.7"/>
<hole x="0" y="-0.9" drill="0.7"/>
<smd name="1" x="-1.95" y="0" dx="2" dy="1.1" layer="1" rot="R90"/>
<smd name="2" x="1.95" y="0" dx="2" dy="1.1" layer="1" rot="R90"/>
<wire x1="-2" y1="1.2" x2="-2" y2="1.5" width="0.2032" layer="21"/>
<wire x1="-2" y1="1.5" x2="2" y2="1.5" width="0.2032" layer="21"/>
<wire x1="2" y1="1.5" x2="2" y2="1.2" width="0.2032" layer="21"/>
<wire x1="-2" y1="-1.2" x2="-2" y2="-1.5" width="0.2032" layer="21"/>
<wire x1="-2" y1="-1.5" x2="-0.7" y2="-1.5" width="0.2032" layer="21"/>
<wire x1="-0.7" y1="-1.5" x2="0.7" y2="-1.5" width="0.2032" layer="21"/>
<wire x1="0.7" y1="-1.5" x2="2" y2="-1.5" width="0.2032" layer="21"/>
<wire x1="2" y1="-1.5" x2="2" y2="-1.2" width="0.2032" layer="21"/>
<wire x1="-0.7" y1="-2.1" x2="0.7" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="0.7" y1="-2.1" x2="0.7" y2="-1.5" width="0.2032" layer="21"/>
<wire x1="-0.7" y1="-2.1" x2="-0.7" y2="-1.5" width="0.2032" layer="21"/>
<text x="0" y="1.651" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM" urn="urn:adsk.eagle:footprint:40113/1">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<smd name="3" x="2.05" y="0.8" dx="0.9" dy="1" layer="1"/>
<smd name="2" x="2.05" y="-0.8" dx="0.9" dy="1" layer="1"/>
<smd name="1" x="-2.05" y="-0.8" dx="0.9" dy="1" layer="1"/>
<smd name="4" x="-2.05" y="0.8" dx="0.9" dy="1" layer="1"/>
<wire x1="-2.1" y1="1.4" x2="-2.1" y2="-1.4" width="0.127" layer="51"/>
<wire x1="2.1" y1="-1.4" x2="2.1" y2="1.4" width="0.127" layer="51"/>
<wire x1="-2.1" y1="1.4" x2="2.1" y2="1.4" width="0.127" layer="51"/>
<wire x1="-2.1" y1="-1.4" x2="2.1" y2="-1.4" width="0.127" layer="51"/>
<wire x1="1.338" y1="-1.4" x2="-1.338" y2="-1.4" width="0.2032" layer="21"/>
<wire x1="-1.338" y1="1.4" x2="1.338" y2="1.4" width="0.2032" layer="21"/>
<wire x1="-2.1" y1="0.13" x2="-2.1" y2="-0.13" width="0.2032" layer="21"/>
<wire x1="2.1" y1="-0.13" x2="2.1" y2="0.13" width="0.2032" layer="21"/>
<circle x="0" y="0" radius="0.805" width="0.127" layer="21"/>
<rectangle x1="-2.3" y1="0.5" x2="-2.1" y2="1.1" layer="51"/>
<rectangle x1="-2.3" y1="-1.1" x2="-2.1" y2="-0.5" layer="51"/>
<rectangle x1="2.1" y1="-1.1" x2="2.3" y2="-0.5" layer="51" rot="R180"/>
<rectangle x1="2.1" y1="0.5" x2="2.3" y2="1.1" layer="51" rot="R180"/>
<text x="0" y="1.524" size="0.6096" layer="25" font="vector" ratio="20" align="bottom-center">&gt;Name</text>
<text x="0" y="-1.524" size="0.6096" layer="27" font="vector" ratio="20" align="top-center">&gt;Value</text>
</package>
</packages>
<packages3d>
<package3d name="TACTILE_SWITCH_PTH_6.0MM" urn="urn:adsk.eagle:package:40163/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet (B3F-1000)</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_PTH_6.0MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_4.5MM" urn="urn:adsk.eagle:package:40162/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 4.5mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Dimensional Drawing</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_4.5MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_PTH_12MM" urn="urn:adsk.eagle:package:40164/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - PTH, 12mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet (B3F-5050)</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_PTH_12MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_6.0X3.5MM" urn="urn:adsk.eagle:package:40165/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_6.0X3.5MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_6.2MM_TALL" urn="urn:adsk.eagle:package:40172/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet (ADTSM63NVTR)</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_6.2MM_TALL"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT" urn="urn:adsk.eagle:package:40168/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - PTH, Right-angle
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Dimensional Drawing</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_12MM" urn="urn:adsk.eagle:package:40166/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 12mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_12MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_PTH_6.0MM_KIT" urn="urn:adsk.eagle:package:40170/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Warning: This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
Datasheet (B3F-1000)</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_PTH_6.0MM_KIT"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_5.2MM" urn="urn:adsk.eagle:package:40167/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Dimensional Drawing</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_5.2MM"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_RIGHT_ANGLE" urn="urn:adsk.eagle:package:40169/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, Right-angle
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_RIGHT_ANGLE"/>
</packageinstances>
</package3d>
<package3d name="TACTILE_SWITCH_SMD_4.6X2.8MM" urn="urn:adsk.eagle:package:40176/1" type="box">
<description>Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm
Normally-open (NO) SPST momentary switches (buttons, pushbuttons).
Datasheet</description>
<packageinstances>
<packageinstance name="TACTILE_SWITCH_SMD_4.6X2.8MM"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="SWITCH-MOMENTARY-2">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
<wire x1="1.905" y1="0" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="-2.54" y1="0" x2="1.905" y2="1.27" width="0.254" layer="94"/>
<circle x="-2.54" y="0" radius="0.127" width="0.4064" layer="94"/>
<circle x="2.54" y="0" radius="0.127" width="0.4064" layer="94"/>
<text x="0" y="1.524" size="1.778" layer="95" font="vector" align="bottom-center">&gt;NAME</text>
<text x="0" y="-0.508" size="1.778" layer="96" font="vector" align="top-center">&gt;VALUE</text>
<pin name="1" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="2"/>
<pin name="2" x="5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MOMENTARY-SWITCH-SPST" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-12MM - 12mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9190"&gt;Momentary Pushbutton Switch - 12mm Square&lt;/a&gt; (COM-09190)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-6.0MM, PTH-6.0MM-KIT - 6.0mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/97"&gt;Mini Pushbutton Switch&lt;/a&gt; (COM-00097)&lt;/li&gt;
&lt;li&gt;KIT package intended for soldering kit's - only one side of pads' copper is exposed.&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-RIGHT-ANGLE-KIT - Right-angle, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10791"&gt;Right Angle Tactile Button&lt;/a&gt; - Used on &lt;a href="https://www.sparkfun.com/products/11734"&gt;
SparkFun BigTime Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-12MM - 12mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12993"&gt;Tactile Button - SMD (12mm)&lt;/a&gt; (COM-12993)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.5MM - 4.5mm Square Trackball Switch&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13169"&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.6MMX2.8MM -  4.60mm x 2.80mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-5.2MM, SMD-5.2-REDUNDANT - 5.2mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8720"&gt;Mini Pushbutton Switch - SMD&lt;/a&gt; (COM-08720)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;REDUNDANT package connects both switch circuits together&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.0X3.5MM - 6.0 x 3.5mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8229"&gt;Momentary Reset Switch SMD&lt;/a&gt; (COM-08229)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.2MM-TALL - 6.2mm square, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12992"&gt;Tactile Button - SMD (6mm)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-RIGHT-ANGLE - Right-angle, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2" x="0" y="0"/>
</gates>
<devices>
<device name="-PTH-6.0MM" package="TACTILE_SWITCH_PTH_6.0MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40163/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.5MM" package="TACTILE_SWITCH_SMD_4.5MM">
<connects>
<connect gate="G$1" pin="1" pad="2 3"/>
<connect gate="G$1" pin="2" pad="1 4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40162/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09213"/>
</technology>
</technologies>
</device>
<device name="-PTH-12MM" package="TACTILE_SWITCH_PTH_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40164/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.0X3.5MM" package="TACTILE_SWITCH_SMD_6.0X3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40165/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="SF_SKU" value="COM-08229"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.2MM-TALL" package="TACTILE_SWITCH_SMD_6.2MM_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40172/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</technology>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLE-KIT" package="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40168/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</technology>
</technologies>
</device>
<device name="-SMD-12MM" package="TACTILE_SWITCH_SMD_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40166/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11967"/>
<attribute name="SF_SKU" value="COM-12993"/>
</technology>
</technologies>
</device>
<device name="-PTH-6.0MM-KIT" package="TACTILE_SWITCH_PTH_6.0MM_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40170/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097 "/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40167/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2-REDUNDANT" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40167/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-RIGHT-ANGLE" package="TACTILE_SWITCH_SMD_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40169/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12265" constant="no"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.6X2.8MM" package="TACTILE_SWITCH_SMD_4.6X2.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:40176/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13065"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/HGP" urn="urn:adsk.eagle:footprint:5238/1" locally_modified="yes">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
<pad name="1" x="-3.81" y="0" drill="1.016" diameter="2.159" shape="octagon"/>
<pad name="2" x="3.81" y="0" drill="1.016" diameter="2.159" shape="octagon"/>
<text x="4.445" y="6.985" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-3.683" y="-3.81" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<circle x="0" y="0" radius="6.0827625" width="0.127" layer="21"/>
</package>
</packages>
<packages3d>
<package3d name="F/HGP" urn="urn:adsk.eagle:package:5287/1" type="box">
<description>BUZZER</description>
<packageinstances>
<packageinstance name="F/HGP"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="BWS">
<wire x1="-2.54" y1="5.08" x2="5.08" y2="5.08" width="0.254" layer="94" curve="180"/>
<wire x1="-2.54" y1="5.08" x2="5.08" y2="5.08" width="0.254" layer="94"/>
<wire x1="0" y1="3.175" x2="1.27" y2="3.175" width="0.1524" layer="94" curve="-180" cap="flat"/>
<wire x1="1.27" y1="3.175" x2="2.54" y2="3.175" width="0.1524" layer="94" curve="180" cap="flat"/>
<wire x1="2.54" y1="-2.54" x2="2.54" y2="1.397" width="0.1524" layer="94"/>
<wire x1="0" y1="-2.54" x2="0" y2="1.397" width="0.1524" layer="94"/>
<text x="-2.54" y="6.35" size="1.778" layer="95">&gt;NAME</text>
<text x="6.35" y="0" size="1.778" layer="96">&gt;VALUE</text>
<pin name="2" x="5.08" y="-2.54" visible="pad" length="short" direction="pas" rot="R180"/>
<pin name="1" x="-2.54" y="-2.54" visible="pad" length="short" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="F/HGP" prefix="SG">
<description>&lt;b&gt;BUZZER&lt;/b&gt;&lt;p&gt; Source: Buerklin</description>
<gates>
<gate name="G$1" symbol="BWS" x="0" y="0"/>
</gates>
<devices>
<device name="" package="F/HGP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:5287/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="MF" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OC_FARNELL" value="unknown" constant="no"/>
<attribute name="OC_NEWARK" value="unknown" constant="no"/>
<attribute name="POPULARITY" value="0" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
</class>
</classes>
<parts>
<part name="J1" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="" package3d_urn="urn:adsk.eagle:package:38039/1" value="Break"/>
<part name="J2" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_06" device="SILK_FEMALE_PTH" package3d_urn="urn:adsk.eagle:package:38009/1" value="COMM"/>
<part name="J3" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="" package3d_urn="urn:adsk.eagle:package:38039/1" value="PWR"/>
<part name="J4" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_05" device="" package3d_urn="urn:adsk.eagle:package:38104/1" value="DISPLAY"/>
<part name="J5" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_03" device="" package3d_urn="urn:adsk.eagle:package:38063/1" value="THROTTLE"/>
<part name="C1" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C" device="CHIP-1206(3216-METRIC)" package3d_urn="urn:adsk.eagle:package:16290893/2" technology="_" value="0.1uF"/>
<part name="J6" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="" package3d_urn="urn:adsk.eagle:package:38039/1" value="LED"/>
<part name="Q2" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" deviceset="NMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFET"/>
<part name="R2" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="R1" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="D2" library="Diode" library_urn="urn:adsk.eagle:library:16378169" deviceset="DIODE" device="DO-215-AC" package3d_urn="urn:adsk.eagle:package:9427057/2" technology="_" value=""/>
<part name="Q4" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" deviceset="PMOSFET_" device="" package3d_urn="urn:adsk.eagle:package:28738/2" technology="BSS84" value="BSS84"/>
<part name="D3" library="Diode" library_urn="urn:adsk.eagle:library:16378169" deviceset="DIODE" device="DO-215-AC" package3d_urn="urn:adsk.eagle:package:9427057/2" technology="_" value=""/>
<part name="Q5" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" deviceset="NMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFET"/>
<part name="J7" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_06" device="SILK_FEMALE_PTH" package3d_urn="urn:adsk.eagle:package:38009/1" value="SPEED"/>
<part name="C3" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C" device="CHIP-1206(3216-METRIC)" package3d_urn="urn:adsk.eagle:package:16290893/2" technology="_" value="0.1uF"/>
<part name="Q1" library="Transistor" library_urn="urn:adsk.eagle:library:16378713" deviceset="NMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFET"/>
<part name="D4" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1"/>
<part name="D6" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1"/>
<part name="D7" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1"/>
<part name="D8" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1"/>
<part name="R4" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="R5" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="C2" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C" device="CHIP-1206(3216-METRIC)" package3d_urn="urn:adsk.eagle:package:16290893/2" technology="_" value="0.1uF"/>
<part name="GND1" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND2" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="U1" library="eScooter" deviceset="ARDUINO" device="ARDUINO_NANO" package3d_urn="urn:adsk.eagle:package:21849926/1" value="Arduino Nano Every"/>
<part name="S1" library="SparkFun-Switches" deviceset="MOMENTARY-SWITCH-SPST" device="-PTH-6.0MM" package3d_urn="urn:adsk.eagle:package:40163/1"/>
<part name="SG1" library="buzzer" deviceset="F/HGP" device="" package3d_urn="urn:adsk.eagle:package:5287/1"/>
<part name="R3" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="D1" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1"/>
<part name="GND3" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND4" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND5" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND6" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND7" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND8" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="GND9" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<instances>
<instance part="J1" gate="G$1" x="27.94" y="111.76" smashed="yes">
<attribute name="VALUE" x="25.4" y="106.934" size="1.778" layer="96" font="vector"/>
<attribute name="NAME" x="25.4" y="117.348" size="1.778" layer="95" font="vector"/>
</instance>
<instance part="J2" gate="G$1" x="114.3" y="86.36" smashed="yes" rot="R180">
<attribute name="VALUE" x="119.38" y="96.266" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="119.38" y="75.692" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="J3" gate="G$1" x="-119.38" y="73.66" smashed="yes" rot="MR180">
<attribute name="VALUE" x="-121.92" y="78.486" size="1.778" layer="96" font="vector" rot="MR180"/>
<attribute name="NAME" x="-121.92" y="68.072" size="1.778" layer="95" font="vector" rot="MR180"/>
</instance>
<instance part="J4" gate="G$1" x="116.84" y="38.1" smashed="yes" rot="MR0">
<attribute name="VALUE" x="119.634" y="33.02" size="1.778" layer="96" font="vector" rot="MR90"/>
<attribute name="NAME" x="119.38" y="46.228" size="1.778" layer="95" font="vector" rot="MR0"/>
</instance>
<instance part="J5" gate="J$1" x="-10.16" y="111.76" smashed="yes" rot="MR180">
<attribute name="VALUE" x="-15.24" y="106.426" size="1.778" layer="96" font="vector" rot="MR180"/>
<attribute name="NAME" x="-12.7" y="118.872" size="1.778" layer="95" font="vector" rot="MR180"/>
</instance>
<instance part="C1" gate="G$1" x="-25.4" y="109.22" smashed="yes" rot="R180">
<attribute name="NAME" x="-27.94" y="109.22" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="-27.94" y="114.3" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="J6" gate="G$1" x="116.84" y="22.86" smashed="yes" rot="R180">
<attribute name="VALUE" x="119.38" y="17.526" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="119.38" y="27.432" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="Q2" gate="G$1" x="-76.2" y="73.66" smashed="yes" rot="MR0">
<attribute name="NAME" x="-85.09" y="69.85" size="1.778" layer="95"/>
<attribute name="VALUE" x="-85.09" y="77.47" size="1.778" layer="96"/>
</instance>
<instance part="R2" gate="G$1" x="-93.98" y="73.66" smashed="yes" rot="MR0">
<attribute name="NAME" x="-90.17" y="75.1586" size="1.778" layer="95" rot="MR0"/>
<attribute name="VALUE" x="-90.17" y="70.358" size="1.778" layer="96" rot="MR0"/>
</instance>
<instance part="R1" gate="G$1" x="-71.12" y="66.04" smashed="yes" rot="MR180">
<attribute name="NAME" x="-74.93" y="64.5414" size="1.778" layer="95" rot="MR180"/>
<attribute name="VALUE" x="-74.93" y="69.342" size="1.778" layer="96" rot="MR180"/>
</instance>
<instance part="D2" gate="G$1" x="-86.36" y="63.5" smashed="yes" rot="MR270">
<attribute name="NAME" x="-91.44" y="63.5" size="1.778" layer="95" rot="MR180" align="center"/>
<attribute name="VALUE" x="-81.28" y="63.5" size="1.778" layer="95" rot="MR270" align="center"/>
</instance>
<instance part="Q4" gate="G$1" x="-99.06" y="81.28" smashed="yes" rot="R180">
<attribute name="NAME" x="-105.41" y="80.01" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="-105.41" y="82.55" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="D3" gate="G$1" x="-71.12" y="43.18" smashed="yes" rot="MR0">
<attribute name="NAME" x="-71.12" y="40.64" size="1.778" layer="95" rot="MR0" align="center"/>
<attribute name="VALUE" x="-71.12" y="38.1" size="1.778" layer="95" rot="MR0" align="center"/>
</instance>
<instance part="Q5" gate="G$1" x="83.82" y="71.12" smashed="yes" rot="MR270">
<attribute name="NAME" x="82.55" y="64.77" size="1.778" layer="95" rot="MR270"/>
</instance>
<instance part="J7" gate="G$1" x="-78.74" y="109.22" smashed="yes">
<attribute name="VALUE" x="-83.82" y="99.314" size="1.778" layer="96" font="vector"/>
<attribute name="NAME" x="-83.82" y="119.888" size="1.778" layer="95" font="vector"/>
</instance>
<instance part="C3" gate="G$1" x="-58.42" y="116.84" smashed="yes" rot="MR270">
<attribute name="NAME" x="-55.88" y="114.3" size="1.778" layer="95" rot="R270"/>
<attribute name="VALUE" x="-58.42" y="114.3" size="1.778" layer="96" rot="MR270"/>
</instance>
<instance part="Q1" gate="G$1" x="101.6" y="12.7" smashed="yes">
<attribute name="NAME" x="118.11" y="13.97" size="1.778" layer="95"/>
</instance>
<instance part="D4" gate="D$1" x="-17.78" y="111.76" smashed="yes" rot="R180">
<attribute name="NAME" x="-20.32" y="109.22" size="1.778" layer="95" rot="R180"/>
</instance>
<instance part="D6" gate="D$1" x="-63.5" y="104.14" smashed="yes" rot="R270">
<attribute name="NAME" x="-63.5" y="101.6" size="1.778" layer="95" rot="R180"/>
</instance>
<instance part="D7" gate="D$1" x="-58.42" y="63.5" smashed="yes" rot="MR0">
<attribute name="NAME" x="-60.96" y="63.5" size="1.778" layer="95" rot="MR0"/>
</instance>
<instance part="D8" gate="D$1" x="-71.12" y="50.8" smashed="yes" rot="MR90">
<attribute name="NAME" x="-71.12" y="53.34" size="1.778" layer="95" rot="MR0"/>
</instance>
<instance part="R4" gate="G$1" x="99.06" y="68.58" smashed="yes">
<attribute name="NAME" x="95.25" y="70.0786" size="1.778" layer="95"/>
<attribute name="VALUE" x="95.25" y="65.278" size="1.778" layer="96"/>
</instance>
<instance part="R5" gate="G$1" x="96.52" y="2.54" smashed="yes" rot="R90">
<attribute name="NAME" x="95.0214" y="-1.27" size="1.778" layer="95" rot="R90"/>
<attribute name="VALUE" x="99.822" y="-1.27" size="1.778" layer="96" rot="R90"/>
</instance>
<instance part="C2" gate="G$1" x="124.46" y="81.28" smashed="yes">
<attribute name="NAME" x="129.54" y="78.74" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="129.54" y="83.82" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="GND1" gate="1" x="104.14" y="-10.16" smashed="yes">
<attribute name="VALUE" x="101.6" y="-12.7" size="1.778" layer="96"/>
</instance>
<instance part="GND2" gate="1" x="-22.86" y="35.56" smashed="yes">
<attribute name="VALUE" x="-25.4" y="33.02" size="1.778" layer="96"/>
</instance>
<instance part="U1" gate="G$1" x="10.16" y="63.5" smashed="yes">
<attribute name="NAME" x="10.16" y="86.36" size="1.778" layer="95"/>
<attribute name="VALUE" x="0" y="40.64" size="1.778" layer="96"/>
</instance>
<instance part="S1" gate="G$1" x="-78.74" y="55.88" smashed="yes" rot="MR0">
<attribute name="NAME" x="-78.74" y="57.404" size="1.778" layer="95" font="vector" rot="MR0" align="bottom-center"/>
</instance>
<instance part="SG1" gate="G$1" x="55.88" y="2.54" smashed="yes" rot="MR90">
<attribute name="NAME" x="62.23" y="0" size="1.778" layer="95" rot="MR90"/>
</instance>
<instance part="R3" gate="G$1" x="60.96" y="114.3" smashed="yes" rot="R180">
<attribute name="NAME" x="64.77" y="112.8014" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="64.77" y="117.602" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="D1" gate="D$1" x="45.72" y="111.76" smashed="yes" rot="R90">
<attribute name="NAME" x="43.18" y="106.68" size="1.778" layer="95"/>
</instance>
<instance part="GND3" gate="1" x="-104.14" y="35.56" smashed="yes">
<attribute name="VALUE" x="-106.68" y="33.02" size="1.778" layer="96"/>
</instance>
<instance part="GND4" gate="1" x="5.08" y="96.52" smashed="yes">
<attribute name="VALUE" x="2.54" y="93.98" size="1.778" layer="96"/>
</instance>
<instance part="GND5" gate="1" x="-71.12" y="96.52" smashed="yes">
<attribute name="VALUE" x="-73.66" y="93.98" size="1.778" layer="96"/>
</instance>
<instance part="GND6" gate="1" x="53.34" y="-10.16" smashed="yes">
<attribute name="VALUE" x="50.8" y="-12.7" size="1.778" layer="96"/>
</instance>
<instance part="GND7" gate="1" x="40.64" y="96.52" smashed="yes">
<attribute name="VALUE" x="38.1" y="93.98" size="1.778" layer="96"/>
</instance>
<instance part="GND8" gate="1" x="124.46" y="53.34" smashed="yes">
<attribute name="VALUE" x="121.92" y="50.8" size="1.778" layer="96"/>
</instance>
<instance part="GND9" gate="1" x="76.2" y="-10.16" smashed="yes">
<attribute name="VALUE" x="73.66" y="-12.7" size="1.778" layer="96"/>
</instance>
</instances>
<busses>
<bus name="I2C:GND,SCL,SDA">
<segment>
<wire x1="-38.1" y1="116.84" x2="-38.1" y2="45.72" width="0.762" layer="92"/>
</segment>
</bus>
<bus name="SPI:CLK,CS,DIN,GND">
<segment>
<wire x1="58.42" y1="81.28" x2="58.42" y2="33.02" width="0.762" layer="92"/>
</segment>
</bus>
</busses>
<nets>
<net name="GND" class="0">
<segment>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="D4" gate="D$1" pin="P$1"/>
<wire x1="-25.4" y1="101.6" x2="-25.4" y2="106.68" width="0.1524" layer="91"/>
<wire x1="-17.78" y1="101.6" x2="-17.78" y2="107.696" width="0.1524" layer="91"/>
<pinref part="J5" gate="J$1" pin="3"/>
<wire x1="-2.54" y1="109.22" x2="5.08" y2="109.22" width="0.1524" layer="91"/>
<wire x1="5.08" y1="109.22" x2="5.08" y2="101.6" width="0.1524" layer="91"/>
<pinref part="GND4" gate="1" pin="GND"/>
<wire x1="5.08" y1="99.06" x2="5.08" y2="101.6" width="0.1524" layer="91"/>
<label x="-2.54" y="109.22" size="1.778" layer="95"/>
<wire x1="-25.4" y1="101.6" x2="-17.78" y2="101.6" width="0.1524" layer="91"/>
<junction x="-17.78" y="101.6"/>
<wire x1="-17.78" y1="101.6" x2="5.08" y2="101.6" width="0.1524" layer="91"/>
<junction x="5.08" y="101.6"/>
</segment>
<segment>
<pinref part="SG1" gate="G$1" pin="1"/>
<pinref part="GND6" gate="1" pin="GND"/>
<wire x1="53.34" y1="-7.62" x2="53.34" y2="0" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="J7" gate="G$1" pin="1"/>
<wire x1="-73.66" y1="104.14" x2="-71.12" y2="104.14" width="0.1524" layer="91"/>
<pinref part="D6" gate="D$1" pin="P$2"/>
<wire x1="-67.564" y1="104.14" x2="-68.58" y2="104.14" width="0.1524" layer="91"/>
<wire x1="-68.58" y1="104.14" x2="-71.12" y2="104.14" width="0.1524" layer="91"/>
<junction x="-71.12" y="104.14"/>
<wire x1="-71.12" y1="104.14" x2="-71.12" y2="99.06" width="0.1524" layer="91"/>
<label x="-71.12" y="104.14" size="1.778" layer="95" rot="MR0"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="J3" gate="G$1" pin="2"/>
<wire x1="-111.76" y1="71.12" x2="-104.14" y2="71.12" width="0.1524" layer="91"/>
<wire x1="-104.14" y1="71.12" x2="-104.14" y2="38.1" width="0.1524" layer="91"/>
<label x="-106.68" y="71.12" size="1.778" layer="95" rot="MR0"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="J1" gate="G$1" pin="1"/>
<wire x1="35.56" y1="111.76" x2="38.1" y2="111.76" width="0.1524" layer="91"/>
<wire x1="38.1" y1="111.76" x2="40.64" y2="111.76" width="0.1524" layer="91"/>
<pinref part="D1" gate="D$1" pin="P$1"/>
<wire x1="41.656" y1="111.76" x2="43.18" y2="111.76" width="0.1524" layer="91"/>
<wire x1="43.18" y1="111.76" x2="40.64" y2="111.76" width="0.1524" layer="91"/>
<junction x="40.64" y="111.76"/>
<wire x1="40.64" y1="111.76" x2="40.64" y2="99.06" width="0.1524" layer="91"/>
<label x="35.56" y="111.76" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="Q5" gate="G$1" pin="S"/>
<wire x1="88.9" y1="68.58" x2="91.44" y2="68.58" width="0.1524" layer="91"/>
<wire x1="91.44" y1="68.58" x2="93.98" y2="68.58" width="0.1524" layer="91"/>
<junction x="91.44" y="68.58"/>
<pinref part="GND8" gate="1" pin="GND"/>
<wire x1="124.46" y1="55.88" x2="124.46" y2="63.5" width="0.1524" layer="91"/>
<wire x1="124.46" y1="63.5" x2="91.44" y2="63.5" width="0.1524" layer="91"/>
<wire x1="91.44" y1="63.5" x2="91.44" y2="68.58" width="0.1524" layer="91"/>
<junction x="124.46" y="63.5"/>
<pinref part="C2" gate="G$1" pin="2"/>
<wire x1="124.46" y1="76.2" x2="124.46" y2="63.5" width="0.1524" layer="91"/>
</segment>
<segment>
<wire x1="104.14" y1="7.62" x2="104.14" y2="-5.08" width="0.1524" layer="91"/>
<pinref part="Q1" gate="G$1" pin="S"/>
<pinref part="R5" gate="G$1" pin="1"/>
<wire x1="96.52" y1="-2.54" x2="96.52" y2="-5.08" width="0.1524" layer="91"/>
<wire x1="96.52" y1="-5.08" x2="104.14" y2="-5.08" width="0.1524" layer="91"/>
<junction x="104.14" y="-5.08"/>
<wire x1="104.14" y1="-5.08" x2="104.14" y2="-7.62" width="0.1524" layer="91"/>
<pinref part="GND1" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="J7" gate="G$1" pin="5"/>
<label x="-68.58" y="114.3" size="1.778" layer="95" rot="MR0"/>
<wire x1="-73.66" y1="114.3" x2="-50.8" y2="114.3" width="0.1524" layer="91"/>
<wire x1="-50.8" y1="114.3" x2="-50.8" y2="116.84" width="0.1524" layer="91"/>
<wire x1="-50.8" y1="116.84" x2="-53.34" y2="116.84" width="0.1524" layer="91"/>
<pinref part="C3" gate="G$1" pin="2"/>
<junction x="-50.8" y="114.3"/>
<wire x1="-38.1" y1="111.76" x2="-43.18" y2="114.3" width="0.1524" layer="91"/>
<wire x1="-50.8" y1="114.3" x2="-43.18" y2="114.3" width="0.1524" layer="91"/>
<label x="-48.26" y="114.3" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="S1" gate="G$1" pin="1"/>
<wire x1="-73.66" y1="55.88" x2="-63.5" y2="55.88" width="0.1524" layer="91"/>
<pinref part="Q2" gate="G$1" pin="S"/>
<wire x1="-78.74" y1="66.04" x2="-78.74" y2="68.58" width="0.1524" layer="91"/>
<pinref part="R1" gate="G$1" pin="1"/>
<wire x1="-76.2" y1="66.04" x2="-78.74" y2="66.04" width="0.1524" layer="91"/>
<junction x="-78.74" y="66.04"/>
<wire x1="-78.74" y1="60.96" x2="-78.74" y2="66.04" width="0.1524" layer="91"/>
<wire x1="-63.5" y1="60.96" x2="-78.74" y2="60.96" width="0.1524" layer="91"/>
<wire x1="-63.5" y1="60.96" x2="-63.5" y2="55.88" width="0.1524" layer="91"/>
<junction x="-63.5" y="55.88"/>
<pinref part="D8" gate="D$1" pin="P$1"/>
<wire x1="-58.42" y1="50.8" x2="-67.056" y2="50.8" width="0.1524" layer="91"/>
<pinref part="D7" gate="D$1" pin="P$2"/>
<wire x1="-58.42" y1="59.436" x2="-58.42" y2="55.88" width="0.1524" layer="91"/>
<wire x1="-58.42" y1="55.88" x2="-58.42" y2="50.8" width="0.1524" layer="91"/>
<wire x1="-58.42" y1="55.88" x2="-63.5" y2="55.88" width="0.1524" layer="91"/>
<junction x="-58.42" y="55.88"/>
<wire x1="-58.42" y1="55.88" x2="-53.34" y2="55.88" width="0.1524" layer="91"/>
<label x="-53.34" y="55.88" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<wire x1="-38.1" y1="50.8" x2="-33.02" y2="48.26" width="0.1524" layer="91"/>
<wire x1="-33.02" y1="48.26" x2="-22.86" y2="48.26" width="0.1524" layer="91"/>
<label x="-30.48" y="48.26" size="1.778" layer="95"/>
<wire x1="-5.08" y1="48.26" x2="-17.78" y2="48.26" width="0.1524" layer="91"/>
<label x="-10.16" y="48.26" size="1.778" layer="95"/>
<wire x1="-17.78" y1="48.26" x2="-22.86" y2="48.26" width="0.1524" layer="91"/>
<wire x1="-22.86" y1="48.26" x2="-22.86" y2="38.1" width="0.1524" layer="91"/>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="U1" gate="G$1" pin="GND"/>
<junction x="-22.86" y="48.26"/>
</segment>
<segment>
<wire x1="58.42" y1="38.1" x2="63.5" y2="35.56" width="0.1524" layer="91"/>
<label x="66.04" y="35.56" size="1.778" layer="95"/>
<pinref part="J4" gate="G$1" pin="2"/>
<wire x1="63.5" y1="35.56" x2="76.2" y2="35.56" width="0.1524" layer="91"/>
<label x="104.14" y="35.56" size="1.778" layer="95"/>
<wire x1="76.2" y1="35.56" x2="109.22" y2="35.56" width="0.1524" layer="91"/>
<wire x1="76.2" y1="35.56" x2="76.2" y2="-7.62" width="0.1524" layer="91"/>
<junction x="76.2" y="35.56"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
</net>
<net name="VIN" class="0">
<segment>
<pinref part="Q4" gate="G$1" pin="D"/>
<wire x1="-101.6" y1="86.36" x2="-101.6" y2="88.9" width="0.1524" layer="91"/>
<wire x1="-101.6" y1="88.9" x2="-53.34" y2="88.9" width="0.1524" layer="91"/>
<label x="-96.52" y="86.36" size="1.778" layer="95" rot="MR0"/>
<label x="-53.34" y="88.9" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="VIN"/>
<wire x1="-5.08" y1="45.72" x2="-7.62" y2="45.72" width="0.1524" layer="91"/>
<label x="-7.62" y="45.72" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="DIN" class="0">
<segment>
<wire x1="58.42" y1="73.66" x2="53.34" y2="76.2" width="0.1524" layer="91"/>
<label x="48.26" y="76.2" size="1.778" layer="95"/>
<label x="25.4" y="76.2" size="1.778" layer="95"/>
<pinref part="U1" gate="G$1" pin="D10"/>
<wire x1="25.4" y1="76.2" x2="53.34" y2="76.2" width="0.1524" layer="91"/>
</segment>
<segment>
<wire x1="58.42" y1="40.64" x2="63.5" y2="38.1" width="0.1524" layer="91"/>
<label x="66.04" y="38.1" size="1.778" layer="95"/>
<pinref part="J4" gate="G$1" pin="3"/>
<wire x1="63.5" y1="38.1" x2="109.22" y2="38.1" width="0.1524" layer="91"/>
<label x="104.14" y="38.1" size="1.778" layer="95"/>
</segment>
</net>
<net name="CS" class="0">
<segment>
<wire x1="58.42" y1="76.2" x2="53.34" y2="78.74" width="0.1524" layer="91"/>
<label x="48.26" y="78.74" size="1.778" layer="95"/>
<label x="25.4" y="78.74" size="1.778" layer="95"/>
<pinref part="U1" gate="G$1" pin="D11"/>
<wire x1="53.34" y1="78.74" x2="25.4" y2="78.74" width="0.1524" layer="91"/>
</segment>
<segment>
<wire x1="58.42" y1="43.18" x2="63.5" y2="40.64" width="0.1524" layer="91"/>
<label x="66.04" y="40.64" size="1.778" layer="95"/>
<pinref part="J4" gate="G$1" pin="4"/>
<wire x1="63.5" y1="40.64" x2="109.22" y2="40.64" width="0.1524" layer="91"/>
<label x="104.14" y="40.64" size="1.778" layer="95"/>
</segment>
</net>
<net name="CLK" class="0">
<segment>
<wire x1="58.42" y1="78.74" x2="53.34" y2="81.28" width="0.1524" layer="91"/>
<label x="48.26" y="81.28" size="1.778" layer="95"/>
<label x="25.4" y="81.28" size="1.778" layer="95"/>
<pinref part="U1" gate="G$1" pin="D12"/>
<wire x1="25.4" y1="81.28" x2="53.34" y2="81.28" width="0.1524" layer="91"/>
</segment>
<segment>
<wire x1="58.42" y1="45.72" x2="63.5" y2="43.18" width="0.1524" layer="91"/>
<label x="66.04" y="43.18" size="1.778" layer="95"/>
<wire x1="63.5" y1="43.18" x2="109.22" y2="43.18" width="0.1524" layer="91"/>
<pinref part="J4" gate="G$1" pin="5"/>
<label x="104.14" y="43.18" size="1.778" layer="95"/>
</segment>
</net>
<net name="5V" class="0">
<segment>
<pinref part="J6" gate="G$1" pin="1"/>
<wire x1="109.22" y1="22.86" x2="93.98" y2="22.86" width="0.1524" layer="91"/>
<label x="93.98" y="22.86" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="J4" gate="G$1" pin="1"/>
<wire x1="109.22" y1="33.02" x2="93.98" y2="33.02" width="0.1524" layer="91"/>
<label x="93.98" y="33.02" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<wire x1="-5.08" y1="53.34" x2="-7.62" y2="53.34" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="5V"/>
<label x="-7.62" y="53.34" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="J5" gate="J$1" pin="2"/>
<wire x1="-2.54" y1="111.76" x2="10.16" y2="111.76" width="0.1524" layer="91"/>
<label x="-2.54" y="111.76" size="1.778" layer="95"/>
<label x="10.16" y="111.76" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="J7" gate="G$1" pin="2"/>
<wire x1="-73.66" y1="106.68" x2="-68.58" y2="106.68" width="0.1524" layer="91"/>
<label x="-71.12" y="106.68" size="1.778" layer="95" rot="MR0"/>
<wire x1="-68.58" y1="106.68" x2="-55.88" y2="106.68" width="0.1524" layer="91"/>
<label x="-53.34" y="106.68" size="1.778" layer="95" xref="yes"/>
<pinref part="D6" gate="D$1" pin="P$1"/>
<wire x1="-55.88" y1="106.68" x2="-53.34" y2="106.68" width="0.1524" layer="91"/>
<wire x1="-55.88" y1="104.14" x2="-59.436" y2="104.14" width="0.1524" layer="91"/>
<wire x1="-55.88" y1="104.14" x2="-55.88" y2="106.68" width="0.1524" layer="91"/>
<junction x="-55.88" y="106.68"/>
</segment>
</net>
<net name="THIN" class="0">
<segment>
<pinref part="J5" gate="J$1" pin="1"/>
<label x="-2.54" y="114.3" size="1.778" layer="95"/>
<pinref part="C1" gate="G$1" pin="2"/>
<pinref part="D4" gate="D$1" pin="P$2"/>
<wire x1="-25.4" y1="119.38" x2="-25.4" y2="114.3" width="0.1524" layer="91"/>
<wire x1="-2.54" y1="114.3" x2="5.08" y2="114.3" width="0.1524" layer="91"/>
<wire x1="5.08" y1="114.3" x2="5.08" y2="119.38" width="0.1524" layer="91"/>
<wire x1="-17.78" y1="119.38" x2="-17.78" y2="115.824" width="0.1524" layer="91"/>
<label x="10.16" y="119.38" size="1.778" layer="95" xref="yes"/>
<wire x1="-25.4" y1="119.38" x2="-17.78" y2="119.38" width="0.1524" layer="91"/>
<junction x="-17.78" y="119.38"/>
<wire x1="-17.78" y1="119.38" x2="5.08" y2="119.38" width="0.1524" layer="91"/>
<wire x1="5.08" y1="119.38" x2="10.16" y2="119.38" width="0.1524" layer="91"/>
<junction x="5.08" y="119.38"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="A0"/>
<wire x1="-7.62" y1="73.66" x2="-5.08" y2="73.66" width="0.1524" layer="91"/>
<label x="-7.62" y="73.66" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="SDA" class="0">
<segment>
<pinref part="J7" gate="G$1" pin="3"/>
<label x="-68.58" y="109.22" size="1.778" layer="95" rot="MR0"/>
<wire x1="-73.66" y1="109.22" x2="-43.18" y2="109.22" width="0.1524" layer="91"/>
<wire x1="-38.1" y1="106.68" x2="-43.18" y2="109.22" width="0.1524" layer="91"/>
<label x="-48.26" y="109.22" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="A4"/>
<wire x1="-12.7" y1="63.5" x2="-5.08" y2="63.5" width="0.1524" layer="91"/>
<label x="-10.16" y="63.5" size="1.778" layer="95"/>
<wire x1="-38.1" y1="66.04" x2="-33.02" y2="63.5" width="0.1524" layer="91"/>
<wire x1="-33.02" y1="63.5" x2="-22.86" y2="63.5" width="0.1524" layer="91"/>
<label x="-30.48" y="63.5" size="1.778" layer="95"/>
<wire x1="-25.4" y1="63.5" x2="-22.86" y2="63.5" width="0.1524" layer="91"/>
<wire x1="-25.4" y1="63.5" x2="-12.7" y2="63.5" width="0.1524" layer="91"/>
</segment>
</net>
<net name="SCL" class="0">
<segment>
<pinref part="J7" gate="G$1" pin="4"/>
<wire x1="-73.66" y1="111.76" x2="-43.18" y2="111.76" width="0.1524" layer="91"/>
<label x="-68.58" y="111.76" size="1.778" layer="95" rot="MR0"/>
<wire x1="-38.1" y1="109.22" x2="-43.18" y2="111.76" width="0.1524" layer="91"/>
<label x="-48.26" y="111.76" size="1.778" layer="95"/>
</segment>
<segment>
<wire x1="-38.1" y1="63.5" x2="-33.02" y2="60.96" width="0.1524" layer="91"/>
<wire x1="-33.02" y1="60.96" x2="-22.86" y2="60.96" width="0.1524" layer="91"/>
<label x="-30.48" y="60.96" size="1.778" layer="95"/>
<wire x1="-12.7" y1="60.96" x2="-5.08" y2="60.96" width="0.1524" layer="91"/>
<label x="-10.16" y="60.96" size="1.778" layer="95"/>
<pinref part="U1" gate="G$1" pin="A5"/>
<wire x1="-12.7" y1="60.96" x2="-22.86" y2="60.96" width="0.1524" layer="91"/>
</segment>
</net>
<net name="SP" class="0">
<segment>
<wire x1="25.4" y1="58.42" x2="27.94" y2="58.42" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="D3"/>
<label x="27.94" y="58.42" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="Q5" gate="G$1" pin="D"/>
<wire x1="78.74" y1="68.58" x2="76.2" y2="68.58" width="0.1524" layer="91"/>
<label x="76.2" y="68.58" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="STCTL" class="0">
<segment>
<pinref part="J2" gate="G$1" pin="4"/>
<label x="86.36" y="83.82" size="1.778" layer="95" rot="R180" xref="yes"/>
<wire x1="86.36" y1="83.82" x2="109.22" y2="83.82" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="J1" gate="G$1" pin="2"/>
<wire x1="35.56" y1="114.3" x2="53.34" y2="114.3" width="0.1524" layer="91"/>
<pinref part="R3" gate="G$1" pin="2"/>
<label x="35.56" y="114.3" size="1.778" layer="95"/>
<wire x1="53.34" y1="114.3" x2="55.88" y2="114.3" width="0.1524" layer="91"/>
<pinref part="D1" gate="D$1" pin="P$2"/>
<wire x1="49.784" y1="111.76" x2="53.34" y2="111.76" width="0.1524" layer="91"/>
<wire x1="53.34" y1="111.76" x2="53.34" y2="114.3" width="0.1524" layer="91"/>
<junction x="53.34" y="114.3"/>
</segment>
</net>
<net name="BTN" class="0">
<segment>
<pinref part="D3" gate="G$1" pin="A"/>
<wire x1="-53.34" y1="43.18" x2="-66.04" y2="43.18" width="0.1524" layer="91"/>
<label x="-53.34" y="43.18" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<wire x1="25.4" y1="68.58" x2="38.1" y2="68.58" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="D7"/>
<label x="38.1" y="68.58" size="1.778" layer="95" xref="yes"/>
</segment>
</net>
<net name="BAT" class="0">
<segment>
<wire x1="-5.08" y1="68.58" x2="-7.62" y2="68.58" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="A2"/>
<label x="-7.62" y="68.58" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="2"/>
<wire x1="109.22" y1="88.9" x2="93.98" y2="88.9" width="0.1524" layer="91"/>
<pinref part="C2" gate="G$1" pin="1"/>
<wire x1="93.98" y1="88.9" x2="93.98" y2="99.06" width="0.1524" layer="91"/>
<wire x1="93.98" y1="99.06" x2="124.46" y2="99.06" width="0.1524" layer="91"/>
<wire x1="124.46" y1="99.06" x2="124.46" y2="83.82" width="0.1524" layer="91"/>
<label x="86.36" y="88.9" size="1.778" layer="95" rot="R180" xref="yes"/>
<wire x1="86.36" y1="88.9" x2="93.98" y2="88.9" width="0.1524" layer="91"/>
<junction x="93.98" y="88.9"/>
</segment>
</net>
<net name="SPEED" class="0">
<segment>
<pinref part="J2" gate="G$1" pin="6"/>
<pinref part="Q5" gate="G$1" pin="G"/>
<wire x1="86.36" y1="73.66" x2="86.36" y2="78.74" width="0.1524" layer="91"/>
<wire x1="104.14" y1="68.58" x2="106.68" y2="68.58" width="0.1524" layer="91"/>
<pinref part="R4" gate="G$1" pin="2"/>
<wire x1="86.36" y1="78.74" x2="106.68" y2="78.74" width="0.1524" layer="91"/>
<wire x1="106.68" y1="78.74" x2="109.22" y2="78.74" width="0.1524" layer="91"/>
<wire x1="106.68" y1="68.58" x2="106.68" y2="78.74" width="0.1524" layer="91"/>
<junction x="106.68" y="78.74"/>
</segment>
</net>
<net name="LEDCTL" class="0">
<segment>
<wire x1="25.4" y1="73.66" x2="38.1" y2="73.66" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="D9"/>
<label x="38.1" y="73.66" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="Q1" gate="G$1" pin="G"/>
<pinref part="R5" gate="G$1" pin="2"/>
<wire x1="99.06" y1="10.16" x2="96.52" y2="10.16" width="0.1524" layer="91"/>
<wire x1="96.52" y1="10.16" x2="93.98" y2="10.16" width="0.1524" layer="91"/>
<wire x1="96.52" y1="7.62" x2="96.52" y2="10.16" width="0.1524" layer="91"/>
<junction x="96.52" y="10.16"/>
<label x="93.98" y="10.16" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="STLEDCTL" class="0">
<segment>
<wire x1="25.4" y1="60.96" x2="38.1" y2="60.96" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="D4"/>
<label x="38.1" y="60.96" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="5"/>
<wire x1="76.2" y1="81.28" x2="109.22" y2="81.28" width="0.1524" layer="91"/>
<label x="76.2" y="81.28" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="N$1" class="0">
<segment>
<pinref part="J6" gate="G$1" pin="2"/>
<wire x1="109.22" y1="20.32" x2="104.14" y2="20.32" width="0.1524" layer="91"/>
<wire x1="104.14" y1="20.32" x2="104.14" y2="17.78" width="0.1524" layer="91"/>
<pinref part="Q1" gate="G$1" pin="D"/>
</segment>
</net>
<net name="PWON" class="0">
<segment>
<pinref part="Q2" gate="G$1" pin="G"/>
<pinref part="R1" gate="G$1" pin="2"/>
<wire x1="-73.66" y1="71.12" x2="-63.5" y2="71.12" width="0.1524" layer="91"/>
<wire x1="-58.42" y1="67.564" x2="-58.42" y2="71.12" width="0.1524" layer="91"/>
<wire x1="-58.42" y1="71.12" x2="-53.34" y2="71.12" width="0.1524" layer="91"/>
<wire x1="-63.5" y1="71.12" x2="-63.5" y2="66.04" width="0.1524" layer="91"/>
<junction x="-63.5" y="71.12"/>
<wire x1="-63.5" y1="66.04" x2="-66.04" y2="66.04" width="0.1524" layer="91"/>
<pinref part="D7" gate="D$1" pin="P$1"/>
<wire x1="-58.42" y1="71.12" x2="-63.5" y2="71.12" width="0.1524" layer="91"/>
<junction x="-58.42" y="71.12"/>
<label x="-53.34" y="71.12" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="D8"/>
<label x="27.94" y="71.12" size="1.778" layer="95" xref="yes"/>
<wire x1="25.4" y1="71.12" x2="27.94" y2="71.12" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="3"/>
<label x="76.2" y="86.36" size="1.778" layer="95" rot="R180" xref="yes"/>
<wire x1="109.22" y1="86.36" x2="76.2" y2="86.36" width="0.1524" layer="91"/>
</segment>
</net>
<net name="12V" class="0">
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="Q4" gate="G$1" pin="S"/>
<wire x1="-101.6" y1="76.2" x2="-101.6" y2="73.66" width="0.1524" layer="91"/>
<wire x1="-101.6" y1="73.66" x2="-99.06" y2="73.66" width="0.1524" layer="91"/>
<pinref part="J3" gate="G$1" pin="1"/>
<wire x1="-111.76" y1="73.66" x2="-101.6" y2="73.66" width="0.1524" layer="91"/>
<junction x="-101.6" y="73.66"/>
<label x="-106.68" y="73.66" size="1.778" layer="95" rot="MR0"/>
</segment>
</net>
<net name="N$2" class="0">
<segment>
<pinref part="Q4" gate="G$1" pin="G"/>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="Q2" gate="G$1" pin="D"/>
<wire x1="-86.36" y1="78.74" x2="-78.74" y2="78.74" width="0.1524" layer="91"/>
<junction x="-86.36" y="78.74"/>
<wire x1="-96.52" y1="78.74" x2="-86.36" y2="78.74" width="0.1524" layer="91"/>
<pinref part="D2" gate="G$1" pin="A"/>
<wire x1="-86.36" y1="68.58" x2="-86.36" y2="73.66" width="0.1524" layer="91"/>
<junction x="-86.36" y="78.74"/>
<wire x1="-86.36" y1="73.66" x2="-86.36" y2="78.74" width="0.1524" layer="91"/>
<wire x1="-88.9" y1="73.66" x2="-86.36" y2="73.66" width="0.1524" layer="91"/>
<junction x="-86.36" y="73.66"/>
</segment>
</net>
<net name="N$5" class="0">
<segment>
<pinref part="D3" gate="G$1" pin="C"/>
<pinref part="D2" gate="G$1" pin="C"/>
<wire x1="-76.2" y1="43.18" x2="-86.36" y2="43.18" width="0.1524" layer="91"/>
<wire x1="-86.36" y1="55.88" x2="-86.36" y2="58.42" width="0.1524" layer="91"/>
<wire x1="-86.36" y1="50.8" x2="-86.36" y2="43.18" width="0.1524" layer="91"/>
<wire x1="-86.36" y1="50.8" x2="-75.184" y2="50.8" width="0.1524" layer="91"/>
<junction x="-86.36" y="50.8"/>
<pinref part="D8" gate="D$1" pin="P$2"/>
<wire x1="-86.36" y1="55.88" x2="-83.82" y2="55.88" width="0.1524" layer="91"/>
<wire x1="-86.36" y1="55.88" x2="-86.36" y2="50.8" width="0.1524" layer="91"/>
<junction x="-86.36" y="55.88"/>
<pinref part="S1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="THCTL" class="0">
<segment>
<pinref part="J7" gate="G$1" pin="6"/>
<pinref part="C3" gate="G$1" pin="1"/>
<wire x1="-63.5" y1="119.38" x2="-63.5" y2="116.84" width="0.1524" layer="91"/>
<wire x1="-63.5" y1="116.84" x2="-73.66" y2="116.84" width="0.1524" layer="91"/>
<label x="-73.66" y="116.84" size="1.778" layer="95"/>
<wire x1="-63.5" y1="119.38" x2="-53.34" y2="119.38" width="0.1524" layer="91"/>
<wire x1="-60.96" y1="116.84" x2="-63.5" y2="116.84" width="0.1524" layer="91"/>
<junction x="-63.5" y="116.84"/>
<label x="-53.34" y="119.38" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="1"/>
<wire x1="109.22" y1="91.44" x2="76.2" y2="91.44" width="0.1524" layer="91"/>
<label x="76.2" y="91.44" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="SPK" class="0">
<segment>
<wire x1="-5.08" y1="58.42" x2="-7.62" y2="58.42" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="A6"/>
<label x="-7.62" y="58.42" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
<segment>
<wire x1="53.34" y1="7.62" x2="53.34" y2="10.16" width="0.1524" layer="91"/>
<pinref part="SG1" gate="G$1" pin="2"/>
<wire x1="53.34" y1="10.16" x2="45.72" y2="10.16" width="0.1524" layer="91"/>
<label x="45.72" y="10.16" size="1.778" layer="95" rot="R180" xref="yes"/>
</segment>
</net>
<net name="ST" class="0">
<segment>
<pinref part="U1" gate="G$1" pin="D2"/>
<wire x1="25.4" y1="55.88" x2="38.1" y2="55.88" width="0.1524" layer="91"/>
<label x="38.1" y="55.88" size="1.778" layer="95" xref="yes"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
<wire x1="71.12" y1="114.3" x2="66.04" y2="114.3" width="0.1524" layer="91"/>
<label x="71.12" y="114.3" size="1.778" layer="95" xref="yes"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
<compatibility>
<note version="8.2" severity="warning">
Since Version 8.2, EAGLE supports online libraries. The ids
of those online libraries will not be understood (or retained)
with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
<note version="8.4" severity="warning">
Since Version 8.4, EAGLE supports properties for SPICE simulation. 
Probes in schematics and SPICE mapping objects found in parts and library devices
will not be understood with this version. Update EAGLE to the latest version
for full support of SPICE simulation. 
</note>
</compatibility>
</eagle>
