<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="no" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="no" active="no"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="no" active="no"/>
<layer number="17" name="Pads" color="2" fill="1" visible="no" active="no"/>
<layer number="18" name="Vias" color="2" fill="1" visible="no" active="no"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="no" active="no"/>
<layer number="20" name="Dimension" color="24" fill="1" visible="no" active="no"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="no" active="no"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="no" active="no"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="no" active="no"/>
<layer number="25" name="tNames" color="7" fill="1" visible="no" active="no"/>
<layer number="26" name="bNames" color="7" fill="1" visible="no" active="no"/>
<layer number="27" name="tValues" color="7" fill="1" visible="no" active="no"/>
<layer number="28" name="bValues" color="7" fill="1" visible="no" active="no"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="no"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="no"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="no"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="no"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="no"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="no"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="no"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="no"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="no"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="no"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="no" active="no"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="no" active="no"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="no" active="no"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="no" active="no"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="no" active="no"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="no"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="no"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="no"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="no"/>
<layer number="48" name="Document" color="7" fill="1" visible="no" active="no"/>
<layer number="49" name="Reference" color="7" fill="1" visible="no" active="no"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="no"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="no" active="no"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="57" name="tCAD" color="7" fill="1" visible="no" active="no"/>
<layer number="59" name="tCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="60" name="bCarbon" color="7" fill="1" visible="no" active="no"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="yes" active="yes"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="yes" active="yes"/>
<layer number="90" name="Modules" color="5" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="no" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="99" name="SpiceOrder" color="5" fill="1" visible="yes" active="yes"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="yes" active="yes"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="yes" active="yes"/>
<layer number="103" name="tMap" color="7" fill="1" visible="yes" active="yes"/>
<layer number="104" name="Name" color="16" fill="1" visible="yes" active="yes"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="yes" active="yes"/>
<layer number="107" name="Crop" color="7" fill="1" visible="yes" active="yes"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="yes" active="yes"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="yes" active="yes"/>
<layer number="110" name="fp0" color="7" fill="1" visible="yes" active="yes"/>
<layer number="111" name="LPC17xx" color="7" fill="1" visible="yes" active="yes"/>
<layer number="112" name="tSilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="113" name="IDFDebug" color="4" fill="1" visible="yes" active="yes"/>
<layer number="114" name="Badge_Outline" color="7" fill="1" visible="yes" active="yes"/>
<layer number="115" name="ReferenceISLANDS" color="7" fill="1" visible="yes" active="yes"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="yes" active="yes"/>
<layer number="118" name="Rect_Pads" color="7" fill="1" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="123" name="tTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="124" name="bTestmark" color="7" fill="1" visible="yes" active="yes"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="126" name="_bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="127" name="_tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="128" name="_bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="129" name="Mask" color="7" fill="1" visible="yes" active="yes"/>
<layer number="131" name="tAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="132" name="bAdjust" color="7" fill="1" visible="yes" active="yes"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="yes" active="yes"/>
<layer number="150" name="Notes" color="7" fill="1" visible="yes" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="yes" active="yes"/>
<layer number="152" name="_bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="153" name="FabDoc1" color="7" fill="1" visible="yes" active="yes"/>
<layer number="154" name="FabDoc2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="155" name="FabDoc3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="199" name="Contour" color="7" fill="1" visible="yes" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="yes" active="yes"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="yes" active="yes"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="yes" active="yes"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="yes" active="yes"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="yes" active="yes"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="yes" active="yes"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="yes" active="yes"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="yes" active="yes"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="yes" active="yes"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="225" name="225bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="226" name="226bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="227" name="227bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="228" name="228bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="229" name="229bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="230" name="230bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="231" name="231bmp" color="7" fill="1" visible="yes" active="yes"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="yes" active="yes"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="yes" active="yes"/>
<layer number="248" name="Housing" color="7" fill="1" visible="yes" active="yes"/>
<layer number="249" name="Edge" color="7" fill="1" visible="yes" active="yes"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="yes" active="yes"/>
<layer number="255" name="routoute" color="7" fill="1" visible="yes" active="yes"/>
</layers>
<schematic xreflabel="%F%N/%S.%C%R" xrefpart="/%S.%C%R">
<libraries>
<library name="Capacitor" urn="urn:adsk.eagle:library:16290819">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC1005X60" urn="urn:adsk.eagle:footprint:16290849/2" library_version="4">
<description>Chip, 1.00 X 0.50 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.60 mm&lt;/p&gt;</description>
<wire x1="0.55" y1="0.6286" x2="-0.55" y2="0.6286" width="0.127" layer="21"/>
<wire x1="0.55" y1="-0.6286" x2="-0.55" y2="-0.6286" width="0.127" layer="21"/>
<wire x1="0.55" y1="-0.3" x2="-0.55" y2="-0.3" width="0.12" layer="51"/>
<wire x1="-0.55" y1="-0.3" x2="-0.55" y2="0.3" width="0.12" layer="51"/>
<wire x1="-0.55" y1="0.3" x2="0.55" y2="0.3" width="0.12" layer="51"/>
<wire x1="0.55" y1="0.3" x2="0.55" y2="-0.3" width="0.12" layer="51"/>
<smd name="1" x="-0.4846" y="0" dx="0.56" dy="0.6291" layer="1"/>
<smd name="2" x="0.4846" y="0" dx="0.56" dy="0.6291" layer="1"/>
<text x="0" y="1.2636" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.2636" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC1110X102" urn="urn:adsk.eagle:footprint:16290845/2" library_version="4">
<description>Chip, 1.17 X 1.02 X 1.02 mm body
&lt;p&gt;Chip package with body size 1.17 X 1.02 X 1.02 mm&lt;/p&gt;</description>
<wire x1="0.66" y1="0.9552" x2="-0.66" y2="0.9552" width="0.127" layer="21"/>
<wire x1="0.66" y1="-0.9552" x2="-0.66" y2="-0.9552" width="0.127" layer="21"/>
<wire x1="0.66" y1="-0.635" x2="-0.66" y2="-0.635" width="0.12" layer="51"/>
<wire x1="-0.66" y1="-0.635" x2="-0.66" y2="0.635" width="0.12" layer="51"/>
<wire x1="-0.66" y1="0.635" x2="0.66" y2="0.635" width="0.12" layer="51"/>
<wire x1="0.66" y1="0.635" x2="0.66" y2="-0.635" width="0.12" layer="51"/>
<smd name="1" x="-0.5388" y="0" dx="0.6626" dy="1.2823" layer="1"/>
<smd name="2" x="0.5388" y="0" dx="0.6626" dy="1.2823" layer="1"/>
<text x="0" y="1.5902" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.5902" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC1608X85" urn="urn:adsk.eagle:footprint:16290847/2" library_version="4">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
<wire x1="0.875" y1="0.7991" x2="-0.875" y2="0.7991" width="0.127" layer="21"/>
<wire x1="0.875" y1="-0.7991" x2="-0.875" y2="-0.7991" width="0.127" layer="21"/>
<wire x1="0.875" y1="-0.475" x2="-0.875" y2="-0.475" width="0.12" layer="51"/>
<wire x1="-0.875" y1="-0.475" x2="-0.875" y2="0.475" width="0.12" layer="51"/>
<wire x1="-0.875" y1="0.475" x2="0.875" y2="0.475" width="0.12" layer="51"/>
<wire x1="0.875" y1="0.475" x2="0.875" y2="-0.475" width="0.12" layer="51"/>
<smd name="1" x="-0.7746" y="0" dx="0.9209" dy="0.9702" layer="1"/>
<smd name="2" x="0.7746" y="0" dx="0.9209" dy="0.9702" layer="1"/>
<text x="0" y="1.4341" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.4341" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC2012X110" urn="urn:adsk.eagle:footprint:16290848/2" library_version="4">
<description>Chip, 2.00 X 1.25 X 1.10 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
<wire x1="1.1" y1="1.0467" x2="-1.1" y2="1.0467" width="0.127" layer="21"/>
<wire x1="1.1" y1="-1.0467" x2="-1.1" y2="-1.0467" width="0.127" layer="21"/>
<wire x1="1.1" y1="-0.725" x2="-1.1" y2="-0.725" width="0.12" layer="51"/>
<wire x1="-1.1" y1="-0.725" x2="-1.1" y2="0.725" width="0.12" layer="51"/>
<wire x1="-1.1" y1="0.725" x2="1.1" y2="0.725" width="0.12" layer="51"/>
<wire x1="1.1" y1="0.725" x2="1.1" y2="-0.725" width="0.12" layer="51"/>
<smd name="1" x="-0.8754" y="0" dx="1.1646" dy="1.4653" layer="1"/>
<smd name="2" x="0.8754" y="0" dx="1.1646" dy="1.4653" layer="1"/>
<text x="0" y="1.6817" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.6817" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC3216X135" urn="urn:adsk.eagle:footprint:16290836/2" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="1.2217" x2="-1.7" y2="1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-1.2217" x2="-1.7" y2="-1.2217" width="0.127" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<smd name="2" x="1.4754" y="0" dx="1.1646" dy="1.8153" layer="1"/>
<text x="0" y="1.8567" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.8567" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC3225X135" urn="urn:adsk.eagle:footprint:16290843/2" library_version="4">
<description>Chip, 3.20 X 2.50 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.50 X 1.35 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="1.6717" x2="-1.7" y2="1.6717" width="0.127" layer="21"/>
<wire x1="1.7" y1="-1.6717" x2="-1.7" y2="-1.6717" width="0.12" layer="21"/>
<wire x1="1.7" y1="-1.35" x2="-1.7" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-1.35" x2="-1.7" y2="1.35" width="0.12" layer="51"/>
<wire x1="-1.7" y1="1.35" x2="1.7" y2="1.35" width="0.12" layer="51"/>
<wire x1="1.7" y1="1.35" x2="1.7" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-1.4754" y="0" dx="1.1646" dy="2.7153" layer="1"/>
<smd name="2" x="1.4754" y="0" dx="1.1646" dy="2.7153" layer="1"/>
<text x="0" y="2.3067" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.3067" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC4532X135" urn="urn:adsk.eagle:footprint:16290841/2" library_version="4">
<description>Chip, 4.50 X 3.20 X 1.35 mm body
&lt;p&gt;Chip package with body size 4.50 X 3.20 X 1.35 mm&lt;/p&gt;</description>
<wire x1="2.4" y1="2.0217" x2="-2.4" y2="2.0217" width="0.127" layer="21"/>
<wire x1="2.4" y1="-2.0217" x2="-2.4" y2="-2.0217" width="0.127" layer="21"/>
<wire x1="2.4" y1="-1.7" x2="-2.4" y2="-1.7" width="0.12" layer="51"/>
<wire x1="-2.4" y1="-1.7" x2="-2.4" y2="1.7" width="0.12" layer="51"/>
<wire x1="-2.4" y1="1.7" x2="2.4" y2="1.7" width="0.12" layer="51"/>
<wire x1="2.4" y1="1.7" x2="2.4" y2="-1.7" width="0.12" layer="51"/>
<smd name="1" x="-2.0565" y="0" dx="1.3973" dy="3.4153" layer="1"/>
<smd name="2" x="2.0565" y="0" dx="1.3973" dy="3.4153" layer="1"/>
<text x="0" y="2.6567" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.6567" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM3216X180" urn="urn:adsk.eagle:footprint:16290835/2" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<wire x1="-1.7" y1="0.9084" x2="1.7" y2="0.9084" width="0.127" layer="21"/>
<wire x1="-1.7" y1="-0.9084" x2="1.7" y2="-0.9084" width="0.127" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<smd name="2" x="1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<text x="0" y="1.5434" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.5434" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM3528X210" urn="urn:adsk.eagle:footprint:16290844/2" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<wire x1="-1.85" y1="1.5" x2="1.85" y2="1.5" width="0.127" layer="21"/>
<wire x1="-1.85" y1="-1.5" x2="1.85" y2="-1.5" width="0.127" layer="21"/>
<wire x1="1.85" y1="-1.5" x2="-1.85" y2="-1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-1.5" x2="-1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="1.5" x2="1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="1.85" y1="1.5" x2="1.85" y2="-1.5" width="0.12" layer="51"/>
<smd name="1" x="-1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<smd name="2" x="1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<text x="0" y="2.135" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.135" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM6032X280" urn="urn:adsk.eagle:footprint:16290839/2" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<wire x1="-3.15" y1="1.75" x2="3.15" y2="1.75" width="0.127" layer="21"/>
<wire x1="-3.15" y1="-1.75" x2="3.15" y2="-1.75" width="0.127" layer="21"/>
<wire x1="3.15" y1="-1.75" x2="-3.15" y2="-1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="-1.75" x2="-3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="1.75" x2="3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="3.15" y1="1.75" x2="3.15" y2="-1.75" width="0.12" layer="51"/>
<smd name="1" x="-2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<smd name="2" x="2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<text x="0" y="2.385" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.385" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPM7343X310" urn="urn:adsk.eagle:footprint:16290840/2" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.127" layer="21"/>
<wire x1="-3.8" y1="-2.3" x2="3.8" y2="-2.3" width="0.127" layer="21"/>
<wire x1="3.8" y1="-2.3" x2="-3.8" y2="-2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="-2.3" x2="-3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="3.8" y1="2.3" x2="3.8" y2="-2.3" width="0.12" layer="51"/>
<smd name="1" x="-3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<smd name="2" x="3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<text x="0" y="2.935" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.935" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPC4564X110" urn="urn:adsk.eagle:footprint:16290837/2" library_version="4">
<description>Chip, 4.50 X 6.40 X 1.10 mm body
&lt;p&gt;Chip package with body size 4.50 X 6.40 X 1.10 mm&lt;/p&gt;</description>
<wire x1="2.4" y1="3.7179" x2="-2.4" y2="3.7179" width="0.127" layer="21"/>
<wire x1="2.4" y1="-3.7179" x2="-2.4" y2="-3.7179" width="0.127" layer="21"/>
<wire x1="2.4" y1="-3.4" x2="-2.4" y2="-3.4" width="0.12" layer="51"/>
<wire x1="-2.4" y1="-3.4" x2="-2.4" y2="3.4" width="0.12" layer="51"/>
<wire x1="-2.4" y1="3.4" x2="2.4" y2="3.4" width="0.12" layer="51"/>
<wire x1="2.4" y1="3.4" x2="2.4" y2="-3.4" width="0.12" layer="51"/>
<smd name="1" x="-2.0565" y="0" dx="1.3973" dy="6.8078" layer="1"/>
<smd name="2" x="2.0565" y="0" dx="1.3973" dy="6.8078" layer="1"/>
<text x="0" y="4.3529" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.3529" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPRD550W60D1025H1250B" urn="urn:adsk.eagle:footprint:16290829/2" library_version="4">
<description>Radial Non-Polarized Capacitor, 5.50 mm pitch, 10.25 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 10.25 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="5.25" width="0.127" layer="21"/>
<circle x="0" y="0" radius="5.25" width="0.12" layer="51"/>
<pad name="1" x="-2.75" y="0" drill="0.8" diameter="1.4"/>
<pad name="2" x="2.75" y="0" drill="0.8" diameter="1.4"/>
<text x="0" y="5.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPRD2261W240D5080H5555B" urn="urn:adsk.eagle:footprint:16290850/2" library_version="4">
<description>Radial Non-Polarized Capacitor, 22.61 mm pitch, 50.80 mm body diameter, 55.55 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 22.61 mm pitch (lead spacing), 2.40 mm lead diameter, 50.80 mm body diameter and 55.55 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="25.79" width="0.127" layer="21"/>
<circle x="0" y="0" radius="25.79" width="0.12" layer="51"/>
<pad name="1" x="-11.305" y="0" drill="2.6" diameter="3.9"/>
<pad name="2" x="11.305" y="0" drill="2.6" diameter="3.9"/>
<text x="0" y="26.425" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-26.425" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP3216X180N" urn="urn:adsk.eagle:footprint:16290838/1" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<wire x1="1.7" y1="0.9084" x2="-2.5217" y2="0.9084" width="0.12" layer="21"/>
<wire x1="-2.5217" y1="0.9084" x2="-2.5217" y2="-0.9084" width="0.12" layer="21"/>
<wire x1="-2.5217" y1="-0.9084" x2="1.7" y2="-0.9084" width="0.12" layer="21"/>
<wire x1="1.7" y1="-0.9" x2="-1.7" y2="-0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="-0.9" x2="-1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="-1.7" y1="0.9" x2="1.7" y2="0.9" width="0.12" layer="51"/>
<wire x1="1.7" y1="0.9" x2="1.7" y2="-0.9" width="0.12" layer="51"/>
<smd name="1" x="-1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<smd name="2" x="1.3099" y="0" dx="1.7955" dy="1.1887" layer="1"/>
<text x="0" y="1.5434" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.5434" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP3528X210N" urn="urn:adsk.eagle:footprint:16290842/1" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<wire x1="1.85" y1="1.5" x2="-2.6717" y2="1.5" width="0.12" layer="21"/>
<wire x1="-2.6717" y1="1.5" x2="-2.6717" y2="-1.5" width="0.12" layer="21"/>
<wire x1="-2.6717" y1="-1.5" x2="1.85" y2="-1.5" width="0.12" layer="21"/>
<wire x1="1.85" y1="-1.5" x2="-1.85" y2="-1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="-1.5" x2="-1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="-1.85" y1="1.5" x2="1.85" y2="1.5" width="0.12" layer="51"/>
<wire x1="1.85" y1="1.5" x2="1.85" y2="-1.5" width="0.12" layer="51"/>
<smd name="1" x="-1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<smd name="2" x="1.4599" y="0" dx="1.7955" dy="2.2036" layer="1"/>
<text x="0" y="2.135" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.135" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP6032X280N" urn="urn:adsk.eagle:footprint:16290825/1" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<wire x1="3.15" y1="1.75" x2="-3.9692" y2="1.75" width="0.12" layer="21"/>
<wire x1="-3.9692" y1="1.75" x2="-3.9692" y2="-1.75" width="0.12" layer="21"/>
<wire x1="-3.9692" y1="-1.75" x2="3.15" y2="-1.75" width="0.12" layer="21"/>
<wire x1="3.15" y1="-1.75" x2="-3.15" y2="-1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="-1.75" x2="-3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="-3.15" y1="1.75" x2="3.15" y2="1.75" width="0.12" layer="51"/>
<wire x1="3.15" y1="1.75" x2="3.15" y2="-1.75" width="0.12" layer="51"/>
<smd name="1" x="-2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<smd name="2" x="2.4712" y="0" dx="2.368" dy="2.2036" layer="1"/>
<text x="0" y="2.385" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.385" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP7343X310N" urn="urn:adsk.eagle:footprint:16290846/1" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<wire x1="3.8" y1="2.3" x2="-4.6192" y2="2.3" width="0.12" layer="21"/>
<wire x1="-4.6192" y1="2.3" x2="-4.6192" y2="-2.3" width="0.12" layer="21"/>
<wire x1="-4.6192" y1="-2.3" x2="3.8" y2="-2.3" width="0.12" layer="21"/>
<wire x1="3.8" y1="-2.3" x2="-3.8" y2="-2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="-2.3" x2="-3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="-3.8" y1="2.3" x2="3.8" y2="2.3" width="0.12" layer="51"/>
<wire x1="3.8" y1="2.3" x2="3.8" y2="-2.3" width="0.12" layer="51"/>
<smd name="1" x="-3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<smd name="2" x="3.1212" y="0" dx="2.368" dy="2.4036" layer="1"/>
<text x="0" y="2.935" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.935" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPPRD508W65D1000H1100B" urn="urn:adsk.eagle:footprint:16290830/1" library_version="4">
<description>Radial Polarized Capacitor, 5.08 mm pitch, 10.00 mm body diameter, 11.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.08 mm pitch (lead spacing), 0.65 mm lead diameter, 10.00 mm body diameter and 11.00 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="5" width="0.12" layer="21"/>
<circle x="0" y="0" radius="5" width="0.12" layer="51"/>
<wire x1="-4.1325" y1="4.1326" x2="-3.3825" y2="4.1326" width="0.12" layer="21"/>
<wire x1="-3.7575" y1="4.5076" x2="-3.7575" y2="3.7576" width="0.12" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="0.85" diameter="1.45"/>
<pad name="2" x="2.54" y="0" drill="0.85" diameter="1.45"/>
<text x="0" y="5.635" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.635" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPAE1030X1050N" urn="urn:adsk.eagle:footprint:16290833/1" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 10.30 X 10.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 10.30 X 10.50 mm&lt;/p&gt;</description>
<wire x1="-5.25" y1="1.3117" x2="-5.25" y2="3.1538" width="0.12" layer="21"/>
<wire x1="-5.25" y1="3.1538" x2="-3.1538" y2="5.25" width="0.12" layer="21"/>
<wire x1="-3.1538" y1="5.25" x2="5.25" y2="5.25" width="0.12" layer="21"/>
<wire x1="5.25" y1="5.25" x2="5.25" y2="1.3117" width="0.12" layer="21"/>
<wire x1="-5.25" y1="-1.3117" x2="-5.25" y2="-3.1538" width="0.12" layer="21"/>
<wire x1="-5.25" y1="-3.1538" x2="-3.1538" y2="-5.25" width="0.12" layer="21"/>
<wire x1="-3.1538" y1="-5.25" x2="5.25" y2="-5.25" width="0.12" layer="21"/>
<wire x1="5.25" y1="-5.25" x2="5.25" y2="-1.3117" width="0.12" layer="21"/>
<wire x1="5.25" y1="-5.25" x2="-5.25" y2="-5.25" width="0.12" layer="51"/>
<wire x1="-5.25" y1="-5.25" x2="-5.25" y2="5.25" width="0.12" layer="51"/>
<wire x1="-5.25" y1="5.25" x2="5.25" y2="5.25" width="0.12" layer="51"/>
<wire x1="5.25" y1="5.25" x2="5.25" y2="-5.25" width="0.12" layer="51"/>
<smd name="1" x="-4.3527" y="0" dx="4.4157" dy="2.1153" layer="1"/>
<smd name="2" x="4.3527" y="0" dx="4.4157" dy="2.1153" layer="1"/>
<text x="0" y="5.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPAE830X1050N" urn="urn:adsk.eagle:footprint:16290826/1" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 8.30 X 10.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 8.30 X 10.50 mm&lt;/p&gt;</description>
<wire x1="-4.25" y1="1.3117" x2="-4.25" y2="2.6538" width="0.12" layer="21"/>
<wire x1="-4.25" y1="2.6538" x2="-2.6538" y2="4.25" width="0.12" layer="21"/>
<wire x1="-2.6538" y1="4.25" x2="4.25" y2="4.25" width="0.12" layer="21"/>
<wire x1="4.25" y1="4.25" x2="4.25" y2="1.3117" width="0.12" layer="21"/>
<wire x1="-4.25" y1="-1.3117" x2="-4.25" y2="-2.6538" width="0.12" layer="21"/>
<wire x1="-4.25" y1="-2.6538" x2="-2.6538" y2="-4.25" width="0.12" layer="21"/>
<wire x1="-2.6538" y1="-4.25" x2="4.25" y2="-4.25" width="0.12" layer="21"/>
<wire x1="4.25" y1="-4.25" x2="4.25" y2="-1.3117" width="0.12" layer="21"/>
<wire x1="4.25" y1="-4.25" x2="-4.25" y2="-4.25" width="0.12" layer="51"/>
<wire x1="-4.25" y1="-4.25" x2="-4.25" y2="4.25" width="0.12" layer="51"/>
<wire x1="-4.25" y1="4.25" x2="4.25" y2="4.25" width="0.12" layer="51"/>
<wire x1="4.25" y1="4.25" x2="4.25" y2="-4.25" width="0.12" layer="51"/>
<smd name="1" x="-3.4259" y="0" dx="3.7636" dy="2.1153" layer="1"/>
<smd name="2" x="3.4259" y="0" dx="3.7636" dy="2.1153" layer="1"/>
<text x="0" y="4.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-4.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPPRD1000W100D2275H3200B" urn="urn:adsk.eagle:footprint:16290828/1" library_version="4">
<description>Radial Polarized Capacitor, 10.00 mm pitch, 22.75 mm body diameter, 32.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 10.00 mm pitch (lead spacing), 1.00 mm lead diameter, 22.75 mm body diameter and 32.00 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="11.75" width="0.12" layer="21"/>
<circle x="0" y="0" radius="11.75" width="0.12" layer="51"/>
<wire x1="-8.9055" y1="8.9056" x2="-8.1555" y2="8.9056" width="0.12" layer="21"/>
<wire x1="-8.5305" y1="9.2806" x2="-8.5305" y2="8.5306" width="0.12" layer="21"/>
<pad name="1" x="-5" y="0" drill="1.2" diameter="1.8"/>
<pad name="2" x="5" y="0" drill="1.2" diameter="1.8"/>
<text x="0" y="12.385" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-12.385" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPAE1905X1660N" urn="urn:adsk.eagle:footprint:16290827/1" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 19.05 X 16.60 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 19.05 X 16.60 mm&lt;/p&gt;</description>
<wire x1="-9.6" y1="1.4617" x2="-9.6" y2="5.4038" width="0.12" layer="21"/>
<wire x1="-9.6" y1="5.4038" x2="-5.4038" y2="9.6" width="0.12" layer="21"/>
<wire x1="-5.4038" y1="9.6" x2="9.6" y2="9.6" width="0.12" layer="21"/>
<wire x1="9.6" y1="9.6" x2="9.6" y2="1.4617" width="0.12" layer="21"/>
<wire x1="-9.6" y1="-1.4617" x2="-9.6" y2="-5.4038" width="0.12" layer="21"/>
<wire x1="-9.6" y1="-5.4038" x2="-5.4038" y2="-9.6" width="0.12" layer="21"/>
<wire x1="-5.4038" y1="-9.6" x2="9.6" y2="-9.6" width="0.12" layer="21"/>
<wire x1="9.6" y1="-9.6" x2="9.6" y2="-1.4617" width="0.12" layer="21"/>
<wire x1="9.6" y1="-9.6" x2="-9.6" y2="-9.6" width="0.12" layer="51"/>
<wire x1="-9.6" y1="-9.6" x2="-9.6" y2="9.6" width="0.12" layer="51"/>
<wire x1="-9.6" y1="9.6" x2="9.6" y2="9.6" width="0.12" layer="51"/>
<wire x1="9.6" y1="9.6" x2="9.6" y2="-9.6" width="0.12" layer="51"/>
<smd name="1" x="-6.9877" y="0" dx="7.6873" dy="2.4153" layer="1"/>
<smd name="2" x="6.9877" y="0" dx="7.6873" dy="2.4153" layer="1"/>
<text x="0" y="10.235" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-10.235" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPPRD550W110D1250H2500B" urn="urn:adsk.eagle:footprint:16290834/1" library_version="4">
<description>Radial Polarized Capacitor, 5.50 mm pitch, 12.50 mm body diameter, 25.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.50 mm pitch (lead spacing), 1.10 mm lead diameter, 12.50 mm body diameter and 25.00 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="6.25" width="0.12" layer="21"/>
<circle x="0" y="0" radius="6.25" width="0.12" layer="51"/>
<wire x1="-5.0164" y1="5.0165" x2="-4.2664" y2="5.0165" width="0.12" layer="21"/>
<wire x1="-4.6414" y1="5.3915" x2="-4.6414" y2="4.6415" width="0.12" layer="21"/>
<pad name="1" x="-2.75" y="0" drill="1.3" diameter="1.95"/>
<pad name="2" x="2.75" y="0" drill="1.3" diameter="1.95"/>
<text x="0" y="6.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPPRD550W60D1200H2000B" urn="urn:adsk.eagle:footprint:16290832/1" library_version="4">
<description>Radial Polarized Capacitor, 5.50 mm pitch, 12.00 mm body diameter, 20.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 12.00 mm body diameter and 20.00 mm body height&lt;/p&gt;</description>
<circle x="0" y="0" radius="6" width="0.12" layer="21"/>
<circle x="0" y="0" radius="6" width="0.12" layer="51"/>
<wire x1="-4.8397" y1="4.8397" x2="-4.0897" y2="4.8397" width="0.12" layer="21"/>
<wire x1="-4.4647" y1="5.2147" x2="-4.4647" y2="4.4647" width="0.12" layer="21"/>
<pad name="1" x="-2.75" y="0" drill="0.8" diameter="1.4"/>
<pad name="2" x="2.75" y="0" drill="0.8" diameter="1.4"/>
<text x="0" y="6.635" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.635" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPMP7443X430N" urn="urn:adsk.eagle:footprint:16290831/1" library_version="4">
<description>Molded Body, 7.42 X 4.35 X 4.30 mm body
&lt;p&gt;Molded Body package with body size 7.42 X 4.35 X 4.30 mm&lt;/p&gt;</description>
<wire x1="3.825" y1="2.25" x2="-4.6458" y2="2.25" width="0.12" layer="21"/>
<wire x1="-4.6458" y1="2.25" x2="-4.6458" y2="-2.25" width="0.12" layer="21"/>
<wire x1="-4.6458" y1="-2.25" x2="3.825" y2="-2.25" width="0.12" layer="21"/>
<wire x1="3.825" y1="-2.25" x2="-3.825" y2="-2.25" width="0.12" layer="51"/>
<wire x1="-3.825" y1="-2.25" x2="-3.825" y2="2.25" width="0.12" layer="51"/>
<wire x1="-3.825" y1="2.25" x2="3.825" y2="2.25" width="0.12" layer="51"/>
<wire x1="3.825" y1="2.25" x2="3.825" y2="-2.25" width="0.12" layer="51"/>
<smd name="1" x="-3.1655" y="0" dx="2.3326" dy="2.5153" layer="1"/>
<smd name="2" x="3.1655" y="0" dx="2.3326" dy="2.5153" layer="1"/>
<text x="0" y="2.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPPAD3410W80L3025D1825B" urn="urn:adsk.eagle:footprint:16290824/1" library_version="4">
<description>Axial Polarized Capacitor, 34.10 mm pitch, 30.25 mm body length, 18.25 mm body diameter
&lt;p&gt;Axial Polarized Capacitor package with 34.10 mm pitch (lead spacing), 0.80 mm lead diameter, 30.25 mm body length and 18.25 mm body diameter&lt;/p&gt;</description>
<wire x1="-15.25" y1="9.25" x2="-15.25" y2="-9.25" width="0.12" layer="21"/>
<wire x1="-15.25" y1="-9.25" x2="15.25" y2="-9.25" width="0.12" layer="21"/>
<wire x1="15.25" y1="-9.25" x2="15.25" y2="9.25" width="0.12" layer="21"/>
<wire x1="15.25" y1="9.25" x2="-15.25" y2="9.25" width="0.12" layer="21"/>
<wire x1="-11.4375" y1="9.25" x2="-11.4375" y2="-9.25" width="0.12" layer="21"/>
<wire x1="-15.25" y1="0" x2="-15.996" y2="0" width="0.12" layer="21"/>
<wire x1="15.25" y1="0" x2="15.996" y2="0" width="0.12" layer="21"/>
<wire x1="15.25" y1="-9.25" x2="-15.25" y2="-9.25" width="0.12" layer="51"/>
<wire x1="-15.25" y1="-9.25" x2="-15.25" y2="9.25" width="0.12" layer="51"/>
<wire x1="-15.25" y1="9.25" x2="15.25" y2="9.25" width="0.12" layer="51"/>
<wire x1="15.25" y1="9.25" x2="15.25" y2="-9.25" width="0.12" layer="51"/>
<pad name="1" x="-17.05" y="0" drill="1" diameter="1.6"/>
<pad name="2" x="17.05" y="0" drill="1" diameter="1.6"/>
<text x="0" y="9.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-9.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="CAPC1005X60" urn="urn:adsk.eagle:package:16290895/2" type="model" library_version="4">
<description>Chip, 1.00 X 0.50 X 0.60 mm body
&lt;p&gt;Chip package with body size 1.00 X 0.50 X 0.60 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1005X60"/>
</packageinstances>
</package3d>
<package3d name="CAPC1110X102" urn="urn:adsk.eagle:package:16290904/2" type="model" library_version="4">
<description>Chip, 1.17 X 1.02 X 1.02 mm body
&lt;p&gt;Chip package with body size 1.17 X 1.02 X 1.02 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1110X102"/>
</packageinstances>
</package3d>
<package3d name="CAPC1608X85" urn="urn:adsk.eagle:package:16290898/2" type="model" library_version="4">
<description>Chip, 1.60 X 0.80 X 0.85 mm body
&lt;p&gt;Chip package with body size 1.60 X 0.80 X 0.85 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC1608X85"/>
</packageinstances>
</package3d>
<package3d name="CAPC2012X110" urn="urn:adsk.eagle:package:16290897/2" type="model" library_version="4">
<description>Chip, 2.00 X 1.25 X 1.10 mm body
&lt;p&gt;Chip package with body size 2.00 X 1.25 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC2012X110"/>
</packageinstances>
</package3d>
<package3d name="CAPC3216X135" urn="urn:adsk.eagle:package:16290893/2" type="model" library_version="4">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC3216X135"/>
</packageinstances>
</package3d>
<package3d name="CAPC3225X135" urn="urn:adsk.eagle:package:16290903/2" type="model" library_version="4">
<description>Chip, 3.20 X 2.50 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 2.50 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC3225X135"/>
</packageinstances>
</package3d>
<package3d name="CAPC4532X135" urn="urn:adsk.eagle:package:16290900/2" type="model" library_version="4">
<description>Chip, 4.50 X 3.20 X 1.35 mm body
&lt;p&gt;Chip package with body size 4.50 X 3.20 X 1.35 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC4532X135"/>
</packageinstances>
</package3d>
<package3d name="CAPM3216X180" urn="urn:adsk.eagle:package:16290894/2" type="model" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM3216X180"/>
</packageinstances>
</package3d>
<package3d name="CAPM3528X210" urn="urn:adsk.eagle:package:16290902/2" type="model" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM3528X210"/>
</packageinstances>
</package3d>
<package3d name="CAPM6032X280" urn="urn:adsk.eagle:package:16290896/2" type="model" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM6032X280"/>
</packageinstances>
</package3d>
<package3d name="CAPM7343X310" urn="urn:adsk.eagle:package:16290891/2" type="model" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPM7343X310"/>
</packageinstances>
</package3d>
<package3d name="CAPC4564X110L" urn="urn:adsk.eagle:package:16290887/3" type="model" library_version="4">
<description>Chip, 4.50 X 6.40 X 1.10 mm body
&lt;p&gt;Chip package with body size 4.50 X 6.40 X 1.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPC4564X110"/>
</packageinstances>
</package3d>
<package3d name="CAPRD550W60D1025H1250B" urn="urn:adsk.eagle:package:16290858/2" type="model" library_version="4">
<description>Radial Non-Polarized Capacitor, 5.50 mm pitch, 10.25 mm body diameter, 12.50 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 10.25 mm body diameter and 12.50 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPRD550W60D1025H1250B"/>
</packageinstances>
</package3d>
<package3d name="CAPRD2261W240D5080H5555B" urn="urn:adsk.eagle:package:16290864/2" type="model" library_version="4">
<description>Radial Non-Polarized Capacitor, 22.61 mm pitch, 50.80 mm body diameter, 55.55 mm body height
&lt;p&gt;Radial Non-Polarized Capacitor package with 22.61 mm pitch (lead spacing), 2.40 mm lead diameter, 50.80 mm body diameter and 55.55 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPRD2261W240D5080H5555B"/>
</packageinstances>
</package3d>
<package3d name="CAPMP3216X180N" urn="urn:adsk.eagle:package:16290884/1" type="model" library_version="4">
<description>Molded Body, 3.20 X 1.60 X 1.80 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 1.60 X 1.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP3216X180N"/>
</packageinstances>
</package3d>
<package3d name="CAPMP3528X210N" urn="urn:adsk.eagle:package:16290901/1" type="model" library_version="4">
<description>Molded Body, 3.50 X 2.80 X 2.10 mm body
&lt;p&gt;Molded Body package with body size 3.50 X 2.80 X 2.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP3528X210N"/>
</packageinstances>
</package3d>
<package3d name="CAPMP6032X280N" urn="urn:adsk.eagle:package:16290892/1" type="model" library_version="4">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP6032X280N"/>
</packageinstances>
</package3d>
<package3d name="CAPMP7343X310N" urn="urn:adsk.eagle:package:16290885/1" type="model" library_version="4">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP7343X310N"/>
</packageinstances>
</package3d>
<package3d name="CAPPRD508W65D1000H1100B" urn="urn:adsk.eagle:package:16290899/1" type="model" library_version="4">
<description>Radial Polarized Capacitor, 5.08 mm pitch, 10.00 mm body diameter, 11.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.08 mm pitch (lead spacing), 0.65 mm lead diameter, 10.00 mm body diameter and 11.00 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPPRD508W65D1000H1100B"/>
</packageinstances>
</package3d>
<package3d name="CAPAE1030X1050N" urn="urn:adsk.eagle:package:16290882/1" type="model" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 10.30 X 10.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 10.30 X 10.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE1030X1050N"/>
</packageinstances>
</package3d>
<package3d name="CAPAE830X1050N" urn="urn:adsk.eagle:package:16290889/1" type="model" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 8.30 X 10.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 8.30 X 10.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE830X1050N"/>
</packageinstances>
</package3d>
<package3d name="CAPPRD1000W100D2275H3200B" urn="urn:adsk.eagle:package:16290888/1" type="model" library_version="4">
<description>Radial Polarized Capacitor, 10.00 mm pitch, 22.75 mm body diameter, 32.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 10.00 mm pitch (lead spacing), 1.00 mm lead diameter, 22.75 mm body diameter and 32.00 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPPRD1000W100D2275H3200B"/>
</packageinstances>
</package3d>
<package3d name="CAPAE1905X1660N" urn="urn:adsk.eagle:package:16290872/1" type="model" library_version="4">
<description>ECAP (Aluminum Electrolytic Capacitor), 19.05 X 16.60 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 19.05 X 16.60 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE1905X1660N"/>
</packageinstances>
</package3d>
<package3d name="CAPPRD550W110D1250H2500B" urn="urn:adsk.eagle:package:16290890/1" type="model" library_version="4">
<description>Radial Polarized Capacitor, 5.50 mm pitch, 12.50 mm body diameter, 25.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.50 mm pitch (lead spacing), 1.10 mm lead diameter, 12.50 mm body diameter and 25.00 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPPRD550W110D1250H2500B"/>
</packageinstances>
</package3d>
<package3d name="CAPPRD550W60D1200H2000B" urn="urn:adsk.eagle:package:16290874/1" type="model" library_version="4">
<description>Radial Polarized Capacitor, 5.50 mm pitch, 12.00 mm body diameter, 20.00 mm body height
&lt;p&gt;Radial Polarized Capacitor package with 5.50 mm pitch (lead spacing), 0.60 mm lead diameter, 12.00 mm body diameter and 20.00 mm body height&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPPRD550W60D1200H2000B"/>
</packageinstances>
</package3d>
<package3d name="CAPMP7443X430N" urn="urn:adsk.eagle:package:16290866/1" type="model" library_version="4">
<description>Molded Body, 7.42 X 4.35 X 4.30 mm body
&lt;p&gt;Molded Body package with body size 7.42 X 4.35 X 4.30 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPMP7443X430N"/>
</packageinstances>
</package3d>
<package3d name="CAPPAD3410W80L3025D1825B" urn="urn:adsk.eagle:package:16290868/1" type="model" library_version="4">
<description>Axial Polarized Capacitor, 34.10 mm pitch, 30.25 mm body length, 18.25 mm body diameter
&lt;p&gt;Axial Polarized Capacitor package with 34.10 mm pitch (lead spacing), 0.80 mm lead diameter, 30.25 mm body length and 18.25 mm body diameter&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPPAD3410W80L3025D1825B"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="C" urn="urn:adsk.eagle:symbol:16290820/1" library_version="4">
<description>Capacitor</description>
<rectangle x1="-2.032" y1="-2.032" x2="2.032" y2="-1.524" layer="94"/>
<rectangle x1="-2.032" y1="-1.016" x2="2.032" y2="-0.508" layer="94"/>
<wire x1="0" y1="0" x2="0" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="0" y1="-2.54" x2="0" y2="-2.032" width="0.1524" layer="94"/>
<pin name="1" x="0" y="2.54" visible="off" length="short" direction="pas" swaplevel="1" rot="R270"/>
<pin name="2" x="0" y="-5.08" visible="off" length="short" direction="pas" swaplevel="1" rot="R90"/>
<text x="2.54" y="2.54" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-2.54" size="1.778" layer="97">&gt;SPICEMODEL</text>
<text x="2.54" y="0" size="1.778" layer="96">&gt;VALUE</text>
<text x="2.54" y="-5.08" size="1.778" layer="97">&gt;SPICEEXTRA</text>
</symbol>
<symbol name="CPOL" urn="urn:adsk.eagle:symbol:16290823/1" library_version="4">
<wire x1="-1.524" y1="-0.889" x2="1.524" y2="-0.889" width="0.254" layer="94"/>
<wire x1="1.524" y1="-0.889" x2="1.524" y2="0" width="0.254" layer="94"/>
<wire x1="-1.524" y1="0" x2="-1.524" y2="-0.889" width="0.254" layer="94"/>
<wire x1="-1.524" y1="0" x2="1.524" y2="0" width="0.254" layer="94"/>
<text x="1.143" y="0.4826" size="1.778" layer="95">&gt;NAME</text>
<text x="-0.5842" y="0.4064" size="1.27" layer="94" rot="R90">+</text>
<text x="1.143" y="-4.5974" size="1.778" layer="96">&gt;VALUE</text>
<rectangle x1="-1.651" y1="-2.54" x2="1.651" y2="-1.651" layer="94"/>
<pin name="-" x="0" y="-5.08" visible="off" length="short" direction="pas" rot="R90"/>
<pin name="+" x="0" y="2.54" visible="off" length="short" direction="pas" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="C" urn="urn:adsk.eagle:component:16290909/4" prefix="C" uservalue="yes" library_version="4">
<description>&lt;B&gt;Capacitor - Generic</description>
<gates>
<gate name="G$1" symbol="C" x="0" y="0"/>
</gates>
<devices>
<device name="CHIP-0402(1005-METRIC)" package="CAPC1005X60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290895/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0504(1310-METRIC)" package="CAPC1110X102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290904/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0603(1608-METRIC)" package="CAPC1608X85">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290898/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-0805(2012-METRIC)" package="CAPC2012X110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290897/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1206(3216-METRIC)" package="CAPC3216X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290893/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1210(3225-METRIC)" package="CAPC3225X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290903/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1812(4532-METRIC)" package="CAPC4532X135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290900/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-1206(3216-METRIC)" package="CAPM3216X180">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290894/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-1411(3528-METRIC)" package="CAPM3528X210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290902/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2412(6032-METRIC)" package="CAPM6032X280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290896/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2917(7343-METRIC)" package="CAPM7343X310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290891/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="CHIP-1825(4564-METRIC)" package="CAPC4564X110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290887/3"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-12.5MM-DIA" package="CAPRD550W60D1025H1250B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290858/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-55.5MM-DIA" package="CAPRD2261W240D5080H5555B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290864/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="C">
<pinmap gate="G$1" pin="1" pinorder="1"/>
<pinmap gate="G$1" pin="2" pinorder="2"/>
</pinmapping>
</spice>
</deviceset>
<deviceset name="C-POL" urn="urn:adsk.eagle:component:16290908/4" prefix="C" uservalue="yes" library_version="4">
<description>&lt;B&gt;Capacitor Polarised - Generic</description>
<gates>
<gate name="G$1" symbol="CPOL" x="0" y="0"/>
</gates>
<devices>
<device name="TANTALUM-1206(3216-METRIC)" package="CAPMP3216X180N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290884/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-1411(3528-METRIC)" package="CAPMP3528X210N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290901/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2412(6032-METRIC)" package="CAPMP6032X280N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290892/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2917(7343-METRIC)" package="CAPMP7343X310N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290885/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-11MM-DIA" package="CAPPRD508W65D1000H1100B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290899/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="ECAP-10.5MM" package="CAPAE1030X1050N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290882/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="ECAP-8.5MM" package="CAPAE830X1050N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290889/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-32MM-DIA" package="CAPPRD1000W100D2275H3200B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290888/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="ECAP-19.2MM" package="CAPAE1905X1660N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290872/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-25MM-DIA" package="CAPPRD550W110D1250H2500B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290890/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="RADIAL-20MM-DIA" package="CAPPRD550W60D1200H2000B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290874/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TANTALUM-2920(7443-METRIC)" package="CAPMP7443X430N">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290866/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="AXIAL-34.1MM-PITCH" package="CAPPAD3410W80L3025D1825B">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16290868/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Capacitor" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="" constant="no"/>
<attribute name="VOLTAGE_RATING" value="" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Diodes" urn="urn:adsk.eagle:library:11396254">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Diodes&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="DO201AD" urn="urn:adsk.eagle:footprint:10898376/1" library_version="1">
<wire x1="-4.2" y1="2.525" x2="-4.2" y2="0" width="0.127" layer="51"/>
<wire x1="-4.2" y1="0" x2="-4.2" y2="-2.525" width="0.127" layer="51"/>
<wire x1="-4.2" y1="-2.525" x2="4.2" y2="-2.525" width="0.127" layer="51"/>
<wire x1="4.2" y1="-2.525" x2="4.2" y2="0" width="0.127" layer="51"/>
<wire x1="4.2" y1="0" x2="4.2" y2="2.525" width="0.127" layer="51"/>
<wire x1="4.2" y1="2.525" x2="-4.2" y2="2.525" width="0.127" layer="51"/>
<wire x1="-4.2" y1="2.525" x2="-4.2" y2="-2.525" width="0.127" layer="21"/>
<wire x1="-4.2" y1="-2.525" x2="4.2" y2="-2.525" width="0.127" layer="21"/>
<wire x1="4.2" y1="-2.525" x2="4.2" y2="2.525" width="0.127" layer="21"/>
<wire x1="4.2" y1="2.525" x2="-4.2" y2="2.525" width="0.127" layer="21"/>
<wire x1="-6.2" y1="0" x2="-4.2" y2="0" width="0.127" layer="51"/>
<wire x1="4.2" y1="0" x2="6.2" y2="0" width="0.127" layer="51"/>
<wire x1="-5" y1="0" x2="-4.25" y2="0" width="0.127" layer="21"/>
<wire x1="4.25" y1="0" x2="5" y2="0" width="0.127" layer="21"/>
<wire x1="-7.45" y1="2.775" x2="-7.45" y2="-2.775" width="0.05" layer="39"/>
<wire x1="-7.45" y1="-2.775" x2="7.4" y2="-2.775" width="0.05" layer="39"/>
<wire x1="7.4" y1="-2.775" x2="7.4" y2="2.775" width="0.05" layer="39"/>
<wire x1="7.4" y1="2.775" x2="-7.45" y2="2.775" width="0.05" layer="39"/>
<pad name="C" x="-6.2" y="0" drill="1.25" shape="square"/>
<pad name="A" x="6.2" y="0" drill="1.25"/>
<rectangle x1="-3.5" y1="-2.525" x2="-2.25" y2="2.525" layer="21"/>
<text x="-7.75" y="3" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-7.5" y="-4.25" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DO201AD" urn="urn:adsk.eagle:package:10898389/2" type="model" library_version="1">
<packageinstances>
<packageinstance name="DO201AD"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="SCHOTTKY" urn="urn:adsk.eagle:symbol:10898387/1" library_version="1">
<wire x1="-1.27" y1="-1.27" x2="1.27" y2="0" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="-1.27" y2="1.27" width="0.254" layer="94"/>
<wire x1="1.905" y1="1.27" x2="1.27" y2="1.27" width="0.254" layer="94"/>
<wire x1="1.27" y1="1.27" x2="1.27" y2="0" width="0.254" layer="94"/>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="0" width="0.254" layer="94"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="-1.27" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="1.27" y2="-1.27" width="0.254" layer="94"/>
<wire x1="1.905" y1="1.27" x2="1.905" y2="1.016" width="0.254" layer="94"/>
<wire x1="1.27" y1="-1.27" x2="0.635" y2="-1.27" width="0.254" layer="94"/>
<wire x1="0.635" y1="-1.016" x2="0.635" y2="-1.27" width="0.254" layer="94"/>
<wire x1="-1.27" y1="0" x2="-2.54" y2="0" width="0.254" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.254" layer="94"/>
<text x="-2.286" y="1.905" size="1.778" layer="95">&gt;NAME</text>
<text x="-2.286" y="-3.429" size="1.778" layer="96">&gt;VALUE</text>
<pin name="A" x="-2.54" y="0" visible="off" length="point" direction="pas"/>
<pin name="C" x="2.54" y="0" visible="off" length="point" direction="pas" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MBR360G" urn="urn:adsk.eagle:component:10898397/9" prefix="D" library_version="1">
<description>&lt;h3&gt; DIODE SCHOTTKY 60V 3A DO201AD&lt;/h3&gt;
&lt;BR&gt;
&lt;a href="https://www.onsemi.com/pub/Collateral/MBR350-D.PDF"&gt; Manufacturer's datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="SCHOTTKY" x="0" y="0"/>
</gates>
<devices>
<device name="" package="DO201AD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:10898389/2"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CREATED_BY" value="PCBLayout.com" constant="no"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MBR360GOS-ND" constant="no"/>
<attribute name="MANUFACTURER" value="ON Semiconductor" constant="no"/>
<attribute name="MPN" value="MBR360G" constant="no"/>
<attribute name="PACKAGE" value="DO-201AD" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="inductors" urn="urn:adsk.eagle:library:243">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR127" urn="urn:adsk.eagle:footprint:15034/1" library_version="4">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
<wire x1="-6.5" y1="6.5" x2="6.525" y2="6.5" width="0.2032" layer="21"/>
<wire x1="6.525" y1="6.5" x2="6.525" y2="-6.5" width="0.2032" layer="21"/>
<wire x1="6.525" y1="-6.5" x2="-6.5" y2="-6.5" width="0.2032" layer="21"/>
<wire x1="-6.5" y1="-6.5" x2="-6.5" y2="6.5" width="0.2032" layer="21"/>
<wire x1="-4.5254" y1="3.783" x2="-3.8006" y2="4.5431" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="-3.783" y1="-4.5254" x2="-4.5431" y2="-3.8006" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="4.5254" y1="-3.783" x2="3.8006" y2="-4.5431" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="3.783" y1="4.5254" x2="4.5431" y2="3.8006" width="1.016" layer="21" curve="-202.065586" cap="flat"/>
<wire x1="0" y1="5.9" x2="4.9" y2="3.275" width="0.2032" layer="21" curve="-56.209779"/>
<wire x1="0" y1="5.9" x2="-4.95" y2="3.225" width="0.2032" layer="21" curve="56.95663"/>
<wire x1="0" y1="-5.9" x2="-4.9" y2="-3.275" width="0.2032" layer="21" curve="-56.209779"/>
<wire x1="0" y1="-5.9" x2="4.95" y2="-3.225" width="0.2032" layer="21" curve="56.95663"/>
<circle x="0" y="0" radius="5.9" width="0.2032" layer="51"/>
<smd name="1" x="-4.975" y="0" dx="3.85" dy="5.5" layer="1"/>
<smd name="2" x="4.975" y="0" dx="3.85" dy="5.5" layer="1"/>
<text x="-2.5" y="3" size="1.27" layer="25">&gt;NAME</text>
<text x="-3" y="-4.5" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DR127" urn="urn:adsk.eagle:package:15117/1" type="box" library_version="4">
<description>High Power Density, High Efficiency, Shielded Inductors
Source: coiltronics_dr_series.pdf</description>
<packageinstances>
<packageinstance name="DR127"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="DRK" urn="urn:adsk.eagle:symbol:28107/2" library_version="4">
<wire x1="-3.81" y1="1.651" x2="3.81" y2="1.651" width="0.254" layer="94"/>
<text x="-3.81" y="2.286" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.937" y="-3.048" size="1.778" layer="96">&gt;VALUE</text>
<rectangle x1="-3.81" y1="-0.889" x2="3.81" y2="0.889" layer="94"/>
<pin name="2" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="1" x="-7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DR127" urn="urn:adsk.eagle:component:15196/4" prefix="L" library_version="4">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
<gates>
<gate name="G$1" symbol="DRK" x="0" y="0"/>
</gates>
<devices>
<device name="" package="DR127">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:15117/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="POPULARITY" value="2" constant="no"/>
<attribute name="SPICEPREFIX" value="L" constant="no"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="L">
<pinmap gate="G$1" pin="1" pinorder="1"/>
<pinmap gate="G$1" pin="2" pinorder="2"/>
</pinmapping>
</spice>
</deviceset>
</devicesets>
</library>
<library name="eagle-ltspice" urn="urn:adsk.eagle:library:217">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0204/7" urn="urn:adsk.eagle:footprint:13215/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
<wire x1="3.81" y1="0" x2="2.921" y2="0" width="0.508" layer="51"/>
<wire x1="-3.81" y1="0" x2="-2.921" y2="0" width="0.508" layer="51"/>
<wire x1="-2.54" y1="0.762" x2="-2.286" y2="1.016" width="0.1524" layer="21" curve="-90"/>
<wire x1="-2.54" y1="-0.762" x2="-2.286" y2="-1.016" width="0.1524" layer="21" curve="90"/>
<wire x1="2.286" y1="-1.016" x2="2.54" y2="-0.762" width="0.1524" layer="21" curve="90"/>
<wire x1="2.286" y1="1.016" x2="2.54" y2="0.762" width="0.1524" layer="21" curve="-90"/>
<wire x1="-2.54" y1="-0.762" x2="-2.54" y2="0.762" width="0.1524" layer="21"/>
<wire x1="-2.286" y1="1.016" x2="-1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="-1.778" y1="0.889" x2="-1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="-2.286" y1="-1.016" x2="-1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="-1.778" y1="-0.889" x2="-1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="0.889" x2="1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="0.889" x2="-1.778" y2="0.889" width="0.1524" layer="21"/>
<wire x1="1.778" y1="-0.889" x2="1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="1.778" y1="-0.889" x2="-1.778" y2="-0.889" width="0.1524" layer="21"/>
<wire x1="2.286" y1="1.016" x2="1.905" y2="1.016" width="0.1524" layer="21"/>
<wire x1="2.286" y1="-1.016" x2="1.905" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="2.54" y1="-0.762" x2="2.54" y2="0.762" width="0.1524" layer="21"/>
<rectangle x1="2.54" y1="-0.254" x2="2.921" y2="0.254" layer="21"/>
<rectangle x1="-2.921" y1="-0.254" x2="-2.54" y2="0.254" layer="21"/>
<pad name="1" x="-3.81" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="3.81" y="0" drill="0.8128" shape="octagon"/>
<text x="-2.54" y="1.2954" size="0.9906" layer="25" ratio="10">&gt;NAME</text>
<text x="-1.6256" y="-0.4826" size="0.9906" layer="27" ratio="10">&gt;VALUE</text>
</package>
<package name="0207/10" urn="urn:adsk.eagle:footprint:13216/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
<wire x1="5.08" y1="0" x2="4.064" y2="0" width="0.6096" layer="51"/>
<wire x1="-5.08" y1="0" x2="-4.064" y2="0" width="0.6096" layer="51"/>
<wire x1="-3.175" y1="0.889" x2="-2.921" y2="1.143" width="0.1524" layer="21" curve="-90"/>
<wire x1="-3.175" y1="-0.889" x2="-2.921" y2="-1.143" width="0.1524" layer="21" curve="90"/>
<wire x1="2.921" y1="-1.143" x2="3.175" y2="-0.889" width="0.1524" layer="21" curve="90"/>
<wire x1="2.921" y1="1.143" x2="3.175" y2="0.889" width="0.1524" layer="21" curve="-90"/>
<wire x1="-3.175" y1="-0.889" x2="-3.175" y2="0.889" width="0.1524" layer="21"/>
<wire x1="-2.921" y1="1.143" x2="-2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="-2.413" y1="1.016" x2="-2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="-2.921" y1="-1.143" x2="-2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="-2.413" y1="-1.016" x2="-2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="1.016" x2="2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="1.016" x2="-2.413" y2="1.016" width="0.1524" layer="21"/>
<wire x1="2.413" y1="-1.016" x2="2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="2.413" y1="-1.016" x2="-2.413" y2="-1.016" width="0.1524" layer="21"/>
<wire x1="2.921" y1="1.143" x2="2.54" y2="1.143" width="0.1524" layer="21"/>
<wire x1="2.921" y1="-1.143" x2="2.54" y2="-1.143" width="0.1524" layer="21"/>
<wire x1="3.175" y1="-0.889" x2="3.175" y2="0.889" width="0.1524" layer="21"/>
<rectangle x1="3.175" y1="-0.3048" x2="4.0386" y2="0.3048" layer="21"/>
<rectangle x1="-4.0386" y1="-0.3048" x2="-3.175" y2="0.3048" layer="21"/>
<pad name="1" x="-5.08" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="5.08" y="0" drill="0.8128" shape="octagon"/>
<text x="-3.048" y="1.524" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-2.2606" y="-0.635" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
</package>
<package name="R0201" urn="urn:adsk.eagle:footprint:13233/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
<rectangle x1="-0.3" y1="-0.15" x2="-0.15" y2="0.15" layer="51"/>
<rectangle x1="0.15" y1="-0.15" x2="0.3" y2="0.15" layer="51"/>
<rectangle x1="-0.15" y1="-0.15" x2="0.15" y2="0.15" layer="21"/>
<smd name="1" x="-0.255" y="0" dx="0.28" dy="0.43" layer="1"/>
<smd name="2" x="0.255" y="0" dx="0.28" dy="0.43" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0402" urn="urn:adsk.eagle:footprint:13234/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.245" y1="0.224" x2="0.245" y2="0.224" width="0.1524" layer="51"/>
<wire x1="0.245" y1="-0.224" x2="-0.245" y2="-0.224" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.483" x2="1.473" y2="0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.483" x2="1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.483" x2="-1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.483" x2="-1.473" y2="0.483" width="0.0508" layer="39"/>
<rectangle x1="-0.554" y1="-0.3048" x2="-0.254" y2="0.2951" layer="51"/>
<rectangle x1="0.2588" y1="-0.3048" x2="0.5588" y2="0.2951" layer="51"/>
<rectangle x1="-0.1999" y1="-0.4001" x2="0.1999" y2="0.4001" layer="35"/>
<smd name="1" x="-0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<smd name="2" x="0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0603" urn="urn:adsk.eagle:footprint:13235/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.432" y1="-0.356" x2="0.432" y2="-0.356" width="0.1524" layer="51"/>
<wire x1="0.432" y1="0.356" x2="-0.432" y2="0.356" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.983" x2="1.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.983" x2="1.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.983" x2="-1.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.983" x2="-1.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4318" y1="-0.4318" x2="0.8382" y2="0.4318" layer="51"/>
<rectangle x1="-0.8382" y1="-0.4318" x2="-0.4318" y2="0.4318" layer="51"/>
<rectangle x1="-0.1999" y1="-0.4001" x2="0.1999" y2="0.4001" layer="35"/>
<smd name="1" x="-0.85" y="0" dx="1" dy="1.1" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1" dy="1.1" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R0805" urn="urn:adsk.eagle:footprint:13236/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
<wire x1="-0.41" y1="0.635" x2="0.41" y2="0.635" width="0.1524" layer="51"/>
<wire x1="-0.41" y1="-0.635" x2="0.41" y2="-0.635" width="0.1524" layer="51"/>
<wire x1="-1.973" y1="0.983" x2="1.973" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="0.983" x2="1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="-0.983" x2="-1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.973" y1="-0.983" x2="-1.973" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4064" y1="-0.6985" x2="1.0564" y2="0.7015" layer="51"/>
<rectangle x1="-1.0668" y1="-0.6985" x2="-0.4168" y2="0.7015" layer="51"/>
<rectangle x1="-0.1999" y1="-0.5001" x2="0.1999" y2="0.5001" layer="35"/>
<smd name="1" x="-0.95" y="0" dx="1.3" dy="1.5" layer="1"/>
<smd name="2" x="0.95" y="0" dx="1.3" dy="1.5" layer="1"/>
<text x="-0.635" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1005" urn="urn:adsk.eagle:footprint:13237/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.245" y1="0.224" x2="0.245" y2="0.224" width="0.1524" layer="51"/>
<wire x1="0.245" y1="-0.224" x2="-0.245" y2="-0.224" width="0.1524" layer="51"/>
<wire x1="-1.473" y1="0.483" x2="1.473" y2="0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="0.483" x2="1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="1.473" y1="-0.483" x2="-1.473" y2="-0.483" width="0.0508" layer="39"/>
<wire x1="-1.473" y1="-0.483" x2="-1.473" y2="0.483" width="0.0508" layer="39"/>
<rectangle x1="-0.554" y1="-0.3048" x2="-0.254" y2="0.2951" layer="51"/>
<rectangle x1="0.2588" y1="-0.3048" x2="0.5588" y2="0.2951" layer="51"/>
<rectangle x1="-0.1999" y1="-0.3" x2="0.1999" y2="0.3" layer="35"/>
<smd name="1" x="-0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<smd name="2" x="0.65" y="0" dx="0.7" dy="0.9" layer="1"/>
<text x="-0.635" y="0.635" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-1.905" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1206" urn="urn:adsk.eagle:footprint:13238/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="0.9525" y1="-0.8128" x2="-0.9652" y2="-0.8128" width="0.1524" layer="51"/>
<wire x1="0.9525" y1="0.8128" x2="-0.9652" y2="0.8128" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="0.983" x2="2.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="0.983" x2="2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-0.983" x2="-2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-0.983" x2="-2.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="-1.6891" y1="-0.8763" x2="-0.9525" y2="0.8763" layer="51"/>
<rectangle x1="0.9525" y1="-0.8763" x2="1.6891" y2="0.8763" layer="51"/>
<rectangle x1="-0.3" y1="-0.7" x2="0.3" y2="0.7" layer="35"/>
<smd name="1" x="-1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<smd name="2" x="1.422" y="0" dx="1.6" dy="1.803" layer="1"/>
<text x="-1.27" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.27" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1210" urn="urn:adsk.eagle:footprint:13239/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="1.219" x2="0.939" y2="1.219" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-1.219" x2="0.939" y2="-1.219" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="1.483" x2="2.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="1.483" x2="2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-1.483" x2="-2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-1.483" x2="-2.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-1.3081" x2="-0.9009" y2="1.2918" layer="51"/>
<rectangle x1="0.9144" y1="-1.3081" x2="1.6645" y2="1.2918" layer="51"/>
<rectangle x1="-0.3" y1="-0.8999" x2="0.3" y2="0.8999" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R1218" urn="urn:adsk.eagle:footprint:13240/1" library_version="1">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
<wire x1="-0.913" y1="-2.219" x2="0.939" y2="-2.219" width="0.1524" layer="51"/>
<wire x1="0.913" y1="2.219" x2="-0.939" y2="2.219" width="0.1524" layer="51"/>
<rectangle x1="-1.651" y1="-2.3" x2="-0.9009" y2="2.3" layer="51"/>
<rectangle x1="0.9144" y1="-2.3" x2="1.6645" y2="2.3" layer="51"/>
<smd name="1" x="-1.475" y="0" dx="1.05" dy="4.9" layer="1"/>
<smd name="2" x="1.475" y="0" dx="1.05" dy="4.9" layer="1"/>
<text x="-2.54" y="2.54" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.81" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2010" urn="urn:adsk.eagle:footprint:13241/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-1.662" y1="1.245" x2="1.662" y2="1.245" width="0.1524" layer="51"/>
<wire x1="-1.637" y1="-1.245" x2="1.687" y2="-1.245" width="0.1524" layer="51"/>
<wire x1="-3.473" y1="1.483" x2="3.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="1.483" x2="3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="-1.483" x2="-3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-3.473" y1="-1.483" x2="-3.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-2.4892" y1="-1.3208" x2="-1.6393" y2="1.3292" layer="51"/>
<rectangle x1="1.651" y1="-1.3208" x2="2.5009" y2="1.3292" layer="51"/>
<smd name="1" x="-2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<smd name="2" x="2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<text x="-3.175" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.175" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2012" urn="urn:adsk.eagle:footprint:13242/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.41" y1="0.635" x2="0.41" y2="0.635" width="0.1524" layer="51"/>
<wire x1="-0.41" y1="-0.635" x2="0.41" y2="-0.635" width="0.1524" layer="51"/>
<wire x1="-1.973" y1="0.983" x2="1.973" y2="0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="0.983" x2="1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="1.973" y1="-0.983" x2="-1.973" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-1.973" y1="-0.983" x2="-1.973" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="0.4064" y1="-0.6985" x2="1.0564" y2="0.7015" layer="51"/>
<rectangle x1="-1.0668" y1="-0.6985" x2="-0.4168" y2="0.7015" layer="51"/>
<rectangle x1="-0.1001" y1="-0.5999" x2="0.1001" y2="0.5999" layer="35"/>
<smd name="1" x="-0.85" y="0" dx="1.3" dy="1.5" layer="1"/>
<smd name="2" x="0.85" y="0" dx="1.3" dy="1.5" layer="1"/>
<text x="-0.635" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-0.635" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R2512" urn="urn:adsk.eagle:footprint:13243/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-2.362" y1="1.473" x2="2.387" y2="1.473" width="0.1524" layer="51"/>
<wire x1="-2.362" y1="-1.473" x2="2.387" y2="-1.473" width="0.1524" layer="51"/>
<wire x1="-3.973" y1="1.983" x2="3.973" y2="1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="1.983" x2="3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="-1.983" x2="-3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="-3.973" y1="-1.983" x2="-3.973" y2="1.983" width="0.0508" layer="39"/>
<rectangle x1="-3.2004" y1="-1.5494" x2="-2.3505" y2="1.5507" layer="51"/>
<rectangle x1="2.3622" y1="-1.5494" x2="3.2121" y2="1.5507" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-2.8" y="0" dx="1.8" dy="3.2" layer="1"/>
<smd name="2" x="2.8" y="0" dx="1.8" dy="3.2" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R3216" urn="urn:adsk.eagle:footprint:13244/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="0.8" x2="0.888" y2="0.8" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-0.8" x2="0.888" y2="-0.8" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="0.983" x2="2.473" y2="0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="0.983" x2="2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-0.983" x2="-2.473" y2="-0.983" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-0.983" x2="-2.473" y2="0.983" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-0.8763" x2="-0.9009" y2="0.8738" layer="51"/>
<rectangle x1="0.889" y1="-0.8763" x2="1.6391" y2="0.8738" layer="51"/>
<rectangle x1="-0.3" y1="-0.7" x2="0.3" y2="0.7" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="1.8" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="1.8" layer="1"/>
<text x="-1.905" y="1.27" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-2.54" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R3225" urn="urn:adsk.eagle:footprint:13245/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-0.913" y1="1.219" x2="0.939" y2="1.219" width="0.1524" layer="51"/>
<wire x1="-0.913" y1="-1.219" x2="0.939" y2="-1.219" width="0.1524" layer="51"/>
<wire x1="-2.473" y1="1.483" x2="2.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="1.483" x2="2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="2.473" y1="-1.483" x2="-2.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-2.473" y1="-1.483" x2="-2.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-1.651" y1="-1.3081" x2="-0.9009" y2="1.2918" layer="51"/>
<rectangle x1="0.9144" y1="-1.3081" x2="1.6645" y2="1.2918" layer="51"/>
<rectangle x1="-0.3" y1="-1" x2="0.3" y2="1" layer="35"/>
<smd name="1" x="-1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<smd name="2" x="1.4" y="0" dx="1.6" dy="2.7" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R4527" urn="urn:adsk.eagle:footprint:13246/1" library_version="1">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
<wire x1="-5.675" y1="-3.375" x2="5.65" y2="-3.375" width="0.2032" layer="21"/>
<wire x1="5.65" y1="-3.375" x2="5.65" y2="3.375" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.375" x2="-5.675" y2="3.375" width="0.2032" layer="21"/>
<wire x1="-5.675" y1="3.375" x2="-5.675" y2="-3.375" width="0.2032" layer="51"/>
<smd name="1" x="-4.575" y="0" dx="3.94" dy="5.84" layer="1"/>
<smd name="2" x="4.575" y="0" dx="3.94" dy="5.84" layer="1"/>
<text x="-5.715" y="3.81" size="1.27" layer="25">&gt;NAME</text>
<text x="-5.715" y="-5.08" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R5025" urn="urn:adsk.eagle:footprint:13247/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
<wire x1="-1.662" y1="1.245" x2="1.662" y2="1.245" width="0.1524" layer="51"/>
<wire x1="-1.637" y1="-1.245" x2="1.687" y2="-1.245" width="0.1524" layer="51"/>
<wire x1="-3.473" y1="1.483" x2="3.473" y2="1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="1.483" x2="3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="3.473" y1="-1.483" x2="-3.473" y2="-1.483" width="0.0508" layer="39"/>
<wire x1="-3.473" y1="-1.483" x2="-3.473" y2="1.483" width="0.0508" layer="39"/>
<rectangle x1="-2.4892" y1="-1.3208" x2="-1.6393" y2="1.3292" layer="51"/>
<rectangle x1="1.651" y1="-1.3208" x2="2.5009" y2="1.3292" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<smd name="2" x="2.2" y="0" dx="1.8" dy="2.7" layer="1"/>
<text x="-3.175" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.175" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
<package name="R6332" urn="urn:adsk.eagle:footprint:13248/1" library_version="1">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
<wire x1="-2.362" y1="1.473" x2="2.387" y2="1.473" width="0.1524" layer="51"/>
<wire x1="-2.362" y1="-1.473" x2="2.387" y2="-1.473" width="0.1524" layer="51"/>
<wire x1="-3.973" y1="1.983" x2="3.973" y2="1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="1.983" x2="3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="3.973" y1="-1.983" x2="-3.973" y2="-1.983" width="0.0508" layer="39"/>
<wire x1="-3.973" y1="-1.983" x2="-3.973" y2="1.983" width="0.0508" layer="39"/>
<rectangle x1="-3.2004" y1="-1.5494" x2="-2.3505" y2="1.5507" layer="51"/>
<rectangle x1="2.3622" y1="-1.5494" x2="3.2121" y2="1.5507" layer="51"/>
<rectangle x1="-0.5001" y1="-1" x2="0.5001" y2="1" layer="35"/>
<smd name="1" x="-3.1" y="0" dx="1" dy="3.2" layer="1"/>
<smd name="2" x="3.1" y="0" dx="1" dy="3.2" layer="1"/>
<text x="-2.54" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-2.54" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="0204/7" urn="urn:adsk.eagle:package:13274/1" type="box" library_version="1">
<description>RESISTOR
type 0204, grid 7.5 mm</description>
<packageinstances>
<packageinstance name="0204/7"/>
</packageinstances>
</package3d>
<package3d name="0207/10" urn="urn:adsk.eagle:package:13275/1" type="box" library_version="1">
<description>RESISTOR
type 0207, grid 10 mm</description>
<packageinstances>
<packageinstance name="0207/10"/>
</packageinstances>
</package3d>
<package3d name="R0201" urn="urn:adsk.eagle:package:13294/1" type="box" library_version="1">
<description>RESISTOR chip
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
<packageinstances>
<packageinstance name="R0201"/>
</packageinstances>
</package3d>
<package3d name="R0402" urn="urn:adsk.eagle:package:13296/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0402"/>
</packageinstances>
</package3d>
<package3d name="R0603" urn="urn:adsk.eagle:package:13302/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0603"/>
</packageinstances>
</package3d>
<package3d name="R0805" urn="urn:adsk.eagle:package:13300/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R0805"/>
</packageinstances>
</package3d>
<package3d name="R1005" urn="urn:adsk.eagle:package:13297/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1005"/>
</packageinstances>
</package3d>
<package3d name="R1206" urn="urn:adsk.eagle:package:13301/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1206"/>
</packageinstances>
</package3d>
<package3d name="R1210" urn="urn:adsk.eagle:package:13299/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R1210"/>
</packageinstances>
</package3d>
<package3d name="R1218" urn="urn:adsk.eagle:package:13303/1" type="box" library_version="1">
<description>CRCW1218 Thick Film, Rectangular Chip Resistors
Source: http://www.vishay.com .. dcrcw.pdf</description>
<packageinstances>
<packageinstance name="R1218"/>
</packageinstances>
</package3d>
<package3d name="R2010" urn="urn:adsk.eagle:package:13309/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2010"/>
</packageinstances>
</package3d>
<package3d name="R2012" urn="urn:adsk.eagle:package:13306/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2012"/>
</packageinstances>
</package3d>
<package3d name="R2512" urn="urn:adsk.eagle:package:13304/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R2512"/>
</packageinstances>
</package3d>
<package3d name="R3216" urn="urn:adsk.eagle:package:13305/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R3216"/>
</packageinstances>
</package3d>
<package3d name="R3225" urn="urn:adsk.eagle:package:13311/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R3225"/>
</packageinstances>
</package3d>
<package3d name="R4527" urn="urn:adsk.eagle:package:13310/1" type="box" library_version="1">
<description>Package 4527
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
<packageinstances>
<packageinstance name="R4527"/>
</packageinstances>
</package3d>
<package3d name="R5025" urn="urn:adsk.eagle:package:13308/1" type="box" library_version="1">
<description>RESISTOR</description>
<packageinstances>
<packageinstance name="R5025"/>
</packageinstances>
</package3d>
<package3d name="R6332" urn="urn:adsk.eagle:package:13307/1" type="box" library_version="1">
<description>RESISTOR
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
<packageinstances>
<packageinstance name="R6332"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="R" urn="urn:adsk.eagle:symbol:13232/1" library_version="1">
<wire x1="-2.54" y1="-0.889" x2="2.54" y2="-0.889" width="0.254" layer="94"/>
<wire x1="2.54" y1="0.889" x2="-2.54" y2="0.889" width="0.254" layer="94"/>
<wire x1="2.54" y1="-0.889" x2="2.54" y2="0.889" width="0.254" layer="94"/>
<wire x1="-2.54" y1="-0.889" x2="-2.54" y2="0.889" width="0.254" layer="94"/>
<pin name="1" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1"/>
<pin name="2" x="5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1" rot="R180"/>
<text x="-3.81" y="1.4986" size="1.778" layer="95">&gt;NAME</text>
<text x="-3.81" y="-3.302" size="1.778" layer="96">&gt;VALUE</text>
<text x="-5.08" y="0" size="0.4064" layer="99" align="center">SpiceOrder 1</text>
<text x="5.08" y="0" size="0.4064" layer="99" align="center">SpiceOrder 2</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="R" urn="urn:adsk.eagle:component:13322/1" prefix="R" uservalue="yes" library_version="1">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="R" x="0" y="0"/>
</gates>
<devices>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13274/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13275/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0201" package="R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13294/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0402" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13296/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R0603" package="R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13302/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="" package="R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13300/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1005" package="R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13297/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13301/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1210" package="R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13299/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R1218" package="R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13303/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13309/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2012" package="R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13306/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13304/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R3216" package="R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13305/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R3225" package="R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13311/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R4527" package="R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13310/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R5025" package="R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13308/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
<device name="R6332" package="R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:13307/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SPICEMODEL" value="NONE" constant="no"/>
<attribute name="SPICEPREFIX" value="R" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1" urn="urn:adsk.eagle:library:371">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="GND" urn="urn:adsk.eagle:symbol:26925/1" library_version="1">
<wire x1="-1.905" y1="0" x2="1.905" y2="0" width="0.254" layer="94"/>
<text x="-2.54" y="-2.54" size="1.778" layer="96">&gt;VALUE</text>
<pin name="GND" x="0" y="2.54" visible="off" length="short" direction="sup" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" urn="urn:adsk.eagle:component:26954/1" prefix="GND" library_version="1">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND" x="0" y="0"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Connectors" urn="urn:adsk.eagle:library:513">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02" urn="urn:adsk.eagle:footprint:37654/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2" urn="urn:adsk.eagle:footprint:37655/1" library_version="1">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2" urn="urn:adsk.eagle:footprint:37656/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="3.15" x2="5.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.75" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD" urn="urn:adsk.eagle:footprint:37657/1" library_version="1">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4" y1="-1" x2="-4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-4" y1="-4.5" x2="-3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-4.5" x2="-3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="-3.2" y1="-2" x2="-2" y2="-2" width="0.2032" layer="21"/>
<wire x1="2" y1="-2" x2="3.2" y2="-2" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-2" x2="3.2" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="3.2" y1="-4.5" x2="4" y2="-4.5" width="0.2032" layer="21"/>
<wire x1="4" y1="-4.5" x2="4" y2="-1" width="0.2032" layer="21"/>
<wire x1="2" y1="3" x2="-2" y2="3" width="0.2032" layer="21"/>
<smd name="1" x="-1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="2" x="1" y="-3.7" dx="1" dy="4.6" layer="1"/>
<smd name="NC1" x="-3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<smd name="NC2" x="3.4" y="1.5" dx="3.4" dy="1.6" layer="1" rot="R90"/>
<text x="-1.397" y="1.778" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="0.635" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_BIG" urn="urn:adsk.eagle:footprint:37658/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="-1.27" width="0.127" layer="21"/>
<wire x1="-1.27" y1="-1.27" x2="5.08" y2="-1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="-1.27" x2="5.08" y2="1.27" width="0.127" layer="21"/>
<wire x1="5.08" y1="1.27" x2="-1.27" y2="1.27" width="0.127" layer="21"/>
<pad name="P$1" x="0" y="0" drill="1.0668"/>
<pad name="P$2" x="3.81" y="0" drill="1.0668"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-SMD-VERT" urn="urn:adsk.eagle:footprint:37659/1" library_version="1">
<description>&lt;h3&gt;JST-Vertical Male Header SMT &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.1" y1="2.97" x2="4.2" y2="2.97" width="0.2032" layer="51"/>
<wire x1="4.2" y1="2.97" x2="4.2" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="4.2" y1="-2.13" x2="-4.1" y2="-2.13" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="-2.13" x2="-4.1" y2="2.97" width="0.2032" layer="51"/>
<wire x1="-4.1" y1="3" x2="4.2" y2="3" width="0.2032" layer="21"/>
<wire x1="4.2" y1="3" x2="4.2" y2="2.3" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="3" x2="-4.1" y2="2.3" width="0.2032" layer="21"/>
<wire x1="2" y1="-2.1" x2="4.2" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="4.2" y1="-2.1" x2="4.2" y2="-1.7" width="0.2032" layer="21"/>
<wire x1="-2" y1="-2.1" x2="-4.1" y2="-2.1" width="0.2032" layer="21"/>
<wire x1="-4.1" y1="-2.1" x2="-4.1" y2="-1.8" width="0.2032" layer="21"/>
<smd name="P$1" x="-3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="P$2" x="3.4" y="0.27" dx="3" dy="1.6" layer="1" rot="R90"/>
<smd name="VCC" x="-1" y="-2" dx="1" dy="5.5" layer="1"/>
<smd name="GND" x="1" y="-2" dx="1" dy="5.5" layer="1"/>
<text x="-3.81" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-3.81" y="2.21" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
</package>
<package name="SCREWTERMINAL-5MM-2" urn="urn:adsk.eagle:footprint:37660/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-3.1" y1="4.2" x2="8.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="4.2" x2="8.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="8.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-3.3" x2="-3.1" y2="-3.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-3.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-2.3" x2="-3.1" y2="4.2" width="0.2032" layer="21"/>
<wire x1="8.1" y1="-2.3" x2="-3.1" y2="-2.3" width="0.2032" layer="21"/>
<wire x1="-3.1" y1="-1.35" x2="-3.7" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-1.35" x2="-3.7" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-3.7" y1="-2.35" x2="-3.1" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="8.1" y1="4" x2="8.7" y2="4" width="0.2032" layer="51"/>
<wire x1="8.7" y1="4" x2="8.7" y2="3" width="0.2032" layer="51"/>
<wire x1="8.7" y1="3" x2="8.1" y2="3" width="0.2032" layer="51"/>
<circle x="2.5" y="3.7" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.3" diameter="2.032" shape="square"/>
<pad name="2" x="5" y="0" drill="1.3" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LOCK" urn="urn:adsk.eagle:footprint:37661/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="-0.1778" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.7178" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X2_LOCK" urn="urn:adsk.eagle:footprint:37662/1" library_version="1">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset from center by 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="3.81" y2="-2.54" width="0.127" layer="21"/>
<wire x1="3.81" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="3.81" y1="-2.54" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="2.54" y2="-1.27" width="0.127" layer="21"/>
<wire x1="2.54" y1="-1.27" x2="2.54" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.667" y="0" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.794" size="0.6096" layer="27" font="vector" ratio="20" align="top-left">&gt;VALUE</text>
</package>
<package name="1X02_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37663/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.651" y1="0" x2="0.889" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.016" y2="0" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.9906" x2="-0.9906" y2="1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0" x2="-1.27" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.9906" x2="-0.9906" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.556" y2="0" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="-0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.9906" x2="3.5306" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0" x2="3.81" y2="0.9906" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.9906" x2="3.5306" y2="1.27" width="0.2032" layer="21"/>
<pad name="1" x="-0.127" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.667" y="0" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.2921" x2="0.2921" y2="0.2921" layer="51"/>
<rectangle x1="2.2479" y1="-0.2921" x2="2.8321" y2="0.2921" layer="51"/>
<text x="-1.27" y="1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK" urn="urn:adsk.eagle:footprint:37664/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<circle x="0" y="0" radius="0.4318" width="0.0254" layer="51"/>
<circle x="3.5" y="0" radius="0.4318" width="0.0254" layer="51"/>
<pad name="1" x="-0.1778" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.6778" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_LONGPADS" urn="urn:adsk.eagle:footprint:37665/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.397" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_NO_SILK" urn="urn:adsk.eagle:footprint:37666/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH" urn="urn:adsk.eagle:footprint:37667/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="2.73" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<wire x1="-2.95" y1="-1.6" x2="-2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="6" x2="2.95" y2="6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="6" x2="2.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.95" y1="-1.6" x2="-2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="2.95" y1="-1.6" x2="2.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-1.6" x2="-2.3" y2="0" width="0.2032" layer="21"/>
<wire x1="2.3" y1="-1.6" x2="2.3" y2="0" width="0.2032" layer="21"/>
</package>
<package name="1X02_XTRA_BIG" urn="urn:adsk.eagle:footprint:37668/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-5.08" y1="2.54" x2="-5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="2.54" width="0.127" layer="21"/>
<wire x1="5.08" y1="2.54" x2="-5.08" y2="2.54" width="0.127" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="2.0574" diameter="3.556"/>
<pad name="2" x="2.54" y="0" drill="2.0574" diameter="3.556"/>
<text x="-5.08" y="2.667" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-5.08" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_PP_HOLES_ONLY" urn="urn:adsk.eagle:footprint:37669/1" library_version="1">
<description>&lt;h3&gt;Pogo Pins Connector - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<text x="-1.27" y="1.143" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-1.778" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS" urn="urn:adsk.eagle:footprint:37670/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="5.25" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.4" x2="5.25" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="5.25" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="51"/>
<wire x1="5.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="51"/>
<wire x1="-1.75" y1="-1.35" x2="-2.15" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-1.35" x2="-2.15" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.15" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="5.25" y1="3.15" x2="5.65" y2="3.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="3.15" x2="5.65" y2="2.15" width="0.2032" layer="51"/>
<wire x1="5.65" y1="2.15" x2="5.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="2" y="3" radius="0.2828" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<text x="-1.27" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-2-PTH-NS" urn="urn:adsk.eagle:footprint:37671/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole- No Silk&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; No silk outline of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.6"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
</package>
<package name="JST-2-PTH-KIT" urn="urn:adsk.eagle:footprint:37672/1" library_version="1">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole - KIT&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
&lt;br&gt; This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2" y1="0" x2="-2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-2" y1="-1.8" x2="-3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="-3" y1="-1.8" x2="-3" y2="6" width="0.2032" layer="51"/>
<wire x1="-3" y1="6" x2="3" y2="6" width="0.2032" layer="51"/>
<wire x1="3" y1="6" x2="3" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="3" y1="-1.8" x2="2" y2="-1.8" width="0.2032" layer="51"/>
<wire x1="2" y1="-1.8" x2="2" y2="0" width="0.2032" layer="51"/>
<pad name="1" x="-1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<pad name="2" x="1" y="0" drill="0.7" diameter="1.4478" stop="no"/>
<text x="-1.27" y="5.27" size="0.6096" layer="25" font="vector" ratio="20">&gt;Name</text>
<text x="-1.27" y="4" size="0.6096" layer="27" font="vector" ratio="20">&gt;Value</text>
<text x="0.6" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<polygon width="0.127" layer="30">
<vertex x="-0.9975" y="-0.6604" curve="-90.025935"/>
<vertex x="-1.6604" y="0" curve="-90.017354"/>
<vertex x="-1" y="0.6604" curve="-90"/>
<vertex x="-0.3396" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="-1" y="-0.2865" curve="-90.08005"/>
<vertex x="-1.2865" y="0" curve="-90.040011"/>
<vertex x="-1" y="0.2865" curve="-90"/>
<vertex x="-0.7135" y="0" curve="-90"/>
</polygon>
<polygon width="0.127" layer="30">
<vertex x="1.0025" y="-0.6604" curve="-90.025935"/>
<vertex x="0.3396" y="0" curve="-90.017354"/>
<vertex x="1" y="0.6604" curve="-90"/>
<vertex x="1.6604" y="0" curve="-90.078137"/>
</polygon>
<polygon width="0.127" layer="29">
<vertex x="1" y="-0.2865" curve="-90.08005"/>
<vertex x="0.7135" y="0" curve="-90.040011"/>
<vertex x="1" y="0.2865" curve="-90"/>
<vertex x="1.2865" y="0" curve="-90"/>
</polygon>
</package>
<package name="SPRINGTERMINAL-2.54MM-2" urn="urn:adsk.eagle:footprint:37673/1" library_version="1">
<description>&lt;h3&gt;Spring Terminal- PCB Mount 2 Pin PTH&lt;/h3&gt;
tDocu marks the spring arms
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/SpringTerminal.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.2" y1="7.88" x2="-4.2" y2="-2.8" width="0.254" layer="21"/>
<wire x1="-4.2" y1="-2.8" x2="-4.2" y2="-4.72" width="0.254" layer="51"/>
<wire x1="-4.2" y1="-4.72" x2="3.44" y2="-4.72" width="0.254" layer="51"/>
<wire x1="3.44" y1="-4.72" x2="3.44" y2="-2.8" width="0.254" layer="51"/>
<wire x1="3.44" y1="7.88" x2="-4.2" y2="7.88" width="0.254" layer="21"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="1"/>
<wire x1="0" y1="0" x2="0" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="16"/>
<wire x1="2.54" y1="0" x2="2.54" y2="5.08" width="0.254" layer="1"/>
<wire x1="-4.2" y1="-2.8" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<wire x1="3.44" y1="4" x2="3.44" y2="1" width="0.254" layer="21"/>
<wire x1="3.44" y1="7.88" x2="3.44" y2="6" width="0.254" layer="21"/>
<wire x1="3.44" y1="-0.9" x2="3.44" y2="-2.8" width="0.254" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1" diameter="1.9"/>
<pad name="P$2" x="0" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="P$3" x="2.54" y="5.08" drill="1.1" diameter="1.9"/>
<pad name="2" x="2.54" y="0" drill="1.1" diameter="1.9"/>
</package>
<package name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:footprint:37674/1" library_version="1">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="P2" x="0" y="0" drill="1.016" shape="square"/>
<pad name="P1" x="2.54" y="0" drill="1.016" shape="square"/>
<wire x1="-1.5" y1="3.25" x2="4" y2="3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="3.25" x2="4" y2="2.5" width="0.2032" layer="21"/>
<wire x1="4" y1="2.5" x2="4" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="4" y1="-3.25" x2="-1.5" y2="-3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="-3.25" x2="-1.5" y2="2.5" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="-1.5" y2="3.25" width="0.2032" layer="21"/>
<wire x1="-1.5" y1="2.5" x2="4" y2="2.5" width="0.2032" layer="21"/>
<text x="-1.27" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-4.064" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X02_POKEHOME" urn="urn:adsk.eagle:footprint:37675/1" library_version="1">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
<wire x1="-7" y1="-4" x2="-7" y2="2" width="0.2032" layer="21"/>
<wire x1="-7" y1="2" x2="-7" y2="4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="4" x2="4.7" y2="-4" width="0.2032" layer="21"/>
<wire x1="4.7" y1="-4" x2="-7" y2="-4" width="0.2032" layer="21"/>
<wire x1="-7" y1="4" x2="4.7" y2="4" width="0.2032" layer="21"/>
<smd name="P2" x="5.25" y="-2" dx="3.5" dy="2" layer="1"/>
<smd name="P1" x="5.25" y="2" dx="3.5" dy="2" layer="1"/>
<smd name="P4" x="-4" y="-2" dx="6" dy="2" layer="1"/>
<smd name="P3" x="-4" y="2" dx="6" dy="2" layer="1"/>
<text x="0.635" y="-3.175" size="0.4064" layer="25">&gt;NAME</text>
<text x="0.635" y="-1.905" size="0.4064" layer="27">&gt;VALUE</text>
</package>
<package name="1X02_RA_PTH_FEMALE" urn="urn:adsk.eagle:footprint:37676/1" library_version="1">
<wire x1="-2.79" y1="4.25" x2="-2.79" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="2.79" y1="4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="4.25" x2="2.79" y2="4.25" width="0.1778" layer="21"/>
<wire x1="-2.79" y1="-4.25" x2="2.79" y2="-4.25" width="0.1778" layer="21"/>
<text x="-1.397" y="0.762" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.524" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<pad name="2" x="-1.27" y="-5.85" drill="0.8"/>
<pad name="1" x="1.27" y="-5.85" drill="0.8"/>
</package>
<package name="1X04" urn="urn:adsk.eagle:footprint:37702/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X4" urn="urn:adsk.eagle:footprint:37703/1" library_version="1">
<description>&lt;h3&gt;Molex 4-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="8.89" y1="3.048" x2="8.89" y2="-2.54" width="0.127" layer="21"/>
<wire x1="8.89" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="8.89" y1="-2.54" x2="7.62" y2="-2.54" width="0.127" layer="21"/>
<wire x1="7.62" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="7.62" y2="-1.27" width="0.127" layer="21"/>
<wire x1="7.62" y1="-1.27" x2="7.62" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796"/>
<text x="2.286" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="2.286" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="SCREWTERMINAL-3.5MM-4" urn="urn:adsk.eagle:footprint:37704/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="12.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="12.25" y1="3.4" x2="12.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="12.25" y1="-2.8" x2="12.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="12.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="12.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="12.25" y1="3.15" x2="12.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="12.75" y1="3.15" x2="12.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="12.75" y1="2.15" x2="12.25" y2="2.15" width="0.2032" layer="51"/>
<circle x="0" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="3.5" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="7" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="10.5" y="0" radius="0.425" width="0.001" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.032"/>
<pad name="4" x="10.5" y="0" drill="1.2" diameter="2.032"/>
<text x="0" y="2.413" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="0" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_1.27MM" urn="urn:adsk.eagle:footprint:37705/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.381" y1="-0.889" x2="0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="-0.889" x2="0.635" y2="-0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="-0.635" x2="0.889" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="-0.889" x2="1.651" y2="-0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="-0.889" x2="1.905" y2="-0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="-0.635" x2="2.159" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="-0.889" x2="2.921" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="-0.889" x2="3.175" y2="-0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="-0.635" x2="3.429" y2="-0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="-0.889" x2="4.191" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="0.889" x2="3.429" y2="0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="0.889" x2="3.175" y2="0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="0.635" x2="2.921" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="0.889" x2="2.159" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="0.889" x2="1.905" y2="0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="0.635" x2="1.651" y2="0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="0.889" x2="0.889" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="0.889" x2="0.635" y2="0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="0.635" x2="0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="0.889" x2="-0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="-0.381" y1="0.889" x2="-0.889" y2="0.381" width="0.127" layer="21"/>
<wire x1="-0.889" y1="-0.381" x2="-0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="-0.889" y1="0.381" x2="-0.889" y2="-0.381" width="0.127" layer="21"/>
<wire x1="4.191" y1="0.889" x2="4.699" y2="0.381" width="0.127" layer="21"/>
<wire x1="4.699" y1="0.381" x2="4.699" y2="-0.381" width="0.127" layer="21"/>
<wire x1="4.699" y1="-0.381" x2="4.191" y2="-0.889" width="0.127" layer="21"/>
<pad name="4" x="3.81" y="0" drill="0.508" diameter="1"/>
<pad name="3" x="2.54" y="0" drill="0.508" diameter="1"/>
<pad name="2" x="1.27" y="0" drill="0.508" diameter="1"/>
<pad name="1" x="0" y="0" drill="0.508" diameter="1"/>
<text x="-0.508" y="1.016" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.508" y="-1.651" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_LOCK" urn="urn:adsk.eagle:footprint:37706/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Locking Footprint&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="-0.127" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37707/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.524" y1="-0.127" x2="1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="4.064" y1="-0.127" x2="3.556" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="6.604" y1="-0.127" x2="6.096" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.8636" x2="-0.9906" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-1.1176" x2="-0.9906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.127" x2="8.636" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.127" x2="8.89" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-1.1176" x2="8.6106" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.127" x2="8.89" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.8636" x2="8.6106" y2="1.143" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51" rot="R90"/>
<text x="-1.27" y="1.651" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.413" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X4_LOCK" urn="urn:adsk.eagle:footprint:37708/1" library_version="1">
<description>&lt;h3&gt;Molex 4-Pin Plated Through-Hole Locking&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="8.89" y1="3.048" x2="8.89" y2="-2.54" width="0.127" layer="21"/>
<wire x1="8.89" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="8.89" y1="-2.54" x2="7.62" y2="-2.54" width="0.127" layer="21"/>
<wire x1="7.62" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="7.62" y2="-1.27" width="0.127" layer="21"/>
<wire x1="7.62" y1="-1.27" x2="7.62" y2="-2.54" width="0.127" layer="21"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796" shape="square"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.127" drill="1.016" diameter="1.8796"/>
<text x="2.667" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="2.032" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_SMD_RA_MALE" urn="urn:adsk.eagle:footprint:37709/1" library_version="1">
<description>&lt;h3&gt;SMD - 4 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="5.08" y1="1.25" x2="-5.08" y2="1.25" width="0.127" layer="51"/>
<wire x1="-5.08" y1="1.25" x2="-5.08" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-5.08" y1="-1.25" x2="-3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="5.08" y2="-1.25" width="0.127" layer="51"/>
<wire x1="5.08" y1="-1.25" x2="5.08" y2="1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="-1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-3.81" y2="-7.25" width="0.127" layer="51"/>
<smd name="4" x="3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="3" x="1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="1" x="-3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<hole x="-2.54" y="0" drill="1.4"/>
<hole x="2.54" y="0" drill="1.4"/>
<text x="-4.318" y="6.731" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-4.318" y="2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_LONGPADS" urn="urn:adsk.eagle:footprint:37710/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_NO_SILK" urn="urn:adsk.eagle:footprint:37711/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="JST-4-PTH" urn="urn:adsk.eagle:footprint:37712/1" library_version="1">
<description>&lt;h3&gt;JST Right Angle 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="-3" y="0" drill="0.7" diameter="1.6"/>
<pad name="2" x="-1" y="0" drill="0.7" diameter="1.6"/>
<pad name="3" x="1" y="0" drill="0.7" diameter="1.6"/>
<pad name="4" x="3" y="0" drill="0.7" diameter="1.6"/>
<text x="-3.4" y="0.7" size="1.27" layer="51">+</text>
<text x="-1.4" y="0.7" size="1.27" layer="51">-</text>
<text x="0.7" y="0.9" size="0.8" layer="51">S</text>
<text x="2.7" y="0.9" size="0.8" layer="51">S</text>
<text x="-1.397" y="3.429" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="2.54" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<wire x1="-4.95" y1="-1.6" x2="-4.95" y2="6" width="0.2032" layer="21"/>
<wire x1="-4.95" y1="6" x2="4.95" y2="6" width="0.2032" layer="21"/>
<wire x1="4.95" y1="6" x2="4.95" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-4.95" y1="-1.6" x2="-4.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="4.95" y1="-1.6" x2="4.3" y2="-1.6" width="0.2032" layer="21"/>
<wire x1="-4.3" y1="-1.6" x2="-4.3" y2="0" width="0.2032" layer="21"/>
<wire x1="4.3" y1="-1.6" x2="4.3" y2="0" width="0.2032" layer="21"/>
</package>
<package name="SCREWTERMINAL-3.5MM-4_LOCK" urn="urn:adsk.eagle:footprint:37713/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH Locking&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2.3" y1="3.4" x2="12.8" y2="3.4" width="0.2032" layer="21"/>
<wire x1="12.8" y1="3.4" x2="12.8" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="12.8" y1="-2.8" x2="12.8" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="12.8" y1="-3.6" x2="-2.3" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-3.6" x2="-2.3" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-2.8" x2="-2.3" y2="3.4" width="0.2032" layer="21"/>
<wire x1="12.8" y1="-2.8" x2="-2.3" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-2.3" y1="-1.35" x2="-2.7" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.7" y1="-1.35" x2="-2.7" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.7" y1="-2.35" x2="-2.3" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="12.8" y1="3.15" x2="13.2" y2="3.15" width="0.2032" layer="51"/>
<wire x1="13.2" y1="3.15" x2="13.2" y2="2.15" width="0.2032" layer="51"/>
<wire x1="13.2" y1="2.15" x2="12.8" y2="2.15" width="0.2032" layer="51"/>
<circle x="0" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="3.5" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="7" y="0" radius="0.425" width="0.001" layer="51"/>
<circle x="10.5" y="0" radius="0.425" width="0.001" layer="51"/>
<pad name="1" x="-0.1778" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.6778" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="6.8222" y="0" drill="1.2" diameter="2.032"/>
<pad name="4" x="10.6778" y="0" drill="1.2" diameter="2.032"/>
<text x="3.81" y="2.413" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="3.81" y="1.524" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_1MM_RA" urn="urn:adsk.eagle:footprint:37714/1" library_version="1">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.5" y1="-4.6" x2="1.5" y2="-4.6" width="0.254" layer="21"/>
<wire x1="-3" y1="-2" x2="-3" y2="-0.35" width="0.254" layer="21"/>
<wire x1="2.25" y1="-0.35" x2="3" y2="-0.35" width="0.254" layer="21"/>
<wire x1="3" y1="-0.35" x2="3" y2="-2" width="0.254" layer="21"/>
<wire x1="-3" y1="-0.35" x2="-2.25" y2="-0.35" width="0.254" layer="21"/>
<circle x="-2.5" y="0.3" radius="0.1414" width="0.4" layer="21"/>
<smd name="NC2" x="-2.8" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="NC1" x="2.8" y="-3.675" dx="1.2" dy="2" layer="1"/>
<smd name="1" x="-1.5" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="2" x="-0.5" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="3" x="0.5" y="0" dx="0.6" dy="1.35" layer="1"/>
<smd name="4" x="1.5" y="0" dx="0.6" dy="1.35" layer="1"/>
<text x="-1.397" y="-2.159" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_SMD_VERTICAL_COMBO" urn="urn:adsk.eagle:footprint:37715/1" library_version="1">
<description>&lt;h3&gt;SMD - 4 Pin Vertical Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;SMD Pad count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="7.62" y1="1.27" x2="7.62" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="5.08" y1="1.27" x2="5.08" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="2.54" y1="1.27" x2="2.54" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="0" y1="1.27" x2="0" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="-1.37" y1="-1.25" x2="-1.37" y2="1.25" width="0.1778" layer="21"/>
<wire x1="8.99" y1="1.25" x2="8.99" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-0.73" y1="-1.25" x2="-1.37" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="8.99" y1="-1.25" x2="8.32" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="8.32" y1="1.25" x2="8.99" y2="1.25" width="0.1778" layer="21"/>
<wire x1="-1.37" y1="1.25" x2="-0.73" y2="1.25" width="0.1778" layer="21"/>
<wire x1="5.869" y1="-1.29" x2="6.831" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="5.869" y1="1.25" x2="6.831" y2="1.25" width="0.1778" layer="21"/>
<wire x1="3.329" y1="-1.29" x2="4.291" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="3.329" y1="1.25" x2="4.291" y2="1.25" width="0.1778" layer="21"/>
<wire x1="0.789" y1="-1.29" x2="1.751" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="0.789" y1="1.25" x2="1.751" y2="1.25" width="0.1778" layer="21"/>
<smd name="3" x="5.08" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1" x="0" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="4" x="7.62" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="2" x="2.54" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1-2" x="0" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="2-2" x="2.54" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="3-2" x="5.08" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="4-2" x="7.62" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<text x="-0.508" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.508" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_SMD_LONG" urn="urn:adsk.eagle:footprint:37716/1" library_version="1">
<description>&lt;h3&gt;SMD - 4 Pin w/ Long Solder Pads&lt;/h3&gt;
No silk, but tDocu layer shows pin position. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="5.08" y1="1.25" x2="-5.08" y2="1.25" width="0.127" layer="51"/>
<wire x1="-5.08" y1="1.25" x2="-5.08" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-5.08" y1="-1.25" x2="-3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="5.08" y2="-1.25" width="0.127" layer="51"/>
<wire x1="5.08" y1="-1.25" x2="5.08" y2="1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="-1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-3.81" y2="-7.25" width="0.127" layer="51"/>
<smd name="4" x="3.81" y="5.5" dx="4" dy="1" layer="1" rot="R90"/>
<smd name="3" x="1.27" y="5.5" dx="4" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-1.27" y="5.5" dx="4" dy="1" layer="1" rot="R90"/>
<smd name="1" x="-3.81" y="5.5" dx="4" dy="1" layer="1" rot="R90"/>
<hole x="-2.54" y="0" drill="1.4"/>
<hole x="2.54" y="0" drill="1.4"/>
</package>
<package name="JST-4-PTH-VERT" urn="urn:adsk.eagle:footprint:37717/1" library_version="1">
<description>&lt;h3&gt;JST Vertical 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-4.95" y1="-2.25" x2="-4.95" y2="2.25" width="0.2032" layer="21"/>
<wire x1="-4.95" y1="2.25" x2="4.95" y2="2.25" width="0.2032" layer="21"/>
<wire x1="4.95" y1="-2.25" x2="1" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-2.25" x2="-4.95" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.75" x2="1" y2="-1.75" width="0.2032" layer="21"/>
<wire x1="1" y1="-1.75" x2="1" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="-1" y1="-1.75" x2="-1" y2="-2.25" width="0.2032" layer="21"/>
<wire x1="4.95" y1="2.25" x2="4.95" y2="-2.25" width="0.2032" layer="21"/>
<pad name="1" x="-3" y="-0.55" drill="0.7" diameter="1.6"/>
<pad name="2" x="-1" y="-0.55" drill="0.7" diameter="1.6"/>
<pad name="3" x="1" y="-0.55" drill="0.7" diameter="1.6"/>
<pad name="4" x="3" y="-0.55" drill="0.7" diameter="1.6"/>
<text x="-1.4" y="0.75" size="1.27" layer="51">+</text>
<text x="0.6" y="0.75" size="1.27" layer="51">-</text>
<text x="2.7" y="0.95" size="0.8" layer="51">Y</text>
<text x="-3.3" y="0.95" size="0.8" layer="51">B</text>
<text x="-1.143" y="2.54" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-3.302" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X04_SMD_RA_FEMALE" urn="urn:adsk.eagle:footprint:37718/1" library_version="1">
<description>&lt;h3&gt;SMD - 4 Pin Right-Angle Female Header&lt;/h3&gt;
Silk outline shows header location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-5.205" y1="4.25" x2="-5.205" y2="-4.25" width="0.1778" layer="21"/>
<wire x1="5.205" y1="4.25" x2="-5.205" y2="4.25" width="0.1778" layer="21"/>
<wire x1="5.205" y1="-4.25" x2="5.205" y2="4.25" width="0.1778" layer="21"/>
<wire x1="-5.205" y1="-4.25" x2="5.205" y2="-4.25" width="0.1778" layer="21"/>
<rectangle x1="-1.59" y1="6.8" x2="-0.95" y2="7.65" layer="51"/>
<rectangle x1="0.95" y1="6.8" x2="1.59" y2="7.65" layer="51"/>
<rectangle x1="-4.13" y1="6.8" x2="-3.49" y2="7.65" layer="51"/>
<rectangle x1="3.49" y1="6.8" x2="4.13" y2="7.65" layer="51"/>
<smd name="3" x="1.27" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="2" x="-1.27" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="1" x="-3.81" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="4" x="3.81" y="7.225" dx="1.25" dy="3" layer="1" rot="R180"/>
<text x="-1.397" y="0.762" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.524" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06" urn="urn:adsk.eagle:footprint:37589/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="11.43" y1="0.635" x2="12.065" y2="1.27" width="0.2032" layer="21"/>
<wire x1="12.065" y1="1.27" x2="13.335" y2="1.27" width="0.2032" layer="21"/>
<wire x1="13.335" y1="1.27" x2="13.97" y2="0.635" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.635" x2="13.335" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.335" y1="-1.27" x2="12.065" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="12.065" y1="-1.27" x2="11.43" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="8.255" y2="1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.27" x2="8.89" y2="0.635" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.635" x2="8.255" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.635" x2="9.525" y2="1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.27" x2="10.795" y2="1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.27" x2="11.43" y2="0.635" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.635" x2="10.795" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.27" x2="9.525" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.27" x2="8.89" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.635" x2="4.445" y2="1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.27" x2="5.715" y2="1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="5.715" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.27" x2="4.445" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.27" x2="3.81" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.27" x2="6.35" y2="0.635" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.635" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.27" x2="6.985" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.635" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.635" x2="1.905" y2="1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.27" x2="3.81" y2="0.635" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.635" x2="3.175" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.27" x2="1.905" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.27" x2="1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="-1.27" y2="0.635" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.635" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6" urn="urn:adsk.eagle:footprint:37738/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="13.97" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="13.97" y1="-2.54" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="12.7" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="12.7" y2="-1.27" width="0.127" layer="21"/>
<wire x1="12.7" y1="-1.27" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="-0.635" y2="1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796"/>
<text x="4.699" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6-RA" urn="urn:adsk.eagle:footprint:37739/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle&lt;/h3&gt;
tPlace shows angle of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="-1.27" y2="0.635" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.175" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="12.7" y1="3.175" x2="0" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="0" y2="7.62" width="0.127" layer="21"/>
<wire x1="0" y1="7.62" x2="12.7" y2="7.62" width="0.127" layer="21"/>
<wire x1="12.7" y1="7.62" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796"/>
<text x="4.953" y="5.334" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="4.445" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-SMD_RA_MALE" urn="urn:adsk.eagle:footprint:37588/1" library_version="1">
<description>&lt;h3&gt;SMD - 6 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="7.62" y1="1.25" x2="-7.62" y2="1.25" width="0.127" layer="51"/>
<wire x1="-7.62" y1="1.25" x2="-7.62" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-7.62" y1="-1.25" x2="-6.35" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-6.35" y1="-1.25" x2="-3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="3.81" y2="-1.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="6.35" y2="-1.25" width="0.127" layer="51"/>
<wire x1="6.35" y1="-1.25" x2="7.62" y2="-1.25" width="0.127" layer="51"/>
<wire x1="7.62" y1="-1.25" x2="7.62" y2="1.25" width="0.127" layer="51"/>
<wire x1="6.35" y1="-1.25" x2="6.35" y2="-7.25" width="0.127" layer="51"/>
<wire x1="3.81" y1="-1.25" x2="3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="1.27" y1="-1.25" x2="1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="-1.27" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-3.81" y1="-1.25" x2="-3.81" y2="-7.25" width="0.127" layer="51"/>
<wire x1="-6.35" y1="-1.25" x2="-6.35" y2="-7.25" width="0.127" layer="51"/>
<smd name="4" x="1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="5" x="3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="6" x="6.35" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="3" x="-1.27" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-3.81" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<smd name="1" x="-6.35" y="5" dx="3" dy="1" layer="1" rot="R90"/>
<hole x="-5.08" y="0" drill="1.4"/>
<hole x="5.08" y="0" drill="1.4"/>
<text x="-1.524" y="0.381" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.016" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LOCK" urn="urn:adsk.eagle:footprint:37592/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.508" x2="-0.635" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="1.143" x2="0.635" y2="1.143" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.143" x2="1.27" y2="0.508" width="0.2032" layer="21"/>
<wire x1="1.27" y1="0.508" x2="1.905" y2="1.143" width="0.2032" layer="21"/>
<wire x1="1.905" y1="1.143" x2="3.175" y2="1.143" width="0.2032" layer="21"/>
<wire x1="3.175" y1="1.143" x2="3.81" y2="0.508" width="0.2032" layer="21"/>
<wire x1="3.81" y1="0.508" x2="4.445" y2="1.143" width="0.2032" layer="21"/>
<wire x1="4.445" y1="1.143" x2="5.715" y2="1.143" width="0.2032" layer="21"/>
<wire x1="5.715" y1="1.143" x2="6.35" y2="0.508" width="0.2032" layer="21"/>
<wire x1="6.35" y1="0.508" x2="6.985" y2="1.143" width="0.2032" layer="21"/>
<wire x1="6.985" y1="1.143" x2="8.255" y2="1.143" width="0.2032" layer="21"/>
<wire x1="8.255" y1="1.143" x2="8.89" y2="0.508" width="0.2032" layer="21"/>
<wire x1="8.89" y1="0.508" x2="9.525" y2="1.143" width="0.2032" layer="21"/>
<wire x1="9.525" y1="1.143" x2="10.795" y2="1.143" width="0.2032" layer="21"/>
<wire x1="10.795" y1="1.143" x2="11.43" y2="0.508" width="0.2032" layer="21"/>
<wire x1="11.43" y1="0.508" x2="12.065" y2="1.143" width="0.2032" layer="21"/>
<wire x1="12.065" y1="1.143" x2="13.335" y2="1.143" width="0.2032" layer="21"/>
<wire x1="13.335" y1="1.143" x2="13.97" y2="0.508" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.508" x2="13.97" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.762" x2="13.335" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.335" y1="-1.397" x2="12.065" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="12.065" y1="-1.397" x2="11.43" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="11.43" y1="-0.762" x2="10.795" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="10.795" y1="-1.397" x2="9.525" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="9.525" y1="-1.397" x2="8.89" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="8.89" y1="-0.762" x2="8.255" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="8.255" y1="-1.397" x2="6.985" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="6.985" y1="-1.397" x2="6.35" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="6.35" y1="-0.762" x2="5.715" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="5.715" y1="-1.397" x2="4.445" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="4.445" y1="-1.397" x2="3.81" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="3.81" y1="-0.762" x2="3.175" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="3.175" y1="-1.397" x2="1.905" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="1.905" y1="-1.397" x2="1.27" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="1.27" y1="-0.762" x2="0.635" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="0.635" y1="-1.397" x2="-0.635" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="-1.397" x2="-1.27" y2="-0.762" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.762" x2="-1.27" y2="0.508" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.286" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LOCK_LONGPADS" urn="urn:adsk.eagle:footprint:37740/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.524" y1="-0.127" x2="1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="4.064" y1="-0.127" x2="3.556" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="6.604" y1="-0.127" x2="6.096" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="9.144" y1="-0.127" x2="8.636" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="11.684" y1="-0.127" x2="11.176" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.016" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="0.8636" x2="-0.9906" y2="1.143" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-0.127" x2="-1.27" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="-1.1176" x2="-0.9906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.716" y2="-0.127" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.97" y2="-1.1176" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-1.1176" x2="13.6906" y2="-1.397" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-0.127" x2="13.97" y2="0.8636" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.8636" x2="13.6906" y2="1.143" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" shape="long" rot="R90"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51" rot="R90"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="-1.143" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.143" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX-1X6_LOCK" urn="urn:adsk.eagle:footprint:37741/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="3.048" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="13.97" y2="-2.54" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.048" x2="-1.27" y2="3.048" width="0.127" layer="21"/>
<wire x1="13.97" y1="-2.54" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="12.7" y1="-2.54" x2="0" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.127" layer="21"/>
<wire x1="0" y1="-2.54" x2="0" y2="-1.27" width="0.127" layer="21"/>
<wire x1="0" y1="-1.27" x2="12.7" y2="-1.27" width="0.127" layer="21"/>
<wire x1="12.7" y1="-1.27" x2="12.7" y2="-2.54" width="0.127" layer="21"/>
<wire x1="-0.635" y1="1.27" x2="0.635" y2="1.27" width="0.2032" layer="21"/>
<wire x1="0.635" y1="1.27" x2="-0.635" y2="1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796"/>
<rectangle x1="-0.2921" y1="-0.4191" x2="0.2921" y2="0.1651" layer="51"/>
<rectangle x1="2.2479" y1="-0.4191" x2="2.8321" y2="0.1651" layer="51"/>
<rectangle x1="4.7879" y1="-0.4191" x2="5.3721" y2="0.1651" layer="51"/>
<rectangle x1="7.3279" y1="-0.4191" x2="7.9121" y2="0.1651" layer="51"/>
<rectangle x1="9.8679" y1="-0.4191" x2="10.4521" y2="0.1651" layer="51"/>
<rectangle x1="12.4079" y1="-0.4191" x2="12.9921" y2="0.1651" layer="51"/>
<text x="4.445" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.191" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="MOLEX_1X6_RA_LOCK" urn="urn:adsk.eagle:footprint:37590/1" library_version="1">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
tPlace shows location of connector.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="3.175" width="0.127" layer="21"/>
<wire x1="13.97" y1="0.635" x2="-1.27" y2="0.635" width="0.127" layer="21"/>
<wire x1="13.97" y1="3.175" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="12.7" y1="3.175" x2="0" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="-1.27" y2="3.175" width="0.127" layer="21"/>
<wire x1="0" y1="3.175" x2="0" y2="7.62" width="0.127" layer="21"/>
<wire x1="0" y1="7.62" x2="12.7" y2="7.62" width="0.127" layer="21"/>
<wire x1="12.7" y1="7.62" x2="12.7" y2="3.175" width="0.127" layer="21"/>
<wire x1="0.635" y1="-1.27" x2="-0.635" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-0.635" y1="-1.27" x2="0.635" y2="-1.27" width="0.2032" layer="22"/>
<pad name="1" x="0" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="2" x="2.54" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="3" x="5.08" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="4" x="7.62" y="-0.127" drill="1.016" diameter="1.8796"/>
<pad name="5" x="10.16" y="0.127" drill="1.016" diameter="1.8796"/>
<pad name="6" x="12.7" y="-0.127" drill="1.016" diameter="1.8796"/>
<text x="4.826" y="5.588" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="4.699" y="4.318" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_FEMALE_LOCK.010" urn="urn:adsk.eagle:footprint:37742/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin Locking Header&lt;/h3&gt;
Includes silk outline for 6 pin female header
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/SP-140520-XX-001.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.27" x2="-1.27" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="-1.27" y1="1.27" x2="13.97" y2="1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="-1.27" x2="-1.27" y2="-1.27" width="0.2032" layer="21"/>
<wire x1="13.97" y1="1.27" x2="13.97" y2="-1.27" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="-0.254" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="-0.3175" y1="-0.1905" x2="0.3175" y2="0.1905" layer="51"/>
<rectangle x1="2.2225" y1="-0.1905" x2="2.8575" y2="0.1905" layer="51"/>
<rectangle x1="4.7625" y1="-0.1905" x2="5.3975" y2="0.1905" layer="51"/>
<rectangle x1="7.3025" y1="-0.1905" x2="7.9375" y2="0.1905" layer="51"/>
<rectangle x1="9.8425" y1="-0.1905" x2="10.4775" y2="0.1905" layer="51"/>
<rectangle x1="12.3825" y1="-0.1905" x2="13.0175" y2="0.1905" layer="51"/>
<text x="-1.143" y="1.524" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.143" y="-2.159" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_LONGPADS" urn="urn:adsk.eagle:footprint:37591/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="0.635" x2="-1.27" y2="-0.635" width="0.2032" layer="21"/>
<wire x1="13.97" y1="0.635" x2="13.97" y2="-0.635" width="0.2032" layer="21"/>
<pad name="1" x="0" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.1176" diameter="1.8796" shape="long" rot="R90"/>
<text x="-1.27" y="2.032" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.667" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
</package>
<package name="SCREWTERMINAL-3.5MM-6" urn="urn:adsk.eagle:footprint:37743/1" library_version="1">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -6 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.75" y1="3.4" x2="19.25" y2="3.4" width="0.2032" layer="21"/>
<wire x1="19.25" y1="3.4" x2="19.25" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-2.8" x2="19.25" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-3.6" x2="-1.75" y2="-3.6" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-3.6" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-2.8" x2="-1.75" y2="3.4" width="0.2032" layer="21"/>
<wire x1="19.25" y1="-2.8" x2="-1.75" y2="-2.8" width="0.2032" layer="21"/>
<wire x1="-1.75" y1="-1.35" x2="-2.25" y2="-1.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-1.35" x2="-2.25" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="-2.25" y1="-2.35" x2="-1.75" y2="-2.35" width="0.2032" layer="51"/>
<wire x1="19.25" y1="3.15" x2="19.75" y2="3.15" width="0.2032" layer="51"/>
<wire x1="19.75" y1="3.15" x2="19.75" y2="2.15" width="0.2032" layer="51"/>
<wire x1="19.75" y1="2.15" x2="19.25" y2="2.15" width="0.2032" layer="51"/>
<pad name="1" x="0" y="0" drill="1.2" diameter="2.032" shape="square"/>
<pad name="2" x="3.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="3" x="7" y="0" drill="1.2" diameter="2.032"/>
<pad name="4" x="10.5" y="0" drill="1.2" diameter="2.032"/>
<pad name="5" x="14" y="0" drill="1.2" diameter="2.032"/>
<pad name="6" x="17.5" y="0" drill="1.2" diameter="2.032"/>
<text x="7.112" y="2.413" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="6.858" y="1.524" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-SMD-FEMALE" urn="urn:adsk.eagle:footprint:37744/1" library_version="1">
<description>&lt;h3&gt;Header - 6 pin Female SMD&lt;/h3&gt;
Right angle 0.1"
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/19686.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-7.5" y1="0.45" x2="-7.5" y2="-8.05" width="0.127" layer="21"/>
<wire x1="7.5" y1="0.45" x2="-7.5" y2="0.45" width="0.127" layer="21"/>
<wire x1="7.5" y1="-8.05" x2="7.5" y2="0.45" width="0.127" layer="21"/>
<wire x1="-7.5" y1="-8.05" x2="7.5" y2="-8.05" width="0.127" layer="21"/>
<smd name="4" x="-1.27" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="5" x="-3.81" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="6" x="-6.35" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="3" x="1.27" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="2" x="3.81" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<smd name="1" x="6.35" y="3.425" dx="1.25" dy="3" layer="1" rot="R180"/>
<text x="-1.524" y="-3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.778" y="-4.826" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_HOLES_ONLY" urn="urn:adsk.eagle:footprint:37745/1" library_version="1">
<description>&lt;h3&gt; 6 Pin Holes&lt;/h3&gt;
No silk, no plating
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<circle x="0" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="5.08" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="7.62" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="10.16" y="0" radius="0.635" width="0.127" layer="51"/>
<circle x="12.7" y="0" radius="0.635" width="0.127" layer="51"/>
<pad name="1" x="0" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="0.889" diameter="0.8128" rot="R90"/>
<hole x="0" y="0" drill="1.4732"/>
<hole x="2.54" y="0" drill="1.4732"/>
<hole x="5.08" y="0" drill="1.4732"/>
<hole x="7.62" y="0" drill="1.4732"/>
<hole x="10.16" y="0" drill="1.4732"/>
<hole x="12.7" y="0" drill="1.4732"/>
</package>
<package name="1X06_SMD_STRAIGHT" urn="urn:adsk.eagle:footprint:37746/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.37" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="1.25" x2="1.37" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="-1.25" x2="-14.07" y2="1.25" width="0.127" layer="21"/>
<wire x1="0.85" y1="1.25" x2="1.37" y2="1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="1.25" x2="-10.883" y2="1.25" width="0.127" layer="21"/>
<wire x1="-13.55" y1="-1.25" x2="-14.07" y2="-1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="-1.25" x2="-1.817" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-4.377" y1="1.25" x2="-0.703" y2="1.25" width="0.127" layer="21"/>
<wire x1="-9.457" y1="1.25" x2="-5.783" y2="1.25" width="0.127" layer="21"/>
<wire x1="-3.329" y1="-1.25" x2="-6.831" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-8.409" y1="-1.25" x2="-11.911" y2="-1.25" width="0.127" layer="21"/>
<smd name="5" x="-10.16" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="3" x="-5.08" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="1" x="0" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="6" x="-12.7" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="4" x="-7.62" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="2" x="-2.54" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<text x="-13.716" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-13.843" y="-3.429" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_STRAIGHT_ALT" urn="urn:adsk.eagle:footprint:37747/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
Alternate pin configuration
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="1.37" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="51"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="51"/>
<wire x1="-14.07" y1="1.25" x2="-14.07" y2="-1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="-1.25" x2="1.37" y2="1.25" width="0.127" layer="21"/>
<wire x1="-13.55" y1="1.25" x2="-14.07" y2="1.25" width="0.127" layer="21"/>
<wire x1="1.37" y1="1.25" x2="-1.817" y2="1.25" width="0.127" layer="21"/>
<wire x1="0.85" y1="-1.25" x2="1.37" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-14.07" y1="-1.25" x2="-10.883" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-8.323" y1="1.25" x2="-11.997" y2="1.25" width="0.127" layer="21"/>
<wire x1="-3.243" y1="1.25" x2="-6.917" y2="1.25" width="0.127" layer="21"/>
<wire x1="-9.371" y1="-1.25" x2="-5.869" y2="-1.25" width="0.127" layer="21"/>
<wire x1="-4.291" y1="-1.25" x2="-0.789" y2="-1.25" width="0.127" layer="21"/>
<smd name="5" x="-10.16" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="3" x="-5.08" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1" x="0" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="6" x="-12.7" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="4" x="-7.62" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="2" x="-2.54" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<text x="-13.716" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-13.843" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_STRAIGHT_COMBO" urn="urn:adsk.eagle:footprint:37748/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Female Header - Combined Footprint&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="12.7" y1="1.27" x2="12.7" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="10.16" y1="1.27" x2="10.16" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="7.62" y1="1.27" x2="7.62" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="5.08" y1="1.27" x2="5.08" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="2.54" y1="1.27" x2="2.54" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="0" y1="1.27" x2="0" y2="-1.27" width="0.4064" layer="1"/>
<wire x1="-1.37" y1="-1.25" x2="-1.37" y2="1.25" width="0.1778" layer="21"/>
<wire x1="14.07" y1="1.25" x2="14.07" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-0.73" y1="-1.25" x2="-1.37" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="14.07" y1="-1.25" x2="13.4" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.4" y1="1.25" x2="14.07" y2="1.25" width="0.1778" layer="21"/>
<wire x1="-1.37" y1="1.25" x2="-0.73" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.949" y1="1.25" x2="11.911" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.949" y1="-1.29" x2="11.911" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="8.409" y1="1.25" x2="9.371" y2="1.25" width="0.1778" layer="21"/>
<wire x1="8.409" y1="-1.29" x2="9.371" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="5.869" y1="-1.29" x2="6.831" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="5.869" y1="1.25" x2="6.831" y2="1.25" width="0.1778" layer="21"/>
<wire x1="3.329" y1="-1.29" x2="4.291" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="3.329" y1="1.25" x2="4.291" y2="1.25" width="0.1778" layer="21"/>
<wire x1="0.789" y1="-1.29" x2="1.751" y2="-1.29" width="0.1778" layer="21"/>
<wire x1="0.789" y1="1.25" x2="1.751" y2="1.25" width="0.1778" layer="21"/>
<smd name="5" x="10.16" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="3" x="5.08" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1" x="0" y="-1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="6" x="12.7" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="4" x="7.62" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="2" x="2.54" y="1.65" dx="2" dy="1" layer="1" rot="R270"/>
<smd name="1-2" x="0" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="2-2" x="2.54" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="3-2" x="5.08" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="4-2" x="7.62" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="5-2" x="10.16" y="1.65" dx="2" dy="1" layer="1" rot="R90"/>
<smd name="6-2" x="12.7" y="-1.65" dx="2" dy="1" layer="1" rot="R90"/>
<text x="-0.508" y="2.921" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.508" y="-3.556" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_SMD_MALE" urn="urn:adsk.eagle:footprint:37749/1" library_version="1">
<description>&lt;h3&gt; 6 Pin SMD Male Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-1.27" y1="1.25" x2="-1.27" y2="-1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="-1.25" x2="13.97" y2="-1.25" width="0.127" layer="51"/>
<wire x1="13.97" y1="-1.25" x2="13.97" y2="1.25" width="0.127" layer="51"/>
<wire x1="13.97" y1="1.25" x2="-1.27" y2="1.25" width="0.127" layer="51"/>
<wire x1="-1.27" y1="1.25" x2="-1.27" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-1.27" y1="-1.25" x2="-0.635" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="-1.27" y1="1.25" x2="-0.635" y2="1.25" width="0.1778" layer="21"/>
<wire x1="0.762" y1="1.25" x2="1.778" y2="1.25" width="0.1778" layer="21"/>
<wire x1="3.302" y1="1.25" x2="4.318" y2="1.25" width="0.1778" layer="21"/>
<wire x1="5.842" y1="1.25" x2="6.858" y2="1.25" width="0.1778" layer="21"/>
<wire x1="8.382" y1="1.25" x2="9.398" y2="1.25" width="0.1778" layer="21"/>
<wire x1="10.922" y1="1.25" x2="11.938" y2="1.25" width="0.1778" layer="21"/>
<wire x1="1.778" y1="-1.25" x2="0.762" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="4.318" y1="-1.25" x2="3.302" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="6.858" y1="-1.25" x2="5.842" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="9.398" y1="-1.25" x2="8.382" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="11.938" y1="-1.25" x2="10.922" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="-1.25" x2="13.97" y2="1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="-1.25" x2="13.335" y2="-1.25" width="0.1778" layer="21"/>
<wire x1="13.97" y1="1.25" x2="13.335" y2="1.25" width="0.1778" layer="21"/>
<circle x="0" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="2.54" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="5.08" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="7.62" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="10.16" y="0" radius="0.64" width="0.127" layer="51"/>
<circle x="12.7" y="0" radius="0.64" width="0.127" layer="51"/>
<rectangle x1="-0.32" y1="0" x2="0.32" y2="2.75" layer="51"/>
<rectangle x1="4.76" y1="0" x2="5.4" y2="2.75" layer="51"/>
<rectangle x1="9.84" y1="0" x2="10.48" y2="2.75" layer="51"/>
<rectangle x1="2.22" y1="-2.75" x2="2.86" y2="0" layer="51" rot="R180"/>
<rectangle x1="7.3" y1="-2.75" x2="7.94" y2="0" layer="51" rot="R180"/>
<rectangle x1="12.38" y1="-2.75" x2="13.02" y2="0" layer="51" rot="R180"/>
<smd name="1" x="0" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="2" x="2.54" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="3" x="5.08" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="4" x="7.62" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="5" x="10.16" y="0" dx="1.02" dy="6" layer="1"/>
<smd name="6" x="12.7" y="0" dx="1.02" dy="6" layer="1"/>
<text x="-0.508" y="3.302" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.635" y="-3.937" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06-1MM" urn="urn:adsk.eagle:footprint:37635/1" library_version="1">
<description>&lt;h3&gt;JST SH Vertical  6-Pin Connector -SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1mm&lt;/li&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;li&gt;EM-406&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-2.54" y1="-1.651" x2="2.54" y2="-1.651" width="0.254" layer="21"/>
<wire x1="-4.318" y1="0.508" x2="-4.318" y2="1.905" width="0.254" layer="21"/>
<wire x1="3.302" y1="1.905" x2="4.318" y2="1.905" width="0.254" layer="21"/>
<wire x1="4.318" y1="1.905" x2="4.318" y2="0.508" width="0.254" layer="21"/>
<wire x1="-4.318" y1="1.905" x2="-3.302" y2="1.905" width="0.254" layer="21"/>
<smd name="1" x="-2.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="2" x="-1.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="3" x="-0.54" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="4" x="0.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="5" x="1.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="6" x="2.46" y="1.27" dx="0.6" dy="1.55" layer="1"/>
<smd name="P$1" x="-3.84" y="-0.955" dx="1.2" dy="1.8" layer="1"/>
<smd name="P$2" x="3.76" y="-0.955" dx="1.2" dy="1.8" layer="1"/>
<text x="-1.397" y="-0.381" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.651" y="-1.27" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
<circle x="-3.6" y="2.47" radius="0.1047" width="0.4064" layer="21"/>
</package>
<package name="1X06_NO_SILK" urn="urn:adsk.eagle:footprint:37750/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pad name="1" x="0" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="2" x="2.54" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="3" x="5.08" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="4" x="7.62" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="5" x="10.16" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<pad name="6" x="12.7" y="0" drill="1.016" diameter="1.8796" rot="R90"/>
<rectangle x1="12.446" y1="-0.254" x2="12.954" y2="0.254" layer="51"/>
<rectangle x1="9.906" y1="-0.254" x2="10.414" y2="0.254" layer="51"/>
<rectangle x1="7.366" y1="-0.254" x2="7.874" y2="0.254" layer="51"/>
<rectangle x1="4.826" y1="-0.254" x2="5.334" y2="0.254" layer="51"/>
<rectangle x1="2.286" y1="-0.254" x2="2.794" y2="0.254" layer="51"/>
<rectangle x1="-0.254" y1="-0.254" x2="0.254" y2="0.254" layer="51"/>
<text x="-1.27" y="1.397" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-1.27" y="-2.032" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
<package name="1X06_1.27MM" urn="urn:adsk.eagle:footprint:37751/1" library_version="1">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<wire x1="-0.381" y1="-0.889" x2="0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="-0.889" x2="0.635" y2="-0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="-0.635" x2="0.889" y2="-0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="-0.889" x2="1.651" y2="-0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="-0.889" x2="1.905" y2="-0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="-0.635" x2="2.159" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="-0.889" x2="2.921" y2="-0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="-0.889" x2="3.175" y2="-0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="-0.635" x2="3.429" y2="-0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="-0.889" x2="4.191" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="-0.889" x2="4.445" y2="-0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="-0.635" x2="4.699" y2="-0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="-0.889" x2="5.461" y2="-0.889" width="0.127" layer="21"/>
<wire x1="5.461" y1="0.889" x2="4.699" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.699" y1="0.889" x2="4.445" y2="0.635" width="0.127" layer="21"/>
<wire x1="4.445" y1="0.635" x2="4.191" y2="0.889" width="0.127" layer="21"/>
<wire x1="4.191" y1="0.889" x2="3.429" y2="0.889" width="0.127" layer="21"/>
<wire x1="3.429" y1="0.889" x2="3.175" y2="0.635" width="0.127" layer="21"/>
<wire x1="3.175" y1="0.635" x2="2.921" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.921" y1="0.889" x2="2.159" y2="0.889" width="0.127" layer="21"/>
<wire x1="2.159" y1="0.889" x2="1.905" y2="0.635" width="0.127" layer="21"/>
<wire x1="1.905" y1="0.635" x2="1.651" y2="0.889" width="0.127" layer="21"/>
<wire x1="1.651" y1="0.889" x2="0.889" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.889" y1="0.889" x2="0.635" y2="0.635" width="0.127" layer="21"/>
<wire x1="0.635" y1="0.635" x2="0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="0.381" y1="0.889" x2="-0.381" y2="0.889" width="0.127" layer="21"/>
<wire x1="-0.381" y1="0.889" x2="-0.889" y2="0.381" width="0.127" layer="21"/>
<wire x1="-0.889" y1="-0.381" x2="-0.381" y2="-0.889" width="0.127" layer="21"/>
<wire x1="-0.889" y1="0.381" x2="-0.889" y2="-0.381" width="0.127" layer="21"/>
<wire x1="5.461" y1="-0.889" x2="5.715" y2="-0.635" width="0.127" layer="21"/>
<wire x1="5.715" y1="-0.635" x2="5.969" y2="-0.889" width="0.127" layer="21"/>
<wire x1="5.969" y1="-0.889" x2="6.731" y2="-0.889" width="0.127" layer="21"/>
<wire x1="6.731" y1="0.889" x2="5.969" y2="0.889" width="0.127" layer="21"/>
<wire x1="5.969" y1="0.889" x2="5.715" y2="0.635" width="0.127" layer="21"/>
<wire x1="5.715" y1="0.635" x2="5.461" y2="0.889" width="0.127" layer="21"/>
<wire x1="6.731" y1="0.889" x2="7.239" y2="0.381" width="0.127" layer="21"/>
<wire x1="7.239" y1="0.381" x2="7.239" y2="-0.381" width="0.127" layer="21"/>
<wire x1="7.239" y1="-0.381" x2="6.731" y2="-0.889" width="0.127" layer="21"/>
<pad name="5" x="5.08" y="0" drill="0.508" diameter="1"/>
<pad name="4" x="3.81" y="0" drill="0.508" diameter="1"/>
<pad name="3" x="2.54" y="0" drill="0.508" diameter="1"/>
<pad name="2" x="1.27" y="0" drill="0.508" diameter="1"/>
<pad name="1" x="0" y="0" drill="0.508" diameter="1"/>
<pad name="6" x="6.35" y="0" drill="0.508" diameter="1"/>
<text x="-0.381" y="1.016" size="0.6096" layer="25" font="vector" ratio="20">&gt;NAME</text>
<text x="-0.381" y="-1.651" size="0.6096" layer="27" font="vector" ratio="20">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="1X02" urn="urn:adsk.eagle:package:38039/1" type="box" library_version="1">
<description>Plated Through Hole
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X2" urn="urn:adsk.eagle:package:38040/1" type="box" library_version="1">
<description>Molex 2-Pin Plated Through-Hole
Specifications:
Pin count:2
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="MOLEX-1X2"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2" urn="urn:adsk.eagle:package:38050/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2"/>
</packageinstances>
</package3d>
<package3d name="JST-2-SMD" urn="urn:adsk.eagle:package:38042/1" type="box" library_version="1">
<description>JST-Right Angle Male Header SMT
Specifications:
Pin count: 2
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
JST_2MM_MALE
</description>
<packageinstances>
<packageinstance name="JST-2-SMD"/>
</packageinstances>
</package3d>
<package3d name="1X02_BIG" urn="urn:adsk.eagle:package:38043/1" type="box" library_version="1">
<description>Plated Through Hole
Specifications:
Pin count:2
Pin pitch:0.15"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_BIG"/>
</packageinstances>
</package3d>
<package3d name="JST-2-SMD-VERT" urn="urn:adsk.eagle:package:38052/1" type="box" library_version="1">
<description>JST-Vertical Male Header SMT 
Specifications:
Pin count: 2
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-SMD-VERT"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-5MM-2" urn="urn:adsk.eagle:package:38044/1" type="box" library_version="1">
<description>Screw Terminal  5mm Pitch -2 Pin PTH
Specifications:
Pin count: 2
Pin pitch: 5mm/197mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-5MM-2"/>
</packageinstances>
</package3d>
<package3d name="1X02_LOCK" urn="urn:adsk.eagle:package:38045/1" type="box" library_version="1">
<description>Plated Through Hole - Locking Footprint
Holes are staggered by 0.005" from center to hold pins while soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LOCK"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X2_LOCK" urn="urn:adsk.eagle:package:38046/1" type="box" library_version="1">
<description>Molex 2-Pin Plated Through-Hole Locking Footprint
Holes are offset from center by 0.005" to hold pins in place during soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="MOLEX-1X2_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X02_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38047/1" type="box" library_version="1">
<description>Plated Through Hole - Long Pads with Locking Footprint
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2_LOCK" urn="urn:adsk.eagle:package:38049/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking
Holes are offset from center 0.005" to hold pins in place during soldering. 
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X02_LONGPADS" urn="urn:adsk.eagle:package:38048/1" type="box" library_version="1">
<description>Plated Through Hole - Long Pads without Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X02_NO_SILK" urn="urn:adsk.eagle:package:38051/1" type="box" library_version="1">
<description>Plated Through Hole - No Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH" urn="urn:adsk.eagle:package:38053/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH"/>
</packageinstances>
</package3d>
<package3d name="1X02_XTRA_BIG" urn="urn:adsk.eagle:package:38054/1" type="box" library_version="1">
<description>Plated Through Hole - 0.1" holes
Specifications:
Pin count:2
Pin pitch:0.2"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_XTRA_BIG"/>
</packageinstances>
</package3d>
<package3d name="1X02_PP_HOLES_ONLY" urn="urn:adsk.eagle:package:38058/1" type="box" library_version="1">
<description>Pogo Pins Connector - No Silk Outline
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_PP_HOLES_ONLY"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-2-NS" urn="urn:adsk.eagle:package:38055/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline
Specifications:
Pin count: 2
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-2-NS"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH-NS" urn="urn:adsk.eagle:package:38056/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole- No Silk
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
 No silk outline of connector. 
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH-NS"/>
</packageinstances>
</package3d>
<package3d name="JST-2-PTH-KIT" urn="urn:adsk.eagle:package:38057/1" type="box" library_version="1">
<description>JST 2 Pin Right Angle Plated Through  Hole - KIT
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
 This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
 This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
Specifications:
Pin count: 2
Pin pitch:2mm

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="JST-2-PTH-KIT"/>
</packageinstances>
</package3d>
<package3d name="SPRINGTERMINAL-2.54MM-2" urn="urn:adsk.eagle:package:38061/1" type="box" library_version="1">
<description>Spring Terminal- PCB Mount 2 Pin PTH
tDocu marks the spring arms
Specifications:
Pin count: 4
Pin pitch: 0.1"

Datasheet referenced for footprint
Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="SPRINGTERMINAL-2.54MM-2"/>
</packageinstances>
</package3d>
<package3d name="1X02_2.54_SCREWTERM" urn="urn:adsk.eagle:package:38059/1" type="box" library_version="1">
<description>2 Pin Screw Terminal - 2.54mm
Specifications:
Pin count:2
Pin pitch:0.1"

Example device(s):
CONN_02
</description>
<packageinstances>
<packageinstance name="1X02_2.54_SCREWTERM"/>
</packageinstances>
</package3d>
<package3d name="1X02_POKEHOME" urn="urn:adsk.eagle:package:38060/1" type="box" library_version="1">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
<packageinstances>
<packageinstance name="1X02_POKEHOME"/>
</packageinstances>
</package3d>
<package3d name="1X02_RA_PTH_FEMALE" urn="urn:adsk.eagle:package:38062/1" type="box" library_version="1">
<packageinstances>
<packageinstance name="1X02_RA_PTH_FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X04" urn="urn:adsk.eagle:package:38085/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X4" urn="urn:adsk.eagle:package:38087/1" type="box" library_version="1">
<description>Molex 4-Pin Plated Through-Hole
Specifications:
Pin count:4
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="MOLEX-1X4"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-4" urn="urn:adsk.eagle:package:38090/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -4 Pin PTH
Specifications:
Pin count: 4
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-4"/>
</packageinstances>
</package3d>
<package3d name="1X04_1.27MM" urn="urn:adsk.eagle:package:38086/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin
Specifications:
Pin count:4
Pin pitch: 1.27mm

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_1.27MM"/>
</packageinstances>
</package3d>
<package3d name="1X04_LOCK" urn="urn:adsk.eagle:package:38089/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin Locking Footprint
Pins are offset 0.005" from center to lock pins in place during soldering. 
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X04_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38091/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin Long Pads w/ Locking Footprint
Holes are offset 0.005" from center to lock pins in place during soldering. 
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X4_LOCK" urn="urn:adsk.eagle:package:38092/1" type="box" library_version="1">
<description>Molex 4-Pin Plated Through-Hole Locking
Holes are offset 0.005" from center to hold pins in place during soldering. 
Specifications:
Pin count:4
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="MOLEX-1X4_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X04_SMD_RA_MALE" urn="urn:adsk.eagle:package:38093/1" type="box" library_version="1">
<description>SMD - 4 Pin Right Angle Male Header
tDocu layer shows pin locations.
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_SMD_RA_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X04_LONGPADS" urn="urn:adsk.eagle:package:38098/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin Long Pads
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="1X04_NO_SILK" urn="urn:adsk.eagle:package:38094/1" type="box" library_version="1">
<description>Plated Through Hole - 4 Pin No Silk Outline
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="JST-4-PTH" urn="urn:adsk.eagle:package:38101/1" type="box" library_version="1">
<description>JST Right Angle 4 Pin Plated Through Hole
Specifications:
Pin count: 4
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="JST-4-PTH"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-4_LOCK" urn="urn:adsk.eagle:package:38095/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -4 Pin PTH Locking
Holes are offset 0.005" from center to hold pins in place during soldering. 
Specifications:
Pin count: 4
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-4_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X04_1MM_RA" urn="urn:adsk.eagle:package:38096/1" type="box" library_version="1">
<description>SMD- 4 Pin Right Angle 
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_1MM_RA"/>
</packageinstances>
</package3d>
<package3d name="1X04_SMD_VERTICAL_COMBO" urn="urn:adsk.eagle:package:38097/1" type="box" library_version="1">
<description>SMD - 4 Pin Vertical Connector
Specifications:
Pin count:4
SMD Pad count:8
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_SMD_VERTICAL_COMBO"/>
</packageinstances>
</package3d>
<package3d name="1X04_SMD_LONG" urn="urn:adsk.eagle:package:38099/1" type="box" library_version="1">
<description>SMD - 4 Pin w/ Long Solder Pads
No silk, but tDocu layer shows pin position. 
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_SMD_LONG"/>
</packageinstances>
</package3d>
<package3d name="JST-4-PTH-VERT" urn="urn:adsk.eagle:package:38102/1" type="box" library_version="1">
<description>JST Vertical 4 Pin Plated Through Hole
Specifications:
Pin count: 4
Pin pitch: 2mm

Datasheet referenced for footprint
Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="JST-4-PTH-VERT"/>
</packageinstances>
</package3d>
<package3d name="1X04_SMD_RA_FEMALE" urn="urn:adsk.eagle:package:38100/1" type="box" library_version="1">
<description>SMD - 4 Pin Right-Angle Female Header
Silk outline shows header location. 
Specifications:
Pin count:4
Pin pitch:0.1"

Example device(s):
CONN_04
</description>
<packageinstances>
<packageinstance name="1X04_SMD_RA_FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X06" urn="urn:adsk.eagle:package:38009/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6" urn="urn:adsk.eagle:package:38117/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6-RA" urn="urn:adsk.eagle:package:38118/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Right Angle
tPlace shows angle of connector. 
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6-RA"/>
</packageinstances>
</package3d>
<package3d name="1X06-SMD_RA_MALE" urn="urn:adsk.eagle:package:38004/1" type="box" library_version="1">
<description>SMD - 6 Pin Right Angle Male Header
tDocu layer shows pin locations.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06-SMD_RA_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X06_LOCK" urn="urn:adsk.eagle:package:38002/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Locking Footprint
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X06_LOCK_LONGPADS" urn="urn:adsk.eagle:package:38121/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Locking Footprint with Long Pads
Holes are offset 0.005" from center, locking pins in place during soldering.
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LOCK_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="MOLEX-1X6_LOCK" urn="urn:adsk.eagle:package:38123/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Locking Footprint
Holes are offset 0.005" from center to hold pins in place during soldering.  
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX-1X6_LOCK"/>
</packageinstances>
</package3d>
<package3d name="MOLEX_1X6_RA_LOCK" urn="urn:adsk.eagle:package:37992/1" type="box" library_version="1">
<description>Molex 6-Pin Plated Through-Hole Right Angle Locking Footprint
Holes are offset 0.005" from center to hold pins in place during soldering.  
tPlace shows location of connector.
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="MOLEX_1X6_RA_LOCK"/>
</packageinstances>
</package3d>
<package3d name="1X06_FEMALE_LOCK.010" urn="urn:adsk.eagle:package:38124/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin Locking Header
Includes silk outline for 6 pin female header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_FEMALE_LOCK.010"/>
</packageinstances>
</package3d>
<package3d name="1X06_LONGPADS" urn="urn:adsk.eagle:package:37991/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin with Long Pads
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_LONGPADS"/>
</packageinstances>
</package3d>
<package3d name="SCREWTERMINAL-3.5MM-6" urn="urn:adsk.eagle:package:38122/1" type="box" library_version="1">
<description>Screw Terminal  3.5mm Pitch -6 Pin PTH
Specifications:
Pin count: 6
Pin pitch: 3.5mm/138mil

Datasheet referenced for footprint
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="SCREWTERMINAL-3.5MM-6"/>
</packageinstances>
</package3d>
<package3d name="1X06-SMD-FEMALE" urn="urn:adsk.eagle:package:38125/1" type="box" library_version="1">
<description>Header - 6 pin Female SMD
Right angle 0.1"
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06-SMD-FEMALE"/>
</packageinstances>
</package3d>
<package3d name="1X06_HOLES_ONLY" urn="urn:adsk.eagle:package:38126/1" type="box" library_version="1">
<description> 6 Pin Holes
No silk, no plating
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_HOLES_ONLY"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT" urn="urn:adsk.eagle:package:38139/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT_ALT" urn="urn:adsk.eagle:package:38141/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header
Alternate pin configuration
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT_ALT"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_STRAIGHT_COMBO" urn="urn:adsk.eagle:package:38127/1" type="box" library_version="1">
<description> 6 Pin SMD Female Header - Combined Footprint

Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_STRAIGHT_COMBO"/>
</packageinstances>
</package3d>
<package3d name="1X06_SMD_MALE" urn="urn:adsk.eagle:package:38128/1" type="box" library_version="1">
<description> 6 Pin SMD Male Header
Specifications:
Pin count:6
Pin pitch:0.1"

Datasheet referenced for footprint:
Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_SMD_MALE"/>
</packageinstances>
</package3d>
<package3d name="1X06-1MM" urn="urn:adsk.eagle:package:38023/1" type="box" library_version="1">
<description>JST SH Vertical  6-Pin Connector -SMD
Specifications:
Pin count:6
Pin pitch:1mm
Datasheet referenced for footprint

Example device(s):
CONN_06
EM-406
</description>
<packageinstances>
<packageinstance name="1X06-1MM"/>
</packageinstances>
</package3d>
<package3d name="1X06_NO_SILK" urn="urn:adsk.eagle:package:38130/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin No Silk Outline
Specifications:
Pin count:6
Pin pitch:0.1"

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_NO_SILK"/>
</packageinstances>
</package3d>
<package3d name="1X06_1.27MM" urn="urn:adsk.eagle:package:38131/1" type="box" library_version="1">
<description>Plated Through Hole - 6 Pin
Specifications:
Pin count:6
Pin pitch:1.27mm

Example device(s):
CONN_06
</description>
<packageinstances>
<packageinstance name="1X06_1.27MM"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="CONN_02" urn="urn:adsk.eagle:symbol:37653/1" library_version="1">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<wire x1="3.81" y1="-2.54" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="1.27" y1="2.54" x2="2.54" y2="2.54" width="0.6096" layer="94"/>
<wire x1="1.27" y1="0" x2="2.54" y2="0" width="0.6096" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="3.81" y1="-2.54" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-2.54" y1="5.08" x2="3.81" y2="5.08" width="0.4064" layer="94"/>
<text x="-2.54" y="-4.826" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-2.54" y="5.588" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="7.62" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="7.62" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
<symbol name="CONN_04" urn="urn:adsk.eagle:symbol:37701/1" library_version="1">
<description>&lt;h3&gt;4 Pin Connection&lt;/h3&gt;</description>
<wire x1="1.27" y1="-5.08" x2="-5.08" y2="-5.08" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="2.54" x2="0" y2="2.54" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="0" x2="0" y2="0" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="-2.54" x2="0" y2="-2.54" width="0.6096" layer="94"/>
<wire x1="-5.08" y1="7.62" x2="-5.08" y2="-5.08" width="0.4064" layer="94"/>
<wire x1="1.27" y1="-5.08" x2="1.27" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="7.62" x2="1.27" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="5.08" x2="0" y2="5.08" width="0.6096" layer="94"/>
<text x="-5.08" y="-7.366" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-5.08" y="8.128" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="5.08" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="5.08" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="3" x="5.08" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="4" x="5.08" y="5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
<symbol name="CONN_06" urn="urn:adsk.eagle:symbol:37638/1" library_version="1">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;</description>
<wire x1="1.27" y1="-7.62" x2="-5.08" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="0" x2="0" y2="0" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="-2.54" x2="0" y2="-2.54" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="-5.08" x2="0" y2="-5.08" width="0.6096" layer="94"/>
<wire x1="-5.08" y1="10.16" x2="-5.08" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="1.27" y1="-7.62" x2="1.27" y2="10.16" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="10.16" x2="1.27" y2="10.16" width="0.4064" layer="94"/>
<wire x1="-1.27" y1="5.08" x2="0" y2="5.08" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="2.54" x2="0" y2="2.54" width="0.6096" layer="94"/>
<wire x1="-1.27" y1="7.62" x2="0" y2="7.62" width="0.6096" layer="94"/>
<text x="-5.08" y="-9.906" size="1.778" layer="96" font="vector">&gt;VALUE</text>
<text x="-5.08" y="10.668" size="1.778" layer="95" font="vector">&gt;NAME</text>
<pin name="1" x="5.08" y="-5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="2" x="5.08" y="-2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="3" x="5.08" y="0" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="4" x="5.08" y="2.54" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="5" x="5.08" y="5.08" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
<pin name="6" x="5.08" y="7.62" visible="pad" length="middle" direction="pas" swaplevel="1" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CONN_02" urn="urn:adsk.eagle:component:38323/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="CONN_02" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38039/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38040/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38050/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38042/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38043/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38052/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38044/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08432" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38045/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38046/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38047/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38049/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38048/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38051/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38053/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863" constant="no"/>
<attribute name="SKU" value="PRT-09914" constant="no"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38054/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38058/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38055/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399" constant="no"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38056/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38057/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38061/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38059/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_POKEHOME" package="1X02_POKEHOME">
<connects>
<connect gate="G$1" pin="1" pad="P1 P3"/>
<connect gate="G$1" pin="2" pad="P2 P4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38060/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
</technology>
</technologies>
</device>
<device name="PTH_RA_FEMALE" package="1X02_RA_PTH_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38062/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13700"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04" urn="urn:adsk.eagle:component:38327/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="G$1" symbol="CONN_04" x="-2.54" y="0"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38085/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696" constant="no"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38087/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08186" constant="no"/>
<attribute name="SF_ID" value="PRT-08231" constant="no"/>
</technology>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38090/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="2xCONN-08399" constant="no"/>
<attribute name="SF_ID" value="2xPRT-08084" constant="no"/>
</technology>
</technologies>
</device>
<device name="1.27MM" package="1X04_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38086/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X04_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38089/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X04_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38091/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696" constant="no"/>
</technology>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38092/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08186" constant="no"/>
<attribute name="SF_ID" value="PRT-08231" constant="no"/>
</technology>
</technologies>
</device>
<device name="SMD" package="1X04_SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38093/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09140" constant="no"/>
<attribute name="SF_ID" value="PRT-12638" constant="no"/>
</technology>
</technologies>
</device>
<device name="LONGPADS" package="1X04_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38098/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696" constant="no"/>
</technology>
</technologies>
</device>
<device name="1X04_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38094/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696" constant="no"/>
</technology>
</technologies>
</device>
<device name="JST-PTH" package="JST-4-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38101/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WIRE-13531" constant="no"/>
<attribute name="SF_ID" value="PRT-09916" constant="no"/>
</technology>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-4_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38095/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="1X04_1MM_RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38096/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10310" constant="no"/>
<attribute name="SF_ID" value="PRT-10208" constant="no"/>
</technology>
</technologies>
</device>
<device name="SMD_STRAIGHT_COMBO" package="1X04_SMD_VERTICAL_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38097/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08511"/>
<attribute name="VALUE" value="1X04_SMD_STRAIGHT_COMBO"/>
</technology>
</technologies>
</device>
<device name="SMD_LONG" package="1X04_SMD_LONG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38099/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09140" constant="no"/>
<attribute name="SF_ID" value="PRT-12638" constant="no"/>
</technology>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-4-PTH-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38102/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13251"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_FEMALE" package="1X04_SMD_RA_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38100/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12382" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06" urn="urn:adsk.eagle:component:38332/1" prefix="J" uservalue="yes" library_version="1">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9280"&gt; Arduino Stackable Header - 6 Pin&lt;/a&gt; (PRT-09280)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06" x="-2.54" y="0"/>
</gates>
<devices>
<device name="SILK_FEMALE_PTH" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38009/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38117/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38118/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38004/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08971" constant="no"/>
<attribute name="VALUE" value="RA 6Pin SMD" constant="no"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38002/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38121/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38123/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX_1X6_RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:37992/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38124/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:37991/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38122/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38125/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09668"/>
</technology>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X06_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38126/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-FEMALE" package="1X06_SMD_STRAIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38139/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT-FEMALE" package="1X06_SMD_STRAIGHT_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38141/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-COMBO-FEMALE" package="1X06_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38127/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD_MALE" package="1X06_SMD_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38128/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11293"/>
</technology>
</technologies>
</device>
<device name="SMD-1MM" package="1X06-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38023/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08249" constant="no"/>
<attribute name="SF_ID" value="GPS-00579" constant="no"/>
</technology>
</technologies>
</device>
<device name="NO_SILK_FEMALE_PTH" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38130/1"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="1.27MM" package="1X06_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38131/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK_NO_POP" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:38130/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="eScooter">
<packages>
<package name="DIOM5027X220N" urn="urn:adsk.eagle:footprint:21928331/1">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<wire x1="2.5" y1="1.35" x2="-3.3699" y2="1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="1.35" x2="-3.3699" y2="-1.35" width="0.12" layer="21"/>
<wire x1="-3.3699" y1="-1.35" x2="2.5" y2="-1.35" width="0.12" layer="21"/>
<wire x1="2.5" y1="-1.35" x2="-2.5" y2="-1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="-1.35" x2="-2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="-2.5" y1="1.35" x2="2.5" y2="1.35" width="0.12" layer="51"/>
<wire x1="2.5" y1="1.35" x2="2.5" y2="-1.35" width="0.12" layer="51"/>
<smd name="1" x="-2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<smd name="2" x="2.1" y="0" dx="1.9118" dy="1.5118" layer="1"/>
<text x="0" y="1.985" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-1.985" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="CAPAE1230X1250N" urn="urn:adsk.eagle:footprint:21812987/1">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<wire x1="-6.25" y1="1.3186" x2="-6.25" y2="3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="3.6573" x2="-3.6573" y2="6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="1.3186" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-1.3186" x2="-6.25" y2="-3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-3.6573" x2="-3.6573" y2="-6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="-6.25" x2="6.25" y2="-6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="6.25" y2="-1.3186" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="-6.25" y2="-6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="-6.25" x2="-6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="-6.25" width="0.12" layer="51"/>
<smd name="1" x="-4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<smd name="2" x="4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<text x="0" y="6.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="DIP8" urn="urn:adsk.eagle:footprint:4470/1">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; Gull Wing Surface Mount Optioon 300&lt;p&gt;
Source: http://www.avagotech.com/docs/AV02-0410EN</description>
<wire x1="-4.81" y1="-3.075" x2="4.81" y2="-3.075" width="0.2032" layer="51"/>
<wire x1="4.81" y1="-3.075" x2="4.81" y2="3.075" width="0.2032" layer="21"/>
<wire x1="4.81" y1="3.075" x2="-4.81" y2="3.075" width="0.2032" layer="51"/>
<wire x1="-4.81" y1="3.075" x2="-4.81" y2="-3.075" width="0.2032" layer="21"/>
<circle x="-3.81" y="-2.159" radius="0.3667" width="0" layer="21"/>
<smd name="1" x="-3.81" y="-4.45" dx="1.16" dy="2" layer="1"/>
<smd name="2" x="-1.27" y="-4.45" dx="1.27" dy="2" layer="1"/>
<smd name="3" x="1.27" y="-4.45" dx="1.27" dy="2" layer="1"/>
<smd name="4" x="3.81" y="-4.45" dx="1.16" dy="2" layer="1"/>
<smd name="5" x="3.81" y="4.45" dx="1.16" dy="2" layer="1"/>
<smd name="6" x="1.27" y="4.45" dx="1.27" dy="2" layer="1"/>
<smd name="7" x="-1.27" y="4.45" dx="1.27" dy="2" layer="1"/>
<smd name="8" x="-3.81" y="4.45" dx="1.16" dy="2" layer="1"/>
<text x="-5.635" y="-3.1351" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.905" y="-4.4051" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-4.0899" y1="-4.825" x2="-3.5301" y2="-3.81" layer="51"/>
<rectangle x1="-1.5499" y1="-4.825" x2="-0.9901" y2="-3.81" layer="51"/>
<rectangle x1="0.9901" y1="-4.825" x2="1.5499" y2="-3.81" layer="51"/>
<rectangle x1="3.5301" y1="-4.825" x2="4.0899" y2="-3.81" layer="51"/>
<rectangle x1="3.5301" y1="3.81" x2="4.0899" y2="4.825" layer="51"/>
<rectangle x1="0.9901" y1="3.81" x2="1.5499" y2="4.825" layer="51"/>
<rectangle x1="-1.5499" y1="3.81" x2="-0.9901" y2="4.825" layer="51"/>
<rectangle x1="-4.0899" y1="3.81" x2="-3.5301" y2="4.825" layer="51"/>
<rectangle x1="-2.15" y1="3.1" x2="-0.4" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="-4.1" y1="3.1" x2="-2.94" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="0.39" y1="3.1" x2="2.14" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="2.93" y1="3.1" x2="4.1" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="-4.075" y1="-3.81" x2="-2.93" y2="-3.1" layer="51"/>
<rectangle x1="-2.14" y1="-3.81" x2="-0.39" y2="-3.1" layer="51"/>
<rectangle x1="0.4" y1="-3.81" x2="2.15" y2="-3.1" layer="51"/>
<rectangle x1="2.94" y1="-3.81" x2="4.1" y2="-3.1" layer="51"/>
</package>
<package name="DIP826W56P254L937H458Q8B" urn="urn:adsk.eagle:footprint:22059849/1">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span, 9.38 X 6.99 X 4.58 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span with body size 9.38 X 6.99 X 4.58 mm&lt;/p&gt;</description>
<circle x="-5.3669" y="3.81" radius="0.25" width="0" layer="21"/>
<wire x1="-3.935" y1="4.7969" x2="-3.935" y2="4.955" width="0.12" layer="21"/>
<wire x1="-3.935" y1="4.955" x2="3.935" y2="4.955" width="0.12" layer="21"/>
<wire x1="3.935" y1="4.955" x2="3.935" y2="4.7969" width="0.12" layer="21"/>
<wire x1="-3.935" y1="-4.7969" x2="-3.935" y2="-4.955" width="0.12" layer="21"/>
<wire x1="-3.935" y1="-4.955" x2="3.935" y2="-4.955" width="0.12" layer="21"/>
<wire x1="3.935" y1="-4.955" x2="3.935" y2="-4.7969" width="0.12" layer="21"/>
<wire x1="3.935" y1="-4.955" x2="-3.935" y2="-4.955" width="0.12" layer="51"/>
<wire x1="-3.935" y1="-4.955" x2="-3.935" y2="4.955" width="0.12" layer="51"/>
<wire x1="-3.935" y1="4.955" x2="3.935" y2="4.955" width="0.12" layer="51"/>
<wire x1="3.935" y1="4.955" x2="3.935" y2="-4.955" width="0.12" layer="51"/>
<pad name="1" x="-4.13" y="3.81" drill="0.8657" diameter="1.4657"/>
<pad name="2" x="-4.13" y="1.27" drill="0.8657" diameter="1.4657"/>
<pad name="3" x="-4.13" y="-1.27" drill="0.8657" diameter="1.4657"/>
<pad name="4" x="-4.13" y="-3.81" drill="0.8657" diameter="1.4657"/>
<pad name="5" x="4.13" y="-3.81" drill="0.8657" diameter="1.4657"/>
<pad name="6" x="4.13" y="-1.27" drill="0.8657" diameter="1.4657"/>
<pad name="7" x="4.13" y="1.27" drill="0.8657" diameter="1.4657"/>
<pad name="8" x="4.13" y="3.81" drill="0.8657" diameter="1.4657"/>
<text x="0" y="5.59" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-5.59" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="XT60">
<pad name="GND" x="-3.6" y="0" drill="2.6" diameter="4" shape="square"/>
<pad name="VCC" x="3.6" y="0" drill="2.6" diameter="4"/>
<text x="-2.9" y="3.5" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.1" y="-4.1" size="1.27" layer="27">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DIOM5027X220N" urn="urn:adsk.eagle:package:21928182/1" type="model">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIOM5027X220N"/>
</packageinstances>
</package3d>
<package3d name="CAPAE1230X1250N" urn="urn:adsk.eagle:package:21812541/1" type="model">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE1230X1250N"/>
</packageinstances>
</package3d>
<package3d name="DIP8" urn="urn:adsk.eagle:package:8089856/1" locally_modified="yes" type="box">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; &lt;p&gt;
dual in line package'</description>
<packageinstances>
<packageinstance name="DIP8"/>
</packageinstances>
</package3d>
<package3d name="DIP826W56P254L937H458Q8B" urn="urn:adsk.eagle:package:22059831/1" type="model">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span, 9.38 X 6.99 X 4.58 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 8.26 mm (0.33 in) span with body size 9.38 X 6.99 X 4.58 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="DIP826W56P254L937H458Q8B"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="TVS_DIODE">
<wire x1="0" y1="0" x2="-2.54" y2="2.54" width="0.254" layer="94"/>
<wire x1="2.54" y1="2.54" x2="0" y2="0" width="0.254" layer="94"/>
<wire x1="-5.08" y1="-2.54" x2="-2.54" y2="0" width="0.254" layer="94"/>
<wire x1="-2.54" y1="0" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="5.08" y2="2.54" width="0.254" layer="94"/>
<wire x1="0" y1="0" x2="-2.54" y2="-2.54" width="0.254" layer="94"/>
<wire x1="2.54" y1="-2.54" x2="0" y2="0" width="0.254" layer="94"/>
<wire x1="-2.54" y1="2.54" x2="2.54" y2="2.54" width="0.254" layer="94"/>
<wire x1="-2.54" y1="-2.54" x2="2.54" y2="-2.54" width="0.254" layer="94"/>
<pin name="P$1" x="0" y="7.62" visible="off" length="middle" rot="R270"/>
<pin name="P$2" x="0" y="-7.62" visible="off" length="middle" rot="R90"/>
<text x="2.54" y="5.08" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-7.62" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="C">
<wire x1="-2.54" y1="1.27" x2="2.54" y2="1.27" width="0.254" layer="94"/>
<wire x1="-2.54" y1="-1.016" x2="2.54" y2="-1.016" width="0.254" layer="94" curve="-90"/>
<pin name="P$1" x="0" y="6.35" visible="off" length="middle" direction="pwr" rot="R270"/>
<pin name="P$2" x="0" y="-5.08" visible="off" length="middle" direction="pwr" rot="R90"/>
<text x="-3.81" y="1.27" size="1.778" layer="94">+</text>
<text x="2.54" y="2.54" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-5.08" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="MX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<wire x1="-10.16" y1="12.7" x2="10.16" y2="12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="12.7" x2="10.16" y2="-12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="-12.7" x2="-10.16" y2="-12.7" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-12.7" x2="-10.16" y2="12.7" width="0.254" layer="94"/>
<pin name="BST" x="-15.24" y="7.62" length="middle" direction="in"/>
<pin name="VD" x="-15.24" y="2.54" length="middle" direction="in"/>
<pin name="SGND" x="-15.24" y="-2.54" length="middle" direction="in"/>
<pin name="FB" x="-15.24" y="-7.62" length="middle" direction="in"/>
<pin name="ON/OFF" x="15.24" y="-7.62" length="middle" direction="in" rot="R180"/>
<pin name="GND" x="15.24" y="-2.54" length="middle" direction="pwr" rot="R180"/>
<pin name="VIN" x="15.24" y="2.54" length="middle" direction="pwr" rot="R180"/>
<pin name="LX" x="15.24" y="7.62" length="middle" direction="pwr" rot="R180"/>
<text x="-10.16" y="15.24" size="1.778" layer="95">&gt;NAME</text>
<text x="-10.16" y="-17.78" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="XT60">
<description>XT60 connector</description>
<pin name="P$1" x="-5.08" y="5.08" visible="off" length="middle" direction="sup"/>
<pin name="P$2" x="-5.08" y="2.54" visible="off" length="middle" direction="sup"/>
<wire x1="-2.54" y1="7.62" x2="2.54" y2="7.62" width="0.254" layer="94"/>
<wire x1="2.54" y1="7.62" x2="2.54" y2="0" width="0.254" layer="94"/>
<wire x1="2.54" y1="0" x2="-2.54" y2="0" width="0.254" layer="94"/>
<wire x1="-2.54" y1="0" x2="-2.54" y2="7.62" width="0.254" layer="94"/>
<text x="-5.08" y="10.16" size="1.778" layer="95">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="TVS_DIODE">
<description>TVS protective diode</description>
<gates>
<gate name="D$1" symbol="TVS_DIODE" x="0" y="0"/>
</gates>
<devices>
<device name="SMA" package="DIOM5027X220N">
<connects>
<connect gate="D$1" pin="P$1" pad="1"/>
<connect gate="D$1" pin="P$2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:21928182/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C">
<gates>
<gate name="G$1" symbol="C" x="-1.27" y="-1.27"/>
</gates>
<devices>
<device name="PANASONIC_H13" package="CAPAE1230X1250N">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:21812541/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<gates>
<gate name="G$1" symbol="MX5035" x="0" y="0"/>
</gates>
<devices>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="BST" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="ON/OFF" pad="5"/>
<connect gate="G$1" pin="SGND" pad="3"/>
<connect gate="G$1" pin="VD" pad="2"/>
<connect gate="G$1" pin="VIN" pad="7"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:8089856/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PDIP8" package="DIP826W56P254L937H458Q8B">
<connects>
<connect gate="G$1" pin="BST" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="ON/OFF" pad="5"/>
<connect gate="G$1" pin="SGND" pad="3"/>
<connect gate="G$1" pin="VD" pad="2"/>
<connect gate="G$1" pin="VIN" pad="7"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:22059831/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XT60">
<gates>
<gate name="G$1" symbol="XT60" x="0" y="0"/>
</gates>
<devices>
<device name="" package="XT60">
<connects>
<connect gate="G$1" pin="P$1" pad="GND"/>
<connect gate="G$1" pin="P$2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Transistor">
<description>&lt;B&gt;BJT, JFET, MOSFET, UJT, Darlington</description>
<packages>
<package name="SOT23" urn="urn:adsk.eagle:footprint:28669/1">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
<wire x1="1.4224" y1="0.6604" x2="1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="1.4224" y1="-0.6604" x2="-1.4224" y2="-0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="-0.6604" x2="-1.4224" y2="0.6604" width="0.1524" layer="51"/>
<wire x1="-1.4224" y1="0.6604" x2="1.4224" y2="0.6604" width="0.1524" layer="51"/>
<smd name="3" x="0" y="1.1" dx="1" dy="1.4" layer="1"/>
<smd name="2" x="0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<smd name="1" x="-0.95" y="-1.1" dx="1" dy="1.4" layer="1"/>
<text x="-1.905" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.2286" y1="0.7112" x2="0.2286" y2="1.2954" layer="51"/>
<rectangle x1="0.7112" y1="-1.2954" x2="1.1684" y2="-0.7112" layer="51"/>
<rectangle x1="-1.1684" y1="-1.2954" x2="-0.7112" y2="-0.7112" layer="51"/>
</package>
<package name="TO92" urn="urn:adsk.eagle:footprint:28459/1">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
<wire x1="-2.0946" y1="-1.651" x2="-2.6549" y2="-0.254" width="0.127" layer="21" curve="-32.781"/>
<wire x1="-2.6549" y1="-0.254" x2="-0.7863" y2="2.5485" width="0.127" layer="21" curve="-78.3185"/>
<wire x1="0.7863" y1="2.5484" x2="2.0945" y2="-1.651" width="0.127" layer="21" curve="-111.1"/>
<wire x1="-2.0945" y1="-1.651" x2="2.0945" y2="-1.651" width="0.127" layer="21"/>
<wire x1="-2.2537" y1="-0.254" x2="-0.2863" y2="-0.254" width="0.127" layer="51"/>
<wire x1="-2.6549" y1="-0.254" x2="-2.2537" y2="-0.254" width="0.127" layer="21"/>
<wire x1="-0.2863" y1="-0.254" x2="0.2863" y2="-0.254" width="0.127" layer="21"/>
<wire x1="2.2537" y1="-0.254" x2="2.6549" y2="-0.254" width="0.127" layer="21"/>
<wire x1="0.2863" y1="-0.254" x2="2.2537" y2="-0.254" width="0.127" layer="51"/>
<wire x1="-0.7863" y1="2.5485" x2="0.7863" y2="2.5485" width="0.127" layer="51" curve="-34.2936"/>
<pad name="1" x="1.27" y="0" drill="0.8128" shape="octagon"/>
<pad name="2" x="0" y="1.905" drill="0.8128" shape="octagon"/>
<pad name="3" x="-1.27" y="0" drill="0.8128" shape="octagon"/>
<text x="3.175" y="0.635" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="3.175" y="-1.27" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<text x="-0.635" y="0.635" size="1.27" layer="51" ratio="10">2</text>
<text x="-2.159" y="0" size="1.27" layer="51" ratio="10">3</text>
<text x="1.143" y="0" size="1.27" layer="51" ratio="10">1</text>
</package>
<package name="TO220BV" urn="urn:adsk.eagle:footprint:29371/1">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
<wire x1="4.699" y1="-4.318" x2="4.953" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="4.699" y1="-4.318" x2="-4.699" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-4.064" x2="-4.699" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="5.08" y1="-1.143" x2="4.953" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-4.064" x2="-5.08" y2="-1.143" width="0.1524" layer="21"/>
<circle x="-4.4958" y="-3.7084" radius="0.254" width="0" layer="21"/>
<pad name="G" x="-2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="D" x="0" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="S" x="2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<text x="-5.08" y="-6.0452" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-5.08" y="-7.62" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<rectangle x1="-5.334" y1="-0.762" x2="5.334" y2="0" layer="21"/>
<rectangle x1="-5.334" y1="-1.27" x2="-3.429" y2="-0.762" layer="21"/>
<rectangle x1="-1.651" y1="-1.27" x2="-0.889" y2="-0.762" layer="21"/>
<rectangle x1="-3.429" y1="-1.27" x2="-1.651" y2="-0.762" layer="51"/>
<rectangle x1="0.889" y1="-1.27" x2="1.651" y2="-0.762" layer="21"/>
<rectangle x1="3.429" y1="-1.27" x2="5.334" y2="-0.762" layer="21"/>
<rectangle x1="-0.889" y1="-1.27" x2="0.889" y2="-0.762" layer="51"/>
<rectangle x1="1.651" y1="-1.27" x2="3.429" y2="-0.762" layer="51"/>
</package>
<package name="DPACK_3" urn="urn:adsk.eagle:footprint:8083910/1">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 3 (Motorola)</description>
<wire x1="3.2766" y1="3.8354" x2="3.277" y2="-2.159" width="0.2032" layer="21"/>
<wire x1="3.277" y1="-2.159" x2="-3.277" y2="-2.159" width="0.2032" layer="21"/>
<wire x1="-3.277" y1="-2.159" x2="-3.2766" y2="3.8354" width="0.2032" layer="21"/>
<wire x1="-3.277" y1="3.835" x2="3.2774" y2="3.8346" width="0.2032" layer="51"/>
<wire x1="-2.5654" y1="3.937" x2="-2.5654" y2="4.6482" width="0.2032" layer="51"/>
<wire x1="-2.5654" y1="4.6482" x2="-2.1082" y2="5.1054" width="0.2032" layer="51"/>
<wire x1="-2.1082" y1="5.1054" x2="2.1082" y2="5.1054" width="0.2032" layer="51"/>
<wire x1="2.1082" y1="5.1054" x2="2.5654" y2="4.6482" width="0.2032" layer="51"/>
<wire x1="2.5654" y1="4.6482" x2="2.5654" y2="3.937" width="0.2032" layer="51"/>
<wire x1="2.5654" y1="3.937" x2="-2.5654" y2="3.937" width="0.2032" layer="51"/>
<smd name="C" x="0" y="2.5" dx="5.4" dy="6.2" layer="1"/>
<smd name="A1" x="-2.28" y="-4.8" dx="1" dy="1.6" layer="1"/>
<smd name="A2" x="2.28" y="-4.8" dx="1" dy="1.6" layer="1"/>
<text x="-3.81" y="-2.54" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="5.08" y="-2.54" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-2.7178" y1="-5.1562" x2="-1.8542" y2="-2.2606" layer="51"/>
<rectangle x1="1.8542" y1="-5.1562" x2="2.7178" y2="-2.2606" layer="51"/>
<rectangle x1="-0.4318" y1="-3.0226" x2="0.4318" y2="-2.2606" layer="21"/>
<polygon width="0.1998" layer="51">
<vertex x="-2.5654" y="3.937"/>
<vertex x="-2.5654" y="4.6482"/>
<vertex x="-2.1082" y="5.1054"/>
<vertex x="2.1082" y="5.1054"/>
<vertex x="2.5654" y="4.6482"/>
<vertex x="2.5654" y="3.937"/>
</polygon>
</package>
<package name="SOT95P237X112-3N" urn="urn:adsk.eagle:footprint:16378720/1">
<description>3-SOT23, 0.95 mm pitch, 2.37 mm span, 2.86 X 1.28 X 1.12 mm body
&lt;p&gt;3-pin SOT23 package with 0.95 mm pitch, 2.37 mm span with body size 2.86 X 1.28 X 1.12 mm&lt;/p&gt;</description>
<circle x="-1.204" y="1.7664" radius="0.25" width="0" layer="21"/>
<wire x1="-0.7" y1="1.5764" x2="0.7" y2="1.5764" width="0.12" layer="21"/>
<wire x1="0.7" y1="1.5764" x2="0.7" y2="0.5664" width="0.12" layer="21"/>
<wire x1="-0.7" y1="-1.5764" x2="0.7" y2="-1.5764" width="0.12" layer="21"/>
<wire x1="0.7" y1="-1.5764" x2="0.7" y2="-0.5664" width="0.12" layer="21"/>
<wire x1="0.7" y1="-1.525" x2="-0.7" y2="-1.525" width="0.12" layer="51"/>
<wire x1="-0.7" y1="-1.525" x2="-0.7" y2="1.525" width="0.12" layer="51"/>
<wire x1="-0.7" y1="1.525" x2="0.7" y2="1.525" width="0.12" layer="51"/>
<wire x1="0.7" y1="1.525" x2="0.7" y2="-1.525" width="0.12" layer="51"/>
<smd name="1" x="-1.064" y="0.95" dx="1.2235" dy="0.6248" layer="1"/>
<smd name="2" x="-1.064" y="-0.95" dx="1.2235" dy="0.6248" layer="1"/>
<smd name="3" x="1.064" y="0" dx="1.2235" dy="0.6248" layer="1"/>
<text x="0" y="2.6514" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-2.2114" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
<package name="SC59" urn="urn:adsk.eagle:footprint:29647/1">
<description>&lt;b&gt;ROHM : SMT3 ; EIAJ : SC-59&lt;/b&gt;</description>
<wire x1="1.4224" y1="0.8604" x2="1.4224" y2="-0.8604" width="0.127" layer="51"/>
<wire x1="1.4224" y1="-0.8604" x2="-1.4224" y2="-0.8604" width="0.127" layer="51"/>
<wire x1="-1.4224" y1="-0.8604" x2="-1.4224" y2="0.8604" width="0.127" layer="51"/>
<wire x1="-1.4224" y1="0.8604" x2="1.4224" y2="0.8604" width="0.127" layer="51"/>
<smd name="C" x="0" y="1.2" dx="1" dy="1.4" layer="1"/>
<smd name="E" x="0.95" y="-1.2" dx="1" dy="1.4" layer="1"/>
<smd name="B" x="-0.95" y="-1.2" dx="1" dy="1.4" layer="1"/>
<text x="-1.905" y="1.905" size="1.27" layer="25">&gt;NAME</text>
<text x="-1.905" y="-3.175" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.2286" y1="0.9112" x2="0.2286" y2="1.4954" layer="51"/>
<rectangle x1="0.7112" y1="-1.4954" x2="1.1684" y2="-0.9112" layer="51"/>
<rectangle x1="-1.1684" y1="-1.4954" x2="-0.7112" y2="-0.9112" layer="51"/>
</package>
<package name="SC70" urn="urn:adsk.eagle:footprint:29646/1">
<description>&lt;b&gt;SC70-3 Reflow soldering&lt;/b&gt;&lt;p&gt;
Philips SC01_Mounting_1996.pdf&lt;p&gt;
ROHM : UMT3 ; EIAJ : SC-70</description>
<wire x1="0.9224" y1="0.4604" x2="0.9224" y2="-0.4604" width="0.1524" layer="51"/>
<wire x1="0.9224" y1="-0.4604" x2="-0.9224" y2="-0.4604" width="0.1524" layer="51"/>
<wire x1="-0.9224" y1="-0.4604" x2="-0.9224" y2="0.4604" width="0.1524" layer="51"/>
<wire x1="-0.9224" y1="0.4604" x2="0.9224" y2="0.4604" width="0.1524" layer="51"/>
<wire x1="0.9224" y1="0.4604" x2="0.9224" y2="-0.4604" width="0.1524" layer="21"/>
<wire x1="0.9224" y1="-0.4604" x2="-0.9224" y2="-0.4604" width="0.1524" layer="21"/>
<wire x1="-0.9224" y1="-0.4604" x2="-0.9224" y2="0.4604" width="0.1524" layer="21"/>
<wire x1="-0.9224" y1="0.4604" x2="0.9224" y2="0.4604" width="0.1524" layer="21"/>
<smd name="1" x="-0.65" y="-0.925" dx="0.6" dy="0.55" layer="1"/>
<smd name="2" x="0.65" y="-0.925" dx="0.6" dy="0.55" layer="1"/>
<smd name="3" x="0" y="0.925" dx="0.6" dy="0.55" layer="1"/>
<text x="-1" y="1.3" size="1.27" layer="25">&gt;NAME</text>
<text x="-1" y="-2.6" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-0.8" y1="-1.1" x2="-0.5" y2="-0.5" layer="51"/>
<rectangle x1="0.5" y1="-1.1" x2="0.8" y2="-0.5" layer="51"/>
<rectangle x1="-0.15" y1="0.5" x2="0.15" y2="1.1" layer="51"/>
</package>
<package name="TO18" urn="urn:adsk.eagle:footprint:28463/1">
<description>&lt;b&gt;TO 18&lt;/b&gt;</description>
<wire x1="0.9289" y1="2.227" x2="2.227" y2="0.9289" width="0.0508" layer="51" curve="-44.7172"/>
<wire x1="0.9289" y1="-2.227" x2="2.227" y2="-0.9289" width="0.0508" layer="51" curve="44.7172"/>
<wire x1="-3.937" y1="-0.508" x2="-3.937" y2="0.508" width="0.127" layer="21"/>
<wire x1="-2.227" y1="-0.9289" x2="0.929" y2="2.2271" width="0.0508" layer="21" curve="-135.281"/>
<wire x1="-2.227" y1="-0.9289" x2="-0.9289" y2="-2.227" width="0.0508" layer="51" curve="44.7172"/>
<wire x1="-3.937" y1="-0.508" x2="-2.8765" y2="-0.508" width="0.127" layer="21"/>
<wire x1="-0.9289" y1="-2.227" x2="0.9289" y2="-2.227" width="0.0508" layer="21" curve="45.2828"/>
<wire x1="-3.937" y1="0.508" x2="-2.8765" y2="0.508" width="0.127" layer="21"/>
<wire x1="2.227" y1="-0.9289" x2="2.227" y2="0.9289" width="0.0508" layer="21" curve="45.2828"/>
<circle x="0" y="0" radius="2.921" width="0.127" layer="21"/>
<pad name="1" x="-1.27" y="-1.27" drill="0.8128" shape="octagon"/>
<pad name="2" x="1.27" y="-1.27" drill="0.8128" shape="octagon"/>
<pad name="3" x="1.27" y="1.27" drill="0.8128" shape="octagon"/>
<text x="3.175" y="0" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="3.175" y="-1.905" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<text x="-1.905" y="-1.27" size="1.27" layer="51" ratio="10">1</text>
<text x="0.635" y="-1.27" size="1.27" layer="51" ratio="10">2</text>
<text x="0" y="0.635" size="1.27" layer="51" ratio="10">3</text>
</package>
</packages>
<packages3d>
<package3d name="SOT23" urn="urn:adsk.eagle:package:28738/2" type="model">
<description>SOT-23</description>
<packageinstances>
<packageinstance name="SOT23"/>
</packageinstances>
</package3d>
<package3d name="TO92" urn="urn:adsk.eagle:package:16378726/2" type="model">
<description>TO 92</description>
<packageinstances>
<packageinstance name="TO92"/>
</packageinstances>
</package3d>
<package3d name="TO220BV" urn="urn:adsk.eagle:package:29484/4" type="model">
<description>Molded Package
grid 2.54 mm</description>
<packageinstances>
<packageinstance name="TO220BV"/>
</packageinstances>
</package3d>
<package3d name="DPACK_3" urn="urn:adsk.eagle:package:8087963/1" type="box">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 3 (Motorola)</description>
<packageinstances>
<packageinstance name="DPACK_3"/>
</packageinstances>
</package3d>
<package3d name="SOT95P237X112-3N" urn="urn:adsk.eagle:package:16378725/1" type="model">
<description>3-SOT23, 0.95 mm pitch, 2.37 mm span, 2.86 X 1.28 X 1.12 mm body
&lt;p&gt;3-pin SOT23 package with 0.95 mm pitch, 2.37 mm span with body size 2.86 X 1.28 X 1.12 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="SOT95P237X112-3N"/>
</packageinstances>
</package3d>
<package3d name="SC59" urn="urn:adsk.eagle:package:29756/2" type="model">
<description>ROHM : SMT3 ; EIAJ : SC-59</description>
<packageinstances>
<packageinstance name="SC59"/>
</packageinstances>
</package3d>
<package3d name="SC70" urn="urn:adsk.eagle:package:29755/2" type="model">
<description>SC70-3 Reflow soldering
Philips SC01_Mounting_1996.pdf
ROHM : UMT3 ; EIAJ : SC-70</description>
<packageinstances>
<packageinstance name="SC70"/>
</packageinstances>
</package3d>
<package3d name="TO18" urn="urn:adsk.eagle:package:16378727/1" type="model">
<description>TO 18</description>
<packageinstances>
<packageinstance name="TO18"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="MFPS">
<wire x1="-1.016" y1="-2.54" x2="-1.016" y2="2.54" width="0.254" layer="94"/>
<wire x1="-1.016" y1="2.54" x2="-2.54" y2="2.54" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="0.5334" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="0" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="0.508" y1="1.905" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-2.54" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="1.905" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="2.54" y2="2.54" width="0.1524" layer="94"/>
<wire x1="2.2352" y1="0" x2="2.286" y2="0" width="0.1524" layer="94"/>
<wire x1="2.286" y1="0" x2="2.54" y2="0" width="0.1524" layer="94"/>
<wire x1="2.286" y1="0" x2="1.016" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="1.016" y1="-0.508" x2="1.016" y2="0.508" width="0.1524" layer="94"/>
<wire x1="1.016" y1="0.508" x2="2.286" y2="0" width="0.1524" layer="94"/>
<wire x1="1.143" y1="0" x2="0.254" y2="0" width="0.1524" layer="94"/>
<wire x1="1.143" y1="0.254" x2="2.032" y2="0" width="0.3048" layer="94"/>
<wire x1="2.032" y1="0" x2="1.143" y2="-0.254" width="0.3048" layer="94"/>
<wire x1="1.143" y1="-0.254" x2="1.143" y2="0" width="0.3048" layer="94"/>
<wire x1="1.143" y1="0" x2="1.397" y2="0" width="0.3048" layer="94"/>
<wire x1="5.08" y1="1.905" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.715" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="5.715" y1="-0.635" x2="4.445" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="4.445" y1="-0.635" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="4.445" y2="0.762" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="4.191" y2="1.016" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.969" y2="0.508" width="0.1524" layer="94"/>
<circle x="2.54" y="1.905" radius="0.127" width="0.4064" layer="94"/>
<circle x="2.54" y="-1.905" radius="0.127" width="0.4064" layer="94"/>
<text x="6.35" y="1.27" size="1.778" layer="95">&gt;NAME</text>
<text x="6.35" y="-1.27" size="1.778" layer="96">&gt;VALUE</text>
<text x="1.524" y="-3.302" size="0.8128" layer="93">D</text>
<text x="1.524" y="2.54" size="0.8128" layer="93">S</text>
<text x="-2.286" y="1.27" size="0.8128" layer="93">G</text>
<rectangle x1="-0.254" y1="1.27" x2="0.508" y2="2.54" layer="94"/>
<rectangle x1="-0.254" y1="-2.54" x2="0.508" y2="-1.27" layer="94"/>
<rectangle x1="-0.254" y1="-0.889" x2="0.508" y2="0.889" layer="94"/>
<pin name="G" x="-2.54" y="2.54" visible="off" length="point" direction="pas"/>
<pin name="D" x="2.54" y="-5.08" visible="off" length="short" direction="pas" rot="R90"/>
<pin name="S" x="2.54" y="5.08" visible="off" length="short" direction="pas" rot="R270"/>
</symbol>
<symbol name="MFNS">
<wire x1="-1.1176" y1="2.413" x2="-1.1176" y2="-2.54" width="0.254" layer="94"/>
<wire x1="-1.1176" y1="-2.54" x2="-2.54" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="0.5334" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="0" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="0.508" y1="-1.905" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="2.54" x2="2.54" y2="1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="1.905" x2="5.08" y2="1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="1.905" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.08" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="5.08" y1="-1.905" x2="2.54" y2="-1.905" width="0.1524" layer="94"/>
<wire x1="2.54" y1="-1.905" x2="2.54" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="4.445" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="4.445" y1="-0.635" x2="5.715" y2="-0.635" width="0.1524" layer="94"/>
<wire x1="5.715" y1="-0.635" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="5.08" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.08" y1="0.762" x2="5.715" y2="0.762" width="0.1524" layer="94"/>
<wire x1="5.715" y1="0.762" x2="5.969" y2="1.016" width="0.1524" layer="94"/>
<wire x1="4.445" y1="0.762" x2="4.191" y2="0.508" width="0.1524" layer="94"/>
<wire x1="0.508" y1="0" x2="1.778" y2="-0.508" width="0.1524" layer="94"/>
<wire x1="1.778" y1="-0.508" x2="1.778" y2="0.508" width="0.1524" layer="94"/>
<wire x1="1.778" y1="0.508" x2="0.508" y2="0" width="0.1524" layer="94"/>
<wire x1="1.651" y1="0" x2="2.54" y2="0" width="0.1524" layer="94"/>
<wire x1="1.651" y1="0.254" x2="0.762" y2="0" width="0.3048" layer="94"/>
<wire x1="0.762" y1="0" x2="1.651" y2="-0.254" width="0.3048" layer="94"/>
<wire x1="1.651" y1="-0.254" x2="1.651" y2="0" width="0.3048" layer="94"/>
<wire x1="1.651" y1="0" x2="1.397" y2="0" width="0.3048" layer="94"/>
<circle x="2.54" y="-1.905" radius="0.127" width="0.4064" layer="94"/>
<circle x="2.54" y="1.905" radius="0.127" width="0.4064" layer="94"/>
<text x="6.35" y="1.27" size="1.778" layer="95">&gt;NAME</text>
<text x="6.35" y="-1.27" size="1.778" layer="96">&gt;VALUE</text>
<text x="1.27" y="2.54" size="0.8128" layer="93">D</text>
<text x="1.27" y="-3.175" size="0.8128" layer="93">S</text>
<text x="-2.54" y="-1.27" size="0.8128" layer="93">G</text>
<rectangle x1="-0.254" y1="-2.54" x2="0.508" y2="-1.27" layer="94"/>
<rectangle x1="-0.254" y1="1.27" x2="0.508" y2="2.54" layer="94"/>
<rectangle x1="-0.254" y1="-0.889" x2="0.508" y2="0.889" layer="94"/>
<pin name="G" x="-2.54" y="-2.54" visible="off" length="point" direction="pas"/>
<pin name="D" x="2.54" y="5.08" visible="off" length="short" direction="pas" rot="R270"/>
<pin name="S" x="2.54" y="-5.08" visible="off" length="short" direction="pas" rot="R90"/>
</symbol>
<symbol name="NPN">
<wire x1="0" y1="2.54" x2="-2.032" y2="1.524" width="0.1524" layer="94"/>
<wire x1="-0.762" y1="-1.524" x2="0" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="0" y1="-2.54" x2="-1.27" y2="-2.54" width="0.1524" layer="94"/>
<wire x1="-1.27" y1="-2.54" x2="-0.762" y2="-1.524" width="0.1524" layer="94"/>
<wire x1="-1" y1="-2.04" x2="-2.232" y2="-1.424" width="0.1524" layer="94"/>
<wire x1="-1.016" y1="-2.413" x2="-0.254" y2="-2.413" width="0.254" layer="94"/>
<wire x1="-0.254" y1="-2.413" x2="-0.762" y2="-1.778" width="0.254" layer="94"/>
<wire x1="-0.762" y1="-1.778" x2="-1.016" y2="-2.286" width="0.254" layer="94"/>
<wire x1="-1.016" y1="-2.286" x2="-0.635" y2="-2.286" width="0.254" layer="94"/>
<wire x1="-0.635" y1="-2.286" x2="-0.762" y2="-2.032" width="0.254" layer="94"/>
<text x="0.54" y="3" size="1.778" layer="95">&gt;NAME</text>
<text x="0.54" y="0.46" size="1.778" layer="96">&gt;VALUE</text>
<text x="0.54" y="-2.08" size="1.778" layer="97">&gt;SPICEMODEL</text>
<text x="0.54" y="-4.62" size="1.778" layer="97">&gt;SPICEEXTRA</text>
<rectangle x1="-2.794" y1="-2.54" x2="-2.032" y2="2.54" layer="94"/>
<pin name="B" x="-5.08" y="0" visible="off" length="short" direction="pas" swaplevel="1"/>
<pin name="E" x="0" y="-5.08" visible="off" length="short" direction="pas" swaplevel="3" rot="R90"/>
<pin name="C" x="0" y="5.08" visible="off" length="short" direction="pas" swaplevel="2" rot="R270"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PMOSFET" prefix="Q">
<description>&lt;b&gt;P-Channel MOSFET - Generic&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MFPS" x="-2.54" y="0"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:28738/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="P-Channel" constant="no"/>
<attribute name="VALUE" value="PMOSFET" constant="no"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOSFET" prefix="Q">
<description>&lt;b&gt; N-Channel MOSFET - Generic</description>
<gates>
<gate name="G$1" symbol="MFNS" x="-2.54" y="0"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:28738/2"/>
</package3dinstances>
<technologies>
<technology name="">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
<device name="TO92" package="TO92">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378726/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
<device name="TO220" package="TO220BV">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:29484/4"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="DRAIN_CURRENT" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="MOSFET" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="N-Channel" constant="no"/>
<attribute name="VALUE" value="NMOSFET" constant="no"/>
</technology>
</technologies>
</device>
<device name="" package="DPACK_3">
<connects>
<connect gate="G$1" pin="D" pad="C"/>
<connect gate="G$1" pin="G" pad="A1"/>
<connect gate="G$1" pin="S" pad="A2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:8087963/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NPN" prefix="Q">
<description>&lt;B&gt;NPN - Generic</description>
<gates>
<gate name="G$1" symbol="NPN" x="0" y="0"/>
</gates>
<devices>
<device name="TO92" package="TO92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378726/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="IC_MAX" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="BJT" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="NPN" constant="no"/>
<attribute name="VALUE" value="NPN" constant="no"/>
<attribute name="VCEO_MAX" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="SOT23" package="SOT95P237X112-3N">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378725/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="IC_MAX" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="BJT" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="NPN" constant="no"/>
<attribute name="VALUE" value="NPN" constant="no"/>
<attribute name="VCEO_MAX" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="SC-59" package="SC59">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:29756/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="IC_MAX" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="BJT" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="NPN" constant="no"/>
<attribute name="VALUE" value="NPN" constant="no"/>
<attribute name="VCEO_MAX" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="SC-70" package="SC70">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:29755/2"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="IC_MAX" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="BJT" constant="no"/>
<attribute name="THERMALLOSS" value="NPN" constant="no"/>
<attribute name="TYPE" value="" constant="no"/>
<attribute name="VALUE" value="NPN" constant="no"/>
<attribute name="VCEO_MAX" value="" constant="no"/>
</technology>
</technologies>
</device>
<device name="TO-18" package="TO18">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:16378727/1"/>
</package3dinstances>
<technologies>
<technology name="_">
<attribute name="CATEGORY" value="Transistor" constant="no"/>
<attribute name="DESCRIPTION" value="" constant="no"/>
<attribute name="IC_MAX" value="" constant="no"/>
<attribute name="MANUFACTURER" value="" constant="no"/>
<attribute name="MPN" value="" constant="no"/>
<attribute name="OPERATING_TEMP" value="" constant="no"/>
<attribute name="PART_STATUS" value="" constant="no"/>
<attribute name="ROHS_COMPLIANT" value="" constant="no"/>
<attribute name="SERIES" value="" constant="no"/>
<attribute name="SUB-CATEGORY" value="BJT" constant="no"/>
<attribute name="THERMALLOSS" value="" constant="no"/>
<attribute name="TYPE" value="NPN" constant="no"/>
<attribute name="VALUE" value="NPN" constant="no"/>
<attribute name="VCEO_MAX" value="" constant="no"/>
</technology>
</technologies>
</device>
</devices>
<spice>
<pinmapping spiceprefix="Q">
<pinmap gate="G$1" pin="B" pinorder="2"/>
<pinmap gate="G$1" pin="C" pinorder="1"/>
<pinmap gate="G$1" pin="E" pinorder="3"/>
</pinmapping>
<model name="QNPN">
**********************
* Autodesk EAGLE - Spice Model File
* Date: 9/17/17
* basic npn intrinsic model
**********************
.MODEL QNPN NPN</model>
</spice>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<classes>
<class number="0" name="default" width="0" drill="0">
</class>
</classes>
<parts>
<part name="C1" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C" device="CHIP-1206(3216-METRIC)" package3d_urn="urn:adsk.eagle:package:16290893/2" technology="_" value="0.1uF"/>
<part name="D1" library="Diodes" library_urn="urn:adsk.eagle:library:11396254" deviceset="MBR360G" device="" package3d_urn="urn:adsk.eagle:package:10898389/2" value="SB5100"/>
<part name="L1" library="inductors" library_urn="urn:adsk.eagle:library:243" deviceset="DR127" device="" package3d_urn="urn:adsk.eagle:package:15117/1"/>
<part name="C2" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C" device="CHIP-1206(3216-METRIC)" package3d_urn="urn:adsk.eagle:package:16290893/2" technology="_" value="0.1uF"/>
<part name="C3" library="Capacitor" library_urn="urn:adsk.eagle:library:16290819" deviceset="C-POL" device="TANTALUM-2917(7343-METRIC)" package3d_urn="urn:adsk.eagle:package:16290885/1" technology="_" value="15uF"/>
<part name="R1" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="1M"/>
<part name="R2" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="100K"/>
<part name="R3" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="39K"/>
<part name="J3" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="2.54MM_SCREWTERM" package3d_urn="urn:adsk.eagle:package:38059/1" value="ON/OFF"/>
<part name="J2" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="" package3d_urn="urn:adsk.eagle:package:38039/1" value="STOP_LIGHT"/>
<part name="J5" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_04" device="" package3d_urn="urn:adsk.eagle:package:38085/1" value="DRIVER"/>
<part name="GND2" library="supply1" library_urn="urn:adsk.eagle:library:371" deviceset="GND" device=""/>
<part name="D2" library="eScooter" deviceset="TVS_DIODE" device="SMA" package3d_urn="urn:adsk.eagle:package:21928182/1" value="P4SMAJ12CA"/>
<part name="C4" library="eScooter" deviceset="C" device="PANASONIC_H13" package3d_urn="urn:adsk.eagle:package:21812541/1" value="68uF"/>
<part name="U1" library="eScooter" deviceset="MAX5035" device="PDIP8" package3d_urn="urn:adsk.eagle:package:22059831/1"/>
<part name="J4" library="eScooter" deviceset="XT60" device="" value="BATTERY"/>
<part name="J6" library="eScooter" deviceset="XT60" device="" value="DRIVER POWER"/>
<part name="R9" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="47K"/>
<part name="R10" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="47K"/>
<part name="R11" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="J1" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_02" device="PTH3" package3d_urn="urn:adsk.eagle:package:38048/1"/>
<part name="J7" library="SparkFun-Connectors" library_urn="urn:adsk.eagle:library:513" deviceset="CONN_06" device="LONGPADS" package3d_urn="urn:adsk.eagle:package:37991/1"/>
<part name="R4" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="133K"/>
<part name="R5" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="1M"/>
<part name="Q1" library="Transistor" deviceset="PMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" technology="_" value="PMOSFET"/>
<part name="Q3" library="Transistor" deviceset="PMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" technology="_" value="PMOSFET"/>
<part name="Q7" library="Transistor" deviceset="NMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" value="NMOSFET"/>
<part name="Q2" library="Transistor" deviceset="NPN" device="SOT23" package3d_urn="urn:adsk.eagle:package:16378725/1" technology="_" value="NPN"/>
<part name="R6" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="R7" library="eagle-ltspice" library_urn="urn:adsk.eagle:library:217" deviceset="R" device="R1206" package3d_urn="urn:adsk.eagle:package:13301/1" value="10K"/>
<part name="Q4" library="Transistor" deviceset="PMOSFET" device="SOT23" package3d_urn="urn:adsk.eagle:package:28738/2" technology="_" value="PMOSFET"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<instances>
<instance part="C1" gate="G$1" x="129.54" y="124.46" smashed="yes" rot="R90">
<attribute name="NAME" x="129.54" y="124.46" size="1.778" layer="95" rot="R90"/>
<attribute name="VALUE" x="134.62" y="124.46" size="1.778" layer="96" rot="R90"/>
</instance>
<instance part="D1" gate="G$1" x="149.86" y="132.08" smashed="yes" rot="R180">
<attribute name="NAME" x="152.146" y="130.175" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="152.146" y="135.509" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="L1" gate="G$1" x="119.38" y="132.08" smashed="yes" rot="R180">
<attribute name="NAME" x="123.19" y="129.794" size="1.778" layer="95" rot="R180"/>
<attribute name="VALUE" x="123.317" y="135.128" size="1.778" layer="96" rot="R180"/>
</instance>
<instance part="C2" gate="G$1" x="106.68" y="104.14" smashed="yes" rot="R90">
<attribute name="NAME" x="106.68" y="104.14" size="1.778" layer="95" rot="R90"/>
<attribute name="VALUE" x="111.76" y="104.14" size="1.778" layer="96" rot="R90"/>
</instance>
<instance part="C3" gate="G$1" x="83.82" y="119.38" smashed="yes">
<attribute name="NAME" x="84.963" y="119.8626" size="1.778" layer="95"/>
<attribute name="VALUE" x="84.963" y="114.7826" size="1.778" layer="96"/>
</instance>
<instance part="R1" gate="G$1" x="182.88" y="101.6" smashed="yes" rot="R270">
<attribute name="NAME" x="179.2986" y="100.33" size="1.778" layer="95" rot="MR90"/>
<attribute name="VALUE" x="184.658" y="100.33" size="1.778" layer="96" rot="MR90"/>
</instance>
<instance part="R2" gate="G$1" x="182.88" y="86.36" smashed="yes" rot="R270">
<attribute name="NAME" x="179.2986" y="85.09" size="1.778" layer="95" rot="MR90"/>
<attribute name="VALUE" x="184.658" y="85.09" size="1.778" layer="96" rot="MR90"/>
</instance>
<instance part="R3" gate="G$1" x="182.88" y="73.66" smashed="yes" rot="R90">
<attribute name="NAME" x="181.3814" y="72.39" size="1.778" layer="95" rot="R90"/>
<attribute name="VALUE" x="186.182" y="72.39" size="1.778" layer="96" rot="R90"/>
</instance>
<instance part="J3" gate="G$1" x="195.58" y="93.98" smashed="yes" rot="R180">
<attribute name="VALUE" x="198.12" y="98.806" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="198.12" y="88.392" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="J2" gate="G$1" x="58.42" y="68.58" smashed="yes" rot="R180">
<attribute name="VALUE" x="60.96" y="73.406" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="60.96" y="62.992" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="J5" gate="G$1" x="55.88" y="86.36" smashed="yes" rot="R180">
<attribute name="VALUE" x="60.96" y="93.726" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="60.96" y="78.232" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="GND2" gate="1" x="104.14" y="0" smashed="yes">
<attribute name="VALUE" x="101.6" y="-2.54" size="1.778" layer="96"/>
</instance>
<instance part="D2" gate="D$1" x="73.66" y="116.84" smashed="yes">
<attribute name="NAME" x="76.2" y="121.92" size="1.778" layer="95"/>
</instance>
<instance part="C4" gate="G$1" x="160.02" y="106.68" smashed="yes">
<attribute name="NAME" x="162.56" y="109.22" size="1.778" layer="95"/>
<attribute name="VALUE" x="162.56" y="104.14" size="1.778" layer="96" rot="MR180"/>
</instance>
<instance part="U1" gate="G$1" x="132.08" y="101.6" smashed="yes">
<attribute name="NAME" x="132.08" y="116.84" size="1.778" layer="95"/>
<attribute name="VALUE" x="121.92" y="83.82" size="1.778" layer="96"/>
</instance>
<instance part="J4" gate="G$1" x="215.9" y="114.3" smashed="yes">
<attribute name="NAME" x="213.36" y="121.92" size="1.778" layer="95"/>
<attribute name="VALUE" x="213.36" y="111.76" size="1.778" layer="96"/>
</instance>
<instance part="J6" gate="G$1" x="215.9" y="22.86" smashed="yes" rot="MR180">
<attribute name="NAME" x="213.36" y="15.24" size="1.778" layer="95" rot="MR180"/>
<attribute name="VALUE" x="210.82" y="25.4" size="1.778" layer="96" rot="MR180"/>
</instance>
<instance part="R9" gate="G$1" x="93.98" y="121.92" smashed="yes" rot="R270">
<attribute name="NAME" x="90.3986" y="120.65" size="1.778" layer="95" rot="MR90"/>
<attribute name="VALUE" x="95.758" y="120.65" size="1.778" layer="96" rot="MR90"/>
</instance>
<instance part="R10" gate="G$1" x="93.98" y="104.14" smashed="yes" rot="R270">
<attribute name="NAME" x="90.3986" y="102.87" size="1.778" layer="95" rot="MR90"/>
<attribute name="VALUE" x="95.758" y="102.87" size="1.778" layer="96" rot="MR90"/>
</instance>
<instance part="R11" gate="G$1" x="93.98" y="83.82" smashed="yes" rot="R270">
<attribute name="NAME" x="90.3986" y="82.55" size="1.778" layer="95" rot="MR90"/>
<attribute name="VALUE" x="95.758" y="82.55" size="1.778" layer="96" rot="MR90"/>
</instance>
<instance part="J1" gate="G$1" x="58.42" y="127" smashed="yes" rot="R180">
<attribute name="VALUE" x="60.96" y="131.826" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="60.96" y="121.412" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="J7" gate="G$1" x="55.88" y="109.22" smashed="yes" rot="R180">
<attribute name="VALUE" x="60.96" y="119.126" size="1.778" layer="96" font="vector" rot="R180"/>
<attribute name="NAME" x="60.96" y="98.552" size="1.778" layer="95" font="vector" rot="R180"/>
</instance>
<instance part="R4" gate="G$1" x="104.14" y="17.78" smashed="yes" rot="R90">
<attribute name="NAME" x="107.7214" y="19.05" size="1.778" layer="95" rot="MR270"/>
<attribute name="VALUE" x="102.362" y="19.05" size="1.778" layer="96" rot="MR270"/>
</instance>
<instance part="R5" gate="G$1" x="111.76" y="33.02" smashed="yes">
<attribute name="NAME" x="113.03" y="29.4386" size="1.778" layer="95" rot="MR0"/>
<attribute name="VALUE" x="113.03" y="34.798" size="1.778" layer="96" rot="MR0"/>
</instance>
<instance part="Q1" gate="G$1" x="-20.32" y="96.52" smashed="yes">
<attribute name="NAME" x="-13.97" y="97.79" size="1.778" layer="95"/>
<attribute name="VALUE" x="-13.97" y="95.25" size="1.778" layer="96"/>
</instance>
<instance part="Q3" gate="G$1" x="-20.32" y="73.66" smashed="yes">
<attribute name="NAME" x="-13.97" y="74.93" size="1.778" layer="95"/>
<attribute name="VALUE" x="-13.97" y="72.39" size="1.778" layer="96"/>
</instance>
<instance part="Q7" gate="G$1" x="33.02" y="55.88" smashed="yes">
<attribute name="NAME" x="39.37" y="57.15" size="1.778" layer="95"/>
<attribute name="VALUE" x="39.37" y="54.61" size="1.778" layer="96"/>
</instance>
<instance part="Q2" gate="G$1" x="-2.54" y="17.78" smashed="yes">
<attribute name="NAME" x="-2" y="20.78" size="1.778" layer="95"/>
<attribute name="VALUE" x="-2" y="18.24" size="1.778" layer="96"/>
</instance>
<instance part="R6" gate="G$1" x="-15.24" y="17.78" smashed="yes">
<attribute name="NAME" x="-13.97" y="14.1986" size="1.778" layer="95" rot="MR0"/>
<attribute name="VALUE" x="-13.97" y="19.558" size="1.778" layer="96" rot="MR0"/>
</instance>
<instance part="R7" gate="G$1" x="-15.24" y="25.4" smashed="yes">
<attribute name="NAME" x="-13.97" y="21.8186" size="1.778" layer="95" rot="MR0"/>
<attribute name="VALUE" x="-13.97" y="27.178" size="1.778" layer="96" rot="MR0"/>
</instance>
<instance part="Q4" gate="G$1" x="-20.32" y="119.38" smashed="yes">
<attribute name="NAME" x="-13.97" y="120.65" size="1.778" layer="95"/>
<attribute name="VALUE" x="-13.97" y="118.11" size="1.778" layer="96"/>
</instance>
</instances>
<busses>
</busses>
<nets>
<net name="N$1" class="0">
<segment>
<wire x1="116.84" y1="109.22" x2="114.3" y2="109.22" width="0.1524" layer="91"/>
<wire x1="114.3" y1="109.22" x2="114.3" y2="124.46" width="0.1524" layer="91"/>
<pinref part="C1" gate="G$1" pin="1"/>
<wire x1="114.3" y1="124.46" x2="127" y2="124.46" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="BST"/>
</segment>
</net>
<net name="N$2" class="0">
<segment>
<pinref part="C1" gate="G$1" pin="2"/>
<wire x1="134.62" y1="124.46" x2="137.16" y2="124.46" width="0.1524" layer="91"/>
<wire x1="137.16" y1="124.46" x2="149.86" y2="124.46" width="0.1524" layer="91"/>
<wire x1="149.86" y1="124.46" x2="149.86" y2="109.22" width="0.1524" layer="91"/>
<wire x1="149.86" y1="109.22" x2="147.32" y2="109.22" width="0.1524" layer="91"/>
<wire x1="137.16" y1="132.08" x2="137.16" y2="124.46" width="0.1524" layer="91"/>
<junction x="137.16" y="124.46"/>
<pinref part="D1" gate="G$1" pin="C"/>
<wire x1="147.32" y1="132.08" x2="137.16" y2="132.08" width="0.1524" layer="91"/>
<wire x1="137.16" y1="132.08" x2="127" y2="132.08" width="0.1524" layer="91"/>
<junction x="137.16" y="132.08"/>
<pinref part="L1" gate="G$1" pin="1"/>
<pinref part="U1" gate="G$1" pin="LX"/>
</segment>
</net>
<net name="12V" class="0">
<segment>
<pinref part="L1" gate="G$1" pin="2"/>
<wire x1="111.76" y1="132.08" x2="93.98" y2="132.08" width="0.1524" layer="91"/>
<wire x1="93.98" y1="132.08" x2="83.82" y2="132.08" width="0.1524" layer="91"/>
<wire x1="83.82" y1="132.08" x2="83.82" y2="121.92" width="0.1524" layer="91"/>
<junction x="83.82" y="132.08"/>
<pinref part="C3" gate="G$1" pin="+"/>
<label x="86.36" y="132.08" size="1.778" layer="95"/>
<wire x1="50.8" y1="127" x2="40.64" y2="127" width="0.1524" layer="91"/>
<label x="45.72" y="127" size="1.778" layer="95"/>
<wire x1="83.82" y1="132.08" x2="73.66" y2="132.08" width="0.1524" layer="91"/>
<wire x1="73.66" y1="132.08" x2="40.64" y2="132.08" width="0.1524" layer="91"/>
<wire x1="40.64" y1="132.08" x2="40.64" y2="127" width="0.1524" layer="91"/>
<pinref part="D2" gate="D$1" pin="P$1"/>
<wire x1="73.66" y1="132.08" x2="73.66" y2="124.46" width="0.1524" layer="91"/>
<junction x="73.66" y="132.08"/>
<pinref part="R9" gate="G$1" pin="1"/>
<wire x1="93.98" y1="132.08" x2="93.98" y2="127" width="0.1524" layer="91"/>
<junction x="93.98" y="132.08"/>
<pinref part="J1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$4" class="0">
<segment>
<pinref part="C2" gate="G$1" pin="2"/>
<wire x1="111.76" y1="104.14" x2="116.84" y2="104.14" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="VD"/>
</segment>
</net>
<net name="N$5" class="0">
<segment>
<wire x1="147.32" y1="93.98" x2="182.88" y2="93.98" width="0.1524" layer="91"/>
<pinref part="R1" gate="G$1" pin="2"/>
<wire x1="182.88" y1="96.52" x2="182.88" y2="93.98" width="0.1524" layer="91"/>
<wire x1="182.88" y1="93.98" x2="182.88" y2="91.44" width="0.1524" layer="91"/>
<junction x="182.88" y="93.98"/>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="J3" gate="G$1" pin="1"/>
<wire x1="182.88" y1="93.98" x2="187.96" y2="93.98" width="0.1524" layer="91"/>
<pinref part="U1" gate="G$1" pin="ON/OFF"/>
</segment>
</net>
<net name="N$7" class="0">
<segment>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="R3" gate="G$1" pin="2"/>
<wire x1="182.88" y1="81.28" x2="182.88" y2="78.74" width="0.1524" layer="91"/>
</segment>
</net>
<net name="THCTL" class="0">
<segment>
<wire x1="38.1" y1="101.6" x2="50.8" y2="101.6" width="0.1524" layer="91"/>
<pinref part="J7" gate="G$1" pin="6"/>
<label x="43.18" y="101.6" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q1" gate="G$1" pin="S"/>
<wire x1="-17.78" y1="101.6" x2="-17.78" y2="106.68" width="0.1524" layer="91"/>
<label x="-38.1" y="106.68" size="1.778" layer="95"/>
<wire x1="-17.78" y1="106.68" x2="-38.1" y2="106.68" width="0.1524" layer="91"/>
</segment>
</net>
<net name="ST_DR" class="0">
<segment>
<pinref part="J5" gate="G$1" pin="3"/>
<wire x1="50.8" y1="83.82" x2="33.02" y2="83.82" width="0.1524" layer="91"/>
<label x="43.18" y="83.82" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q3" gate="G$1" pin="D"/>
<wire x1="-17.78" y1="68.58" x2="-17.78" y2="66.04" width="0.1524" layer="91"/>
<label x="-38.1" y="66.04" size="1.778" layer="95"/>
<wire x1="-17.78" y1="66.04" x2="-38.1" y2="66.04" width="0.1524" layer="91"/>
</segment>
</net>
<net name="5V" class="0">
<segment>
<pinref part="J5" gate="G$1" pin="4"/>
<wire x1="50.8" y1="81.28" x2="45.72" y2="81.28" width="0.1524" layer="91"/>
<wire x1="45.72" y1="81.28" x2="45.72" y2="68.58" width="0.1524" layer="91"/>
<pinref part="J2" gate="G$1" pin="1"/>
<wire x1="45.72" y1="68.58" x2="50.8" y2="68.58" width="0.1524" layer="91"/>
<label x="48.26" y="81.28" size="1.778" layer="95"/>
<label x="48.26" y="68.58" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q3" gate="G$1" pin="S"/>
<label x="-38.1" y="83.82" size="1.778" layer="95"/>
<wire x1="-17.78" y1="78.74" x2="-17.78" y2="83.82" width="0.1524" layer="91"/>
<wire x1="-17.78" y1="83.82" x2="-38.1" y2="83.82" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="R7" gate="G$1" pin="1"/>
<wire x1="-20.32" y1="25.4" x2="-30.48" y2="25.4" width="0.1524" layer="91"/>
<label x="-30.48" y="25.4" size="1.778" layer="95"/>
</segment>
</net>
<net name="STLEDOUT" class="0">
<segment>
<pinref part="J2" gate="G$1" pin="2"/>
<label x="38.1" y="66.04" size="1.778" layer="95"/>
<pinref part="Q7" gate="G$1" pin="D"/>
<wire x1="35.56" y1="60.96" x2="35.56" y2="66.04" width="0.1524" layer="91"/>
<wire x1="50.8" y1="66.04" x2="35.56" y2="66.04" width="0.1524" layer="91"/>
</segment>
</net>
<net name="STLEDCTL" class="0">
<segment>
<label x="38.1" y="109.22" size="1.778" layer="95"/>
<wire x1="38.1" y1="109.22" x2="50.8" y2="109.22" width="0.1524" layer="91"/>
<pinref part="J7" gate="G$1" pin="3"/>
</segment>
<segment>
<pinref part="Q7" gate="G$1" pin="G"/>
<wire x1="30.48" y1="53.34" x2="17.78" y2="53.34" width="0.1524" layer="91"/>
<label x="17.78" y="53.34" size="1.778" layer="95"/>
</segment>
</net>
<net name="PWON" class="0">
<segment>
<pinref part="J7" gate="G$1" pin="1"/>
<wire x1="50.8" y1="114.3" x2="38.1" y2="114.3" width="0.1524" layer="91"/>
<label x="40.64" y="114.3" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q2" gate="G$1" pin="B"/>
<wire x1="-7.62" y1="17.78" x2="-10.16" y2="17.78" width="0.1524" layer="91"/>
<label x="-30.48" y="17.78" size="1.778" layer="95"/>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="BAT" class="0">
<segment>
<pinref part="J7" gate="G$1" pin="2"/>
<wire x1="50.8" y1="111.76" x2="38.1" y2="111.76" width="0.1524" layer="91"/>
<label x="40.64" y="111.76" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q4" gate="G$1" pin="D"/>
<wire x1="-17.78" y1="114.3" x2="-17.78" y2="111.76" width="0.1524" layer="91"/>
<label x="-38.1" y="111.76" size="1.778" layer="95"/>
<wire x1="-17.78" y1="111.76" x2="-38.1" y2="111.76" width="0.1524" layer="91"/>
</segment>
</net>
<net name="STCTL" class="0">
<segment>
<label x="43.18" y="106.68" size="1.778" layer="95"/>
<pinref part="J7" gate="G$1" pin="4"/>
<wire x1="50.8" y1="106.68" x2="38.1" y2="106.68" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="Q3" gate="G$1" pin="G"/>
<wire x1="-22.86" y1="76.2" x2="-38.1" y2="76.2" width="0.1524" layer="91"/>
<label x="-38.1" y="76.2" size="1.778" layer="95"/>
</segment>
</net>
<net name="N$6" class="0">
<segment>
<pinref part="R10" gate="G$1" pin="1"/>
<pinref part="R9" gate="G$1" pin="2"/>
<wire x1="93.98" y1="109.22" x2="93.98" y2="116.84" width="0.1524" layer="91"/>
</segment>
</net>
<net name="N$9" class="0">
<segment>
<pinref part="U1" gate="G$1" pin="FB"/>
<wire x1="116.84" y1="93.98" x2="93.98" y2="93.98" width="0.1524" layer="91"/>
<pinref part="R11" gate="G$1" pin="1"/>
<wire x1="93.98" y1="93.98" x2="93.98" y2="88.9" width="0.1524" layer="91"/>
<pinref part="R10" gate="G$1" pin="2"/>
<wire x1="93.98" y1="93.98" x2="93.98" y2="99.06" width="0.1524" layer="91"/>
<junction x="93.98" y="93.98"/>
</segment>
</net>
<net name="VIN" class="0">
<segment>
<wire x1="147.32" y1="104.14" x2="154.94" y2="104.14" width="0.1524" layer="91"/>
<wire x1="182.88" y1="116.84" x2="182.88" y2="106.68" width="0.1524" layer="91"/>
<pinref part="R1" gate="G$1" pin="1"/>
<wire x1="182.88" y1="116.84" x2="203.2" y2="116.84" width="0.1524" layer="91"/>
<junction x="182.88" y="116.84"/>
<wire x1="203.2" y1="116.84" x2="210.82" y2="116.84" width="0.1524" layer="91"/>
<wire x1="154.94" y1="104.14" x2="154.94" y2="116.84" width="0.1524" layer="91"/>
<wire x1="154.94" y1="116.84" x2="160.02" y2="116.84" width="0.1524" layer="91"/>
<wire x1="160.02" y1="116.84" x2="182.88" y2="116.84" width="0.1524" layer="91"/>
<wire x1="160.02" y1="113.03" x2="160.02" y2="116.84" width="0.1524" layer="91"/>
<junction x="160.02" y="116.84"/>
<label x="203.2" y="116.84" size="1.778" layer="95"/>
<pinref part="C4" gate="G$1" pin="P$1"/>
<label x="147.32" y="104.14" size="1.778" layer="95"/>
<pinref part="U1" gate="G$1" pin="VIN"/>
<pinref part="J4" gate="G$1" pin="P$2"/>
<pinref part="J6" gate="G$1" pin="P$2"/>
<wire x1="210.82" y1="20.32" x2="203.2" y2="20.32" width="0.1524" layer="91"/>
<wire x1="203.2" y1="33.02" x2="203.2" y2="40.64" width="0.1524" layer="91"/>
<wire x1="203.2" y1="40.64" x2="203.2" y2="43.18" width="0.1524" layer="91"/>
<wire x1="116.84" y1="33.02" x2="203.2" y2="33.02" width="0.1524" layer="91"/>
<wire x1="203.2" y1="20.32" x2="203.2" y2="33.02" width="0.1524" layer="91"/>
<junction x="203.2" y="33.02"/>
<pinref part="R5" gate="G$1" pin="2"/>
<wire x1="203.2" y1="116.84" x2="203.2" y2="43.18" width="0.1524" layer="91"/>
<junction x="203.2" y="116.84"/>
</segment>
</net>
<net name="GND" class="0">
<segment>
<pinref part="J6" gate="G$1" pin="P$1"/>
<wire x1="210.82" y1="17.78" x2="203.2" y2="17.78" width="0.1524" layer="91"/>
<pinref part="GND2" gate="1" pin="GND"/>
<wire x1="104.14" y1="12.7" x2="104.14" y2="7.62" width="0.1524" layer="91"/>
<wire x1="104.14" y1="7.62" x2="104.14" y2="2.54" width="0.1524" layer="91"/>
<junction x="104.14" y="7.62"/>
<pinref part="R3" gate="G$1" pin="1"/>
<wire x1="35.56" y1="7.62" x2="104.14" y2="7.62" width="0.1524" layer="91"/>
<wire x1="182.88" y1="68.58" x2="182.88" y2="66.04" width="0.1524" layer="91"/>
<wire x1="182.88" y1="66.04" x2="160.02" y2="66.04" width="0.1524" layer="91"/>
<junction x="182.88" y="66.04"/>
<pinref part="C3" gate="G$1" pin="-"/>
<wire x1="187.96" y1="66.04" x2="182.88" y2="66.04" width="0.1524" layer="91"/>
<wire x1="160.02" y1="66.04" x2="101.6" y2="66.04" width="0.1524" layer="91"/>
<wire x1="101.6" y1="66.04" x2="93.98" y2="66.04" width="0.1524" layer="91"/>
<wire x1="93.98" y1="66.04" x2="83.82" y2="66.04" width="0.1524" layer="91"/>
<wire x1="83.82" y1="66.04" x2="83.82" y2="114.3" width="0.1524" layer="91"/>
<pinref part="D1" gate="G$1" pin="A"/>
<wire x1="152.4" y1="132.08" x2="200.66" y2="132.08" width="0.1524" layer="91"/>
<wire x1="200.66" y1="132.08" x2="223.52" y2="132.08" width="0.1524" layer="91"/>
<pinref part="J3" gate="G$1" pin="2"/>
<wire x1="187.96" y1="91.44" x2="187.96" y2="66.04" width="0.1524" layer="91"/>
<wire x1="160.02" y1="99.06" x2="160.02" y2="101.6" width="0.1524" layer="91"/>
<wire x1="147.32" y1="99.06" x2="160.02" y2="99.06" width="0.1524" layer="91"/>
<junction x="160.02" y="99.06"/>
<label x="147.32" y="99.06" size="1.778" layer="95"/>
<wire x1="160.02" y1="99.06" x2="160.02" y2="66.04" width="0.1524" layer="91"/>
<junction x="160.02" y="66.04"/>
<label x="203.2" y="119.38" size="1.778" layer="95"/>
<pinref part="D2" gate="D$1" pin="P$2"/>
<wire x1="73.66" y1="109.22" x2="73.66" y2="66.04" width="0.1524" layer="91"/>
<wire x1="73.66" y1="66.04" x2="83.82" y2="66.04" width="0.1524" layer="91"/>
<junction x="83.82" y="66.04"/>
<wire x1="104.14" y1="7.62" x2="73.66" y2="7.62" width="0.1524" layer="91"/>
<wire x1="200.66" y1="119.38" x2="200.66" y2="132.08" width="0.1524" layer="91"/>
<junction x="200.66" y="132.08"/>
<wire x1="223.52" y1="132.08" x2="223.52" y2="7.62" width="0.1524" layer="91"/>
<wire x1="223.52" y1="7.62" x2="203.2" y2="7.62" width="0.1524" layer="91"/>
<wire x1="203.2" y1="7.62" x2="73.66" y2="7.62" width="0.1524" layer="91"/>
<wire x1="116.84" y1="99.06" x2="101.6" y2="99.06" width="0.1524" layer="91"/>
<wire x1="101.6" y1="99.06" x2="101.6" y2="104.14" width="0.1524" layer="91"/>
<wire x1="101.6" y1="104.14" x2="104.14" y2="104.14" width="0.1524" layer="91"/>
<pinref part="C2" gate="G$1" pin="1"/>
<wire x1="101.6" y1="99.06" x2="101.6" y2="66.04" width="0.1524" layer="91"/>
<junction x="101.6" y="99.06"/>
<junction x="101.6" y="66.04"/>
<label x="111.76" y="99.06" size="1.778" layer="95"/>
<wire x1="73.66" y1="66.04" x2="73.66" y2="7.62" width="0.1524" layer="91"/>
<junction x="73.66" y="66.04"/>
<junction x="73.66" y="7.62"/>
<pinref part="C4" gate="G$1" pin="P$2"/>
<pinref part="U1" gate="G$1" pin="SGND"/>
<pinref part="U1" gate="G$1" pin="GND"/>
<pinref part="J4" gate="G$1" pin="P$1"/>
<wire x1="200.66" y1="119.38" x2="210.82" y2="119.38" width="0.1524" layer="91"/>
<pinref part="R11" gate="G$1" pin="2"/>
<wire x1="93.98" y1="78.74" x2="93.98" y2="66.04" width="0.1524" layer="91"/>
<junction x="93.98" y="66.04"/>
<junction x="203.2" y="7.62"/>
<wire x1="203.2" y1="17.78" x2="203.2" y2="7.62" width="0.1524" layer="91"/>
<pinref part="R4" gate="G$1" pin="1"/>
<pinref part="Q7" gate="G$1" pin="S"/>
<wire x1="35.56" y1="50.8" x2="35.56" y2="7.62" width="0.1524" layer="91"/>
<label x="35.56" y="48.26" size="1.778" layer="95"/>
<wire x1="-2.54" y1="7.62" x2="35.56" y2="7.62" width="0.1524" layer="91"/>
<junction x="35.56" y="7.62"/>
<pinref part="Q2" gate="G$1" pin="E"/>
<wire x1="-2.54" y1="12.7" x2="-2.54" y2="7.62" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="J1" gate="G$1" pin="2"/>
<wire x1="50.8" y1="124.46" x2="40.64" y2="124.46" width="0.1524" layer="91"/>
<label x="45.72" y="124.46" size="1.778" layer="95"/>
</segment>
</net>
<net name="BATOUT" class="0">
<segment>
<wire x1="104.14" y1="27.94" x2="88.9" y2="27.94" width="0.1524" layer="91"/>
<label x="88.9" y="27.94" size="1.778" layer="95"/>
<wire x1="106.68" y1="33.02" x2="104.14" y2="33.02" width="0.1524" layer="91"/>
<wire x1="104.14" y1="33.02" x2="104.14" y2="27.94" width="0.1524" layer="91"/>
<wire x1="104.14" y1="27.94" x2="104.14" y2="22.86" width="0.1524" layer="91"/>
<junction x="104.14" y="27.94"/>
<pinref part="R4" gate="G$1" pin="2"/>
<pinref part="R5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="Q4" gate="G$1" pin="S"/>
<wire x1="-17.78" y1="124.46" x2="-17.78" y2="129.54" width="0.1524" layer="91"/>
<label x="-38.1" y="129.54" size="1.778" layer="95"/>
<wire x1="-17.78" y1="129.54" x2="-38.1" y2="129.54" width="0.1524" layer="91"/>
</segment>
</net>
<net name="SPEED_DR" class="0">
<segment>
<pinref part="J5" gate="G$1" pin="2"/>
<wire x1="50.8" y1="86.36" x2="33.02" y2="86.36" width="0.1524" layer="91"/>
<label x="38.1" y="86.36" size="1.778" layer="95"/>
</segment>
<segment>
<wire x1="38.1" y1="104.14" x2="50.8" y2="104.14" width="0.1524" layer="91"/>
<pinref part="J7" gate="G$1" pin="5"/>
<label x="38.1" y="104.14" size="1.778" layer="95"/>
</segment>
</net>
<net name="TH_DR" class="0">
<segment>
<pinref part="J5" gate="G$1" pin="1"/>
<wire x1="50.8" y1="88.9" x2="33.02" y2="88.9" width="0.1524" layer="91"/>
<label x="43.18" y="88.9" size="1.778" layer="95"/>
</segment>
<segment>
<pinref part="Q1" gate="G$1" pin="D"/>
<wire x1="-17.78" y1="91.44" x2="-17.78" y2="88.9" width="0.1524" layer="91"/>
<label x="-38.1" y="88.9" size="1.778" layer="95"/>
<wire x1="-17.78" y1="88.9" x2="-38.1" y2="88.9" width="0.1524" layer="91"/>
</segment>
</net>
<net name="PWON_REV" class="0">
<segment>
<pinref part="Q1" gate="G$1" pin="G"/>
<label x="-38.1" y="99.06" size="1.778" layer="95"/>
<wire x1="-22.86" y1="99.06" x2="-38.1" y2="99.06" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="Q2" gate="G$1" pin="C"/>
<wire x1="-2.54" y1="22.86" x2="-2.54" y2="25.4" width="0.1524" layer="91"/>
<label x="-30.48" y="33.02" size="1.778" layer="95"/>
<pinref part="R7" gate="G$1" pin="2"/>
<wire x1="-10.16" y1="25.4" x2="-2.54" y2="25.4" width="0.1524" layer="91"/>
<wire x1="-2.54" y1="25.4" x2="-2.54" y2="33.02" width="0.1524" layer="91"/>
<junction x="-2.54" y="25.4"/>
<wire x1="-2.54" y1="33.02" x2="-30.48" y2="33.02" width="0.1524" layer="91"/>
</segment>
<segment>
<pinref part="Q4" gate="G$1" pin="G"/>
<wire x1="-22.86" y1="121.92" x2="-38.1" y2="121.92" width="0.1524" layer="91"/>
<label x="-38.1" y="121.92" size="1.778" layer="95"/>
</segment>
</net>
<net name="N$3" class="0">
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
<wire x1="-20.32" y1="17.78" x2="-30.48" y2="17.78" width="0.1524" layer="91"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
<compatibility>
<note version="8.2" severity="warning">
Since Version 8.2, EAGLE supports online libraries. The ids
of those online libraries will not be understood (or retained)
with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
<note version="8.4" severity="warning">
Since Version 8.4, EAGLE supports properties for SPICE simulation. 
Probes in schematics and SPICE mapping objects found in parts and library devices
will not be understood with this version. Update EAGLE to the latest version
for full support of SPICE simulation. 
</note>
</compatibility>
</eagle>
