<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="DIP8">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; Gull Wing Surface Mount Optioon 300&lt;p&gt;
Source: http://www.avagotech.com/docs/AV02-0410EN</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
<package name="CAPAE1230X1250N">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
</package>
<package name="SON254P1750X4300X120-30M">
<description>30-SON (DFN), 2.54 mm pitch, 43.00 X 17.50 X 1.20 mm body
&lt;p&gt;30-pin SON (DFN) package with 2.54 mm pitch with body size 43.00 X 17.50 X 1.20 mm&lt;/p&gt;</description>
</package>
<package name="RND430">
</package>
<package name="DIOM5027X220N">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="MX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<pin name="BST" direction="in"/>
<pin name="VD" direction="in"/>
<pin name="SGND" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="ON/OFF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="LX" direction="pwr"/>
</symbol>
<symbol name="C">
<pin name="P$1" direction="pwr"/>
<pin name="P$2" direction="pwr"/>
</symbol>
<symbol name="ARDUINO">
<pin name="D13"/>
<pin name="3V3" direction="pwr"/>
<pin name="REF"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="5V" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="TX1" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="RST2" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
</symbol>
<symbol name="BUZZER">
<pin name="5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TVS_DIODE">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<gates>
<gate name="G$1" symbol="MX5035"/>
</gates>
<devices>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="BST" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="ON/OFF" pad="5"/>
<connect gate="G$1" pin="SGND" pad="3"/>
<connect gate="G$1" pin="VD" pad="2"/>
<connect gate="G$1" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C">
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="PANASONIC_H13" package="CAPAE1230X1250N">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO">
<description>Ardino nano</description>
<gates>
<gate name="G$1" symbol="ARDUINO"/>
</gates>
<devices>
<device name="ARDUINO_NANO" package="SON254P1750X4300X120-30M">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="5V" pad="12"/>
<connect gate="G$1" pin="A0" pad="4"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="9"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="11"/>
<connect gate="G$1" pin="D10" pad="28"/>
<connect gate="G$1" pin="D11" pad="29"/>
<connect gate="G$1" pin="D12" pad="30"/>
<connect gate="G$1" pin="D13" pad="1"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="D8" pad="26"/>
<connect gate="G$1" pin="D9" pad="27"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="GND2" pad="19"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="RST" pad="13"/>
<connect gate="G$1" pin="RST2" pad="18"/>
<connect gate="G$1" pin="RX0" pad="17"/>
<connect gate="G$1" pin="TX1" pad="16"/>
<connect gate="G$1" pin="VIN" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUZZER">
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="" package="RND430">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVS_DIODE">
<description>TVS protective diode</description>
<gates>
<gate name="D$1" symbol="TVS_DIODE"/>
</gates>
<devices>
<device name="SMA" package="DIOM5027X220N">
<connects>
<connect gate="D$1" pin="P$1" pad="1"/>
<connect gate="D$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
