<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="yes" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="24" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="88" name="SimResults" color="9" fill="1" visible="yes" active="yes"/>
<layer number="89" name="SimProbes" color="9" fill="1" visible="yes" active="yes"/>
<layer number="90" name="Modules" color="5" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
</layers>
<library>
<packages>
<package name="DIP8" urn="urn:adsk.eagle:footprint:4470/1">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; Gull Wing Surface Mount Optioon 300&lt;p&gt;
Source: http://www.avagotech.com/docs/AV02-0410EN</description>
<wire x1="-4.81" y1="-3.075" x2="4.81" y2="-3.075" width="0.2032" layer="51"/>
<wire x1="4.81" y1="-3.075" x2="4.81" y2="3.075" width="0.2032" layer="21"/>
<wire x1="4.81" y1="3.075" x2="-4.81" y2="3.075" width="0.2032" layer="51"/>
<wire x1="-4.81" y1="3.075" x2="-4.81" y2="-3.075" width="0.2032" layer="21"/>
<circle x="-3.81" y="-2.159" radius="0.3667" width="0" layer="21"/>
<smd name="1" x="-3.81" y="-4.45" dx="1.16" dy="2" layer="1"/>
<smd name="2" x="-1.27" y="-4.45" dx="1.27" dy="2" layer="1"/>
<smd name="3" x="1.27" y="-4.45" dx="1.27" dy="2" layer="1"/>
<smd name="4" x="3.81" y="-4.45" dx="1.16" dy="2" layer="1"/>
<smd name="5" x="3.81" y="4.45" dx="1.16" dy="2" layer="1"/>
<smd name="6" x="1.27" y="4.45" dx="1.27" dy="2" layer="1"/>
<smd name="7" x="-1.27" y="4.45" dx="1.27" dy="2" layer="1"/>
<smd name="8" x="-3.81" y="4.45" dx="1.16" dy="2" layer="1"/>
<text x="-5.635" y="-3.1351" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.905" y="-4.4051" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-4.0899" y1="-4.825" x2="-3.5301" y2="-3.81" layer="51"/>
<rectangle x1="-1.5499" y1="-4.825" x2="-0.9901" y2="-3.81" layer="51"/>
<rectangle x1="0.9901" y1="-4.825" x2="1.5499" y2="-3.81" layer="51"/>
<rectangle x1="3.5301" y1="-4.825" x2="4.0899" y2="-3.81" layer="51"/>
<rectangle x1="3.5301" y1="3.81" x2="4.0899" y2="4.825" layer="51"/>
<rectangle x1="0.9901" y1="3.81" x2="1.5499" y2="4.825" layer="51"/>
<rectangle x1="-1.5499" y1="3.81" x2="-0.9901" y2="4.825" layer="51"/>
<rectangle x1="-4.0899" y1="3.81" x2="-3.5301" y2="4.825" layer="51"/>
<rectangle x1="-2.15" y1="3.1" x2="-0.4" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="-4.1" y1="3.1" x2="-2.94" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="0.39" y1="3.1" x2="2.14" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="2.93" y1="3.1" x2="4.1" y2="3.81" layer="51" rot="R180"/>
<rectangle x1="-4.075" y1="-3.81" x2="-2.93" y2="-3.1" layer="51"/>
<rectangle x1="-2.14" y1="-3.81" x2="-0.39" y2="-3.1" layer="51"/>
<rectangle x1="0.4" y1="-3.81" x2="2.15" y2="-3.1" layer="51"/>
<rectangle x1="2.94" y1="-3.81" x2="4.1" y2="-3.1" layer="51"/>
</package>
<package name="PANASONIC_C" urn="urn:adsk.eagle:footprint:22926/1">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
<wire x1="-2.6" y1="2.6" x2="1.25" y2="2.6" width="0.1016" layer="51"/>
<wire x1="1.25" y1="2.6" x2="2.6" y2="1.25" width="0.1016" layer="51"/>
<wire x1="2.6" y1="1.25" x2="2.6" y2="-1.25" width="0.1016" layer="51"/>
<wire x1="2.6" y1="-1.25" x2="1.25" y2="-2.6" width="0.1016" layer="51"/>
<wire x1="1.25" y1="-2.6" x2="-2.6" y2="-2.6" width="0.1016" layer="51"/>
<wire x1="-2.6" y1="-2.6" x2="-2.6" y2="2.6" width="0.1016" layer="51"/>
<wire x1="-2.6" y1="0.95" x2="-2.6" y2="2.6" width="0.1016" layer="21"/>
<wire x1="-2.6" y1="2.6" x2="1.25" y2="2.6" width="0.1016" layer="21"/>
<wire x1="1.25" y1="2.6" x2="2.6" y2="1.25" width="0.1016" layer="21"/>
<wire x1="2.6" y1="1.25" x2="2.6" y2="0.95" width="0.1016" layer="21"/>
<wire x1="2.6" y1="-0.95" x2="2.6" y2="-1.25" width="0.1016" layer="21"/>
<wire x1="2.6" y1="-1.25" x2="1.25" y2="-2.6" width="0.1016" layer="21"/>
<wire x1="1.25" y1="-2.6" x2="-2.6" y2="-2.6" width="0.1016" layer="21"/>
<wire x1="-2.6" y1="-2.6" x2="-2.6" y2="-0.95" width="0.1016" layer="21"/>
<wire x1="-2.3" y1="0.85" x2="2.3" y2="0.85" width="0.1016" layer="21" curve="-139.434882"/>
<wire x1="-2.3" y1="-0.85" x2="2.3" y2="-0.85" width="0.1016" layer="21" curve="139.434882"/>
<wire x1="-1.55" y1="1.85" x2="-1.55" y2="-1.85" width="0.1016" layer="51"/>
<circle x="0" y="0" radius="2.45" width="0.1016" layer="51"/>
<smd name="-" x="-2.05" y="0" dx="2.6" dy="1.4" layer="1"/>
<smd name="+" x="2.05" y="0" dx="2.6" dy="1.4" layer="1"/>
<text x="-2.6" y="2.75" size="1.016" layer="25">&gt;NAME</text>
<text x="-2.65" y="-3.775" size="1.016" layer="27">&gt;VALUE</text>
<rectangle x1="-2.95" y1="-0.35" x2="-2.4" y2="0.35" layer="51"/>
<rectangle x1="2.4" y1="-0.35" x2="2.95" y2="0.35" layer="51"/>
<polygon width="0.1016" layer="51">
<vertex x="-1.6" y="1.8"/>
<vertex x="-2" y="1.35"/>
<vertex x="-2.25" y="0.75"/>
<vertex x="-2.45" y="0.05"/>
<vertex x="-2.25" y="-0.75"/>
<vertex x="-1.95" y="-1.35"/>
<vertex x="-1.6" y="-1.8"/>
</polygon>
</package>
<package name="CAPAE1230X1250N" urn="urn:adsk.eagle:footprint:21812987/1">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<wire x1="-6.25" y1="1.3186" x2="-6.25" y2="3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="3.6573" x2="-3.6573" y2="6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="1.3186" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-1.3186" x2="-6.25" y2="-3.6573" width="0.12" layer="21"/>
<wire x1="-6.25" y1="-3.6573" x2="-3.6573" y2="-6.25" width="0.12" layer="21"/>
<wire x1="-3.6573" y1="-6.25" x2="6.25" y2="-6.25" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="6.25" y2="-1.3186" width="0.12" layer="21"/>
<wire x1="6.25" y1="-6.25" x2="-6.25" y2="-6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="-6.25" x2="-6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="-6.25" y1="6.25" x2="6.25" y2="6.25" width="0.12" layer="51"/>
<wire x1="6.25" y1="6.25" x2="6.25" y2="-6.25" width="0.12" layer="51"/>
<smd name="1" x="-4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<smd name="2" x="4.925" y="0" dx="5.4618" dy="2.1291" layer="1"/>
<text x="0" y="6.885" size="1.27" layer="25" align="bottom-center">&gt;NAME</text>
<text x="0" y="-6.885" size="1.27" layer="27" align="top-center">&gt;VALUE</text>
</package>
</packages>
<packages3d>
<package3d name="DIP8" urn="urn:adsk.eagle:package:8089856/1" locally_modified="yes" type="box">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; &lt;p&gt;
dual in line package'</description>
<packageinstances>
<packageinstance name="DIP8"/>
</packageinstances>
</package3d>
<package3d name="DIP8" urn="urn:adsk.eagle:package:4484/1" type="box">
<description>SMD DIL08 Gull Wing Surface Mount Optioon 300
Source: http://www.avagotech.com/docs/AV02-0410EN</description>
<packageinstances>
<packageinstance name="DIP8"/>
</packageinstances>
</package3d>
<package3d name="PANASONIC_C" urn="urn:adsk.eagle:package:23422/2" type="model">
<description>Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C</description>
<packageinstances>
<packageinstance name="PANASONIC_C"/>
</packageinstances>
</package3d>
<package3d name="CAPAE1230X1250N" urn="urn:adsk.eagle:package:21812541/1" type="model">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
<packageinstances>
<packageinstance name="CAPAE1230X1250N"/>
</packageinstances>
</package3d>
</packages3d>
<symbols>
<symbol name="MX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<wire x1="-10.16" y1="12.7" x2="10.16" y2="12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="12.7" x2="10.16" y2="-12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="-12.7" x2="-10.16" y2="-12.7" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-12.7" x2="-10.16" y2="12.7" width="0.254" layer="94"/>
<pin name="BST" x="-15.24" y="7.62" length="middle" direction="in"/>
<pin name="VD" x="-15.24" y="2.54" length="middle" direction="in"/>
<pin name="SGND" x="-15.24" y="-2.54" length="middle" direction="in"/>
<pin name="FB" x="-15.24" y="-7.62" length="middle" direction="in"/>
<pin name="ON/OFF" x="15.24" y="-7.62" length="middle" direction="in" rot="R180"/>
<pin name="GND" x="15.24" y="-2.54" length="middle" direction="pwr" rot="R180"/>
<pin name="VIN" x="15.24" y="2.54" length="middle" direction="pwr" rot="R180"/>
<pin name="LX" x="15.24" y="7.62" length="middle" direction="pwr" rot="R180"/>
<text x="-10.16" y="15.24" size="1.778" layer="95">&gt;NAME</text>
<text x="-10.16" y="-17.78" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="C">
<wire x1="-2.54" y1="1.27" x2="2.54" y2="1.27" width="0.254" layer="94"/>
<wire x1="-2.54" y1="-1.016" x2="2.54" y2="-1.016" width="0.254" layer="94" curve="-90"/>
<pin name="P$1" x="0" y="6.35" visible="off" length="middle" direction="pwr" rot="R270"/>
<pin name="P$2" x="0" y="-5.08" visible="off" length="middle" direction="pwr" rot="R90"/>
<text x="-3.81" y="1.27" size="1.778" layer="94">+</text>
<text x="2.54" y="2.54" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-5.08" size="1.778" layer="96">&gt;VALUE</text>
</symbol>
<symbol name="ARDUINO">
<wire x1="-10.16" y1="20.32" x2="-10.16" y2="-20.32" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-20.32" x2="10.16" y2="-20.32" width="0.254" layer="94"/>
<wire x1="10.16" y1="-20.32" x2="10.16" y2="20.32" width="0.254" layer="94"/>
<wire x1="10.16" y1="20.32" x2="-10.16" y2="20.32" width="0.254" layer="94"/>
<pin name="D13" x="-15.24" y="17.78" length="middle"/>
<pin name="3V3" x="-15.24" y="15.24" length="middle"/>
<pin name="REF" x="-15.24" y="12.7" length="middle"/>
<pin name="A0" x="-15.24" y="10.16" length="middle"/>
<pin name="A1" x="-15.24" y="7.62" length="middle"/>
<pin name="A2" x="-15.24" y="5.08" length="middle"/>
<pin name="A3" x="-15.24" y="2.54" length="middle"/>
<pin name="A4" x="-15.24" y="0" length="middle"/>
<pin name="A5" x="-15.24" y="-2.54" length="middle"/>
<pin name="A6" x="-15.24" y="-5.08" length="middle"/>
<pin name="A7" x="-15.24" y="-7.62" length="middle"/>
<pin name="5V" x="-15.24" y="-10.16" length="middle"/>
<pin name="RST" x="-15.24" y="-12.7" length="middle"/>
<pin name="RX0" x="-15.24" y="-15.24" length="middle"/>
<pin name="TX1" x="-15.24" y="-17.78" length="middle"/>
<pin name="P$16" x="15.24" y="-17.78" length="middle" rot="R180"/>
<pin name="P$17" x="15.24" y="-15.24" length="middle" rot="R180"/>
<pin name="P$18" x="15.24" y="-12.7" length="middle" rot="R180"/>
<pin name="P$19" x="15.24" y="-10.16" length="middle" rot="R180"/>
<pin name="P$20" x="15.24" y="-7.62" length="middle" rot="R180"/>
<pin name="P$21" x="15.24" y="-5.08" length="middle" rot="R180"/>
<pin name="P$22" x="15.24" y="-2.54" length="middle" rot="R180"/>
<pin name="P$23" x="15.24" y="0" length="middle" rot="R180"/>
<pin name="P$24" x="15.24" y="2.54" length="middle" rot="R180"/>
<pin name="P$25" x="15.24" y="5.08" length="middle" rot="R180"/>
<pin name="P$26" x="15.24" y="7.62" length="middle" rot="R180"/>
<pin name="P$27" x="15.24" y="10.16" length="middle" rot="R180"/>
<pin name="P$28" x="15.24" y="12.7" length="middle" rot="R180"/>
<pin name="P$29" x="15.24" y="15.24" length="middle" rot="R180"/>
<pin name="P$30" x="15.24" y="17.78" length="middle" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MAX5035">
<description>The  MAX5035  easy-to-use,  high-efficiency,  high-volt-age,  step-down  DC-DC  converter  operates  from  aninput voltage up to 76V and consumes only 270μA qui-escent  current  at  no  load.</description>
<gates>
<gate name="G$1" symbol="MX5035" x="0" y="0"/>
</gates>
<devices>
<device name="DIP8" package="DIP8">
<connects>
<connect gate="G$1" pin="BST" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="LX" pad="8"/>
<connect gate="G$1" pin="ON/OFF" pad="5"/>
<connect gate="G$1" pin="SGND" pad="3"/>
<connect gate="G$1" pin="VD" pad="2"/>
<connect gate="G$1" pin="VIN" pad="7"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:8089856/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C">
<gates>
<gate name="G$1" symbol="C" x="-1.27" y="-1.27"/>
</gates>
<devices>
<device name="PANASONIC_H13" package="CAPAE1230X1250N">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<package3dinstances>
<package3dinstance package3d_urn="urn:adsk.eagle:package:21812541/1"/>
</package3dinstances>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO">
<gates>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
<compatibility>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports URNs for individual library
assets (packages, symbols, and devices). The URNs of those assets
will not be understood (or retained) with this version.
</note>
<note version="8.3" severity="warning">
Since Version 8.3, EAGLE supports the association of 3D packages
with devices in libraries, schematics, and board files. Those 3D
packages will not be understood (or retained) with this version.
</note>
</compatibility>
</eagle>
