<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="24" y2="0" width="0" layer="20"/>
<wire x1="24" y1="0" x2="24" y2="72" width="0" layer="20"/>
<wire x1="24" y1="72" x2="0" y2="72" width="0" layer="20"/>
<wire x1="0" y1="72" x2="0" y2="0" width="0" layer="20"/>
<hole x="21" y="70" drill="1.5"/>
<hole x="3" y="70" drill="1.5"/>
<hole x="12" y="2" drill="1.5"/>
</plain>
<libraries>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC3216X135">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Diode">
<description>&lt;B&gt;PN Junction, BridgeRectifier, Zener, Schottky, Switching</description>
<packages>
<package name="SOD6126X290">
<description>SOD, 6.10 mm span, 4.33 X 2.60 X 2.90 mm body
&lt;p&gt;SOD package with 6.10 mm span with body size 4.33 X 2.60 X 2.90 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="eScooter">
<packages>
<package name="DIOM5027X220N">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
</package>
<package name="SON254P1750X4300X120-30M">
<description>30-SON (DFN), 2.54 mm pitch, 43.00 X 17.50 X 1.20 mm body
&lt;p&gt;30-pin SON (DFN) package with 2.54 mm pitch with body size 43.00 X 17.50 X 1.20 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Transistor">
<description>&lt;B&gt;BJT, JFET, MOSFET, UJT, Darlington</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/HGP">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Capacitor" package="CAPC3216X135" value="0.1uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C2" library="Capacitor" package="CAPC3216X135" value="0.1uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C3" library="Capacitor" package="CAPC3216X135" value="0.1uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="D2" library="Diode" package="SOD6126X290" value="">
<attribute name="CATEGORY" value="Diode"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="FORWARD_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="REVERSE_VOLTAGE" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Rectifier"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Diode" package="SOD6126X290" value="">
<attribute name="CATEGORY" value="Diode"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="FORWARD_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="REVERSE_VOLTAGE" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Rectifier"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="eScooter" package="DIOM5027X220N" value="TVS_DIODESMA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="eScooter" package="DIOM5027X220N" value="TVS_DIODESMA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="eScooter" package="DIOM5027X220N" value="TVS_DIODESMA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="eScooter" package="DIOM5027X220N" value="TVS_DIODESMA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="Break">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06" value="COMM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X05" value="DISPLAY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03" value="THROTTLE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02" value="LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X06" value="SPEED">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Transistor" package="SOT23" value="NMOSFETSOT23">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Transistor" package="SOT23" value="">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Transistor" package="SOT23" value="">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value="MOSFET P-CH 50V 130MA SOT-23"/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="BSS84"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="P-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Transistor" package="SOT23" value="NMOSFETSOT23">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="VALUE"/>
</element>
<element name="SG1" library="buzzer" package="F/HGP" value="F/HGP">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="eScooter" package="SON254P1750X4300X120-30M" value="Arduino Nano Every">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="eScooter" package="DIOM5027X220N" value="TVS_DIODESMA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="U1" pad="2"/>
</signal>
<signal name="GND2">
<contactref element="U1" pad="19"/>
</signal>
<signal name="GND">
<contactref element="D6" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J5" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D8" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="SG1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="J7" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="15"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="DIN">
<contactref element="J4" pad="3"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="CS">
<contactref element="J4" pad="4"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="CLK">
<contactref element="J4" pad="5"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="5V">
<contactref element="J6" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="THIN">
<contactref element="J5" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="J7" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="SCL">
<contactref element="J7" pad="4"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="SP">
<contactref element="Q5" pad="3"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="STCTL">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="BTN">
<contactref element="D3" pad="2"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="BAT">
<contactref element="U1" pad="6"/>
<contactref element="J2" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SPEED">
<contactref element="J2" pad="6"/>
<contactref element="Q5" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="LEDCTL">
<contactref element="Q1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="STLEDCTL">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="J6" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="PWON">
<contactref element="Q2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="D7" pad="1"/>
<contactref element="U1" pad="26"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="12V">
<contactref element="R2" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Q4" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="D8" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="THCTL">
<contactref element="J7" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SPK">
<contactref element="U1" pad="10"/>
<contactref element="SG1" pad="2"/>
</signal>
<signal name="ST">
<contactref element="U1" pad="20"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
