<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="62" y2="43" width="0" layer="20"/>
<wire x1="62" y1="43" x2="0" y2="43" width="0" layer="20"/>
<wire x1="0" y1="43" x2="0" y2="0" width="0" layer="20"/>
<hole x="2.54" y="40.64" drill="3"/>
<hole x="2.54" y="2.54" drill="3"/>
<hole x="59.69" y="2.54" drill="3"/>
<hole x="59.69" y="40.64" drill="3"/>
</plain>
<libraries>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPC3216X135">
<description>Chip, 3.20 X 1.60 X 1.35 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 1.35 mm&lt;/p&gt;</description>
</package>
<package name="CAPMP7343X310N">
<description>Molded Body, 7.30 X 4.30 X 3.10 mm body
&lt;p&gt;Molded Body package with body size 7.30 X 4.30 X 3.10 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Diodes">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Diodes&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="DO201AD">
</package>
</packages>
</library>
<library name="Connectors">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Connectors&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="HDR-02">
</package>
</packages>
</library>
<library name="inductors">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR127">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="regulator">
<packages>
<package name="DIP8">
<description>&lt;b&gt;SMD DIL08&lt;/b&gt; Gull Wing Surface Mount Optioon 300&lt;p&gt;
Source: http://www.avagotech.com/docs/AV02-0410EN</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Transistor">
<description>&lt;B&gt;BJT, JFET, MOSFET, UJT, Darlington</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="eScooter">
<packages>
<package name="DIOM5027X220N">
<description>Molded Body, 5.00 X 2.70 X 2.20 mm body
&lt;p&gt;Molded Body package with body size 5.00 X 2.70 X 2.20 mm&lt;/p&gt;</description>
</package>
<package name="CAPAE1230X1250N">
<description>ECAP (Aluminum Electrolytic Capacitor), 12.30 X 12.50 mm body
&lt;p&gt;ECAP (Aluminum Electrolytic Capacitor) package with body size 12.30 X 12.50 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Capacitor" package="CAPC3216X135" value="0.1uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C2" library="Capacitor" package="CAPC3216X135" value="0.1uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="C3" library="Capacitor" package="CAPMP7343X310N" value="15uF">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="D1" library="Diodes" package="DO201AD" value="SB5100">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="MBR360GOS-ND"/>
<attribute name="MANUFACTURER" value="ON Semiconductor"/>
<attribute name="MPN" value="MBR360G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DO-201AD"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Connectors" package="HDR-02" value="IN">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NUMBER" value="455-1639-ND"/>
<attribute name="MANUFACTURER" value="JST Sales America Inc."/>
<attribute name="MPN" value="B2P-VH(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductors" package="DR127" value="DR127">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="SPICEPREFIX" value="L"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="eagle-ltspice" package="R1206" value="1M">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="eagle-ltspice" package="R1206" value="100K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="eagle-ltspice" package="R1206" value="39K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="regulator" package="DIP8" value="MAX5035DIP8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="ON/OFF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Transistor" package="SOT23" value="NMOSFETSOT23">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X08_LONGPADS" value="COMM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="STOP_LIGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04" value="DRIVER">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="eagle-ltspice" package="R1210" value="1M">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="eagle-ltspice" package="R1210" value="133K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Transistor" package="SOT23" value="NMOSFETSOT23">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Transistor" package="SOT23" value="NMOSFETSOT23">
<attribute name="CATEGORY" value="Transistor"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="DRAIN_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="MOSFET"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value="N-Channel"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="eScooter" package="DIOM5027X220N" value="P4SMAJ12CA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="eagle-ltspice" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="eScooter" package="CAPAE1230X1250N" value="68uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J3" pad="P2"/>
<contactref element="J1" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="D1" pad="C"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="12V">
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="P1"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SPIN">
<contactref element="J5" pad="1"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="SPOUT">
<contactref element="J5" pad="2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="ST">
<contactref element="J5" pad="3"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="5V">
<contactref element="J5" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="STLEDCTL">
<contactref element="Q1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="PWM">
<contactref element="Q2" pad="1"/>
<contactref element="J1" pad="4"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="J1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="STOUT">
<contactref element="J1" pad="6"/>
<contactref element="Q3" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
